{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["浆板机闲置设备"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"浆板机闲置设备","index":0,"n_rows":51,"n_cols":7,"rows_kept":51,"merged":[[0,0,0,6],[6,4,6,6],[51,0,51,6]],"flags":["formulas_cached_only"]}
["江西晨鸣浆板机闲置设备清单"]
["序号","名称","技术参数","单位","数量","品牌","设备现状"]
[1,"外流\n式压力筛\n"," JS4.0 筛选面积：5m2，筛鼓规格：Φ1350×1200mm ，生产能力：460－480t/d,开孔大小：2mm，进浆浓度0.5-2.5%,进浆压力：0.08-0.25MPa，操作压差：0.01-0.03MPa，密封水压力：比进浆压力高0.1MPa，密封水流量：1－3 l/min","台",1,"山东顺通科技有限公司","锈腐"]
[2,"                                                                                                                                                                                    \n吊带式振框筛\n","ZSK（D） 吊带800×140×20MM 筛选面积:1.8m2，处理量：30—60 t/d 筛孔尺寸：Φ3.5mm 进浆浓度：1％-1.5％，出浆浓度：0.8％ n=1430r/min","台",1,"山东邹平顺通造纸筛选设备有限公司","闲置"]
[3,"圆网浓缩机","过滤面积15平方，转鼓规格直径1500X3335   ,电机功率7.5kw(无电机)","台",null,"安丘海洋机械制造有限公司","闲置"]
[4,"安德里兹浆泵","S500-600CD   扬程20米，流量1620立方/小时，无电机","台",1,null,"闲置"]
[5,"浆板机本体","浆板机一台，包含以下部件： 生产能力:500t/d 净纸宽:4200mm,主轨距:5400mm，定量:800-1200g/m2，工作车速:105m/min， 设计车速:120m/min，爬行车速:15m/min 出网部28％，出压榨：50％，出干燥：90％ ,已解体","套","具体清单如下"]
[5,"后处理干燥","处理能力：20m3/min；前、后过滤器、微热","套",1,"\\","闲置"]
[6,"分汽缸","尺寸：Φ600×2930（长）mm 生产能力为23000kg/h  设计压力为1.6MPa","套",1,"\\","锈腐"]
[7,"气垫式干燥箱","\\","套",1,"山东凯信机械","报废"]
[8,"高浓流浆箱","上浆浓度：1.5%－2.5% 喷嘴宽度：4580mm 上唇板调整范围：5－20mm 圆锥管回流量：10％ 与浆料接触部分材质为不锈钢","套",1,"山东凯信机械","锈腐"]
[9,"胸辊","部件规格： 胸辊直径488mm，面宽4750 mm  辊体由低碳钢板卷制， 辊面包胶，胶厚7mm","根",2,"山东凯信机械","闲置"]
[10,"脱水孔板","孔板长度4670mm，高分子聚乙烯面板","套",1,"山东凯信机械","闲置"]
[11,"S辊","规格：直径 Φ410×4850mm，低碳钢无缝钢管车制，辊面包胶，胶厚7.5mm","根",5,"山东凯信机械","闲置"]
[12,"网部压榨辊","φ595mm,面宽4850mm，辊体采用20#钢板卷制，表面挂胶22.5mm","根",8,"山东凯信机械","闲置"]
[13,"上驱网压辊","φ750mm,面宽4850mm，辊体采用20#钢板卷制，表面挂胶22.5mm","根",1,"山东凯信机械","包胶层破损"]
[14,"下驱网压辊","φ750mm,面宽4850mm，辊体采用20#钢板卷制，表面挂胶22.5mm","根",1,"山东凯信机械","包胶层破损"]
[15,"下网下驱网辊","φ650mm,面宽4850mm，辊体采用20#钢板卷制，表面挂胶22.5mm","根",1,"山东凯信机械","闲置"]
[16,"压榨部压榨上辊"," 平辊 φ1350mm，面宽4750mm，铸铁辊体，辊面包胶22,5mm，压榨胶辊设计线压力220kg/cm","根",2,"山东凯信机械","闲置"]
[17,"压榨部压榨下辊","盲孔辊 开孔率约28% φ1350mm，面宽4750mm，铸铁辊体，辊面包胶22,5mm，压榨胶辊设计线压力220kg/cm","根",2,"山东凯信机械","闲置"]
[18,"毛毯电动涨紧器","Y100L1-4，功率P=2.2kw。上毯用涨紧器最大行程1000mm，下毯用涨紧器最大行程1000mm。","套",2,"山东凯信机械","闲置"]
[19,"毛毯吸水箱","吸水箱体及支架均为不锈钢焊接制造，面板采用超高分子聚乙烯，开口宽度为10～12mm。每只吸水箱配有真空表和调节螺栓，","套",4,"山东凯信机械","闲置"]
[20,"液压站","压榨部使用","套",1,"山东凯信机械","锈腐"]
[21,"导网辊","  Φ410×4850 低碳钢无缝钢管车制, 辊面包胶，胶厚7.5mm","根",7,"山东凯信机械","包胶层破损"]
[22," 清洁辊","清洁辊直径385mm，面宽4750mm  低碳钢无缝钢管车制, 辊面包胶，胶厚7.5mm","根",2,"山东凯信机械","闲置"]
[23,"引纸辊","Φ210×4850","根",null,"山东凯信机械","闲置"]
[24," 网子及毛毯导辊","Φ410×4850","根",22,"山东凯信机械","闲置"]
[25,"引纸辊","直径230mm，面宽4750mm 低碳钢无缝管车制，辊面镀铬,镀铬厚0.07mm","根",3,"山东凯信机械","包胶层破损"]
[26,"毛毯舒展辊","直径395mm，面宽4750mm","根",4,"山东凯信机械","包胶层破损"]
[27,"回头辊","直径 350mm，辊面宽4850mm 无缝钢管车制，辊面喷砂处理","根",15,"山东凯信机械","包胶层破损"]
[28,"干燥部导辊","直径268mm，辊面宽4850mm，表面镀硬铬 低碳钢无缝钢管车制,镀层厚0.07 mm ","根",5,"山东凯信机械","包胶层破损"]
[29,"纠偏辊","直径350mm，辊面宽4850mm  低碳钢无缝钢管车制表面镀硬铬","根",1,"山东凯信机械","锈蚀"]
[30,"牵引上辊","直径350mm，辊面宽4850mm  低碳钢无缝钢管车制表面镀硬铬","根",1,"山东凯信机械","锈蚀"]
[31,"牵引下辊","直径350mm，辊面宽4500mm   辊面镀铬","根",1,"山东凯信机械","锈蚀"]
[32,"导辊","机下备件","根",2,"山东凯信机械","锈蚀"]
[33,"升降操作台",null,"套",2,"山东凯信机械","锈腐"]
[34,"回头辊","机下备件","根",2,"山东凯信机械","胶层老化"]
[35,"舒展辊","机下备件","根",2,"山东凯信机械","胶层老化"]
[36,"毛布调偏装置","机下备件","套",2,"山东凯信机械","胶层老化"]
[37,"压榨辊","机下备件","根",1,"山东凯信机械","胶层老化"]
[38,"驱网辊","机下备件","根",2,"山东凯信机械","胶层老化"]
[39,"打包机","80T液压打包机","台",1,"山东凯信机械","闲置"]
[40,"浆包输送链条","含转向链条","节",13,"山东凯信机械","锈蚀"]
[41,"电机含风机","Y2-160L-4",11,1,"380V","锈蚀"]
[42,"配电柜","ABB传动柜+进线柜",null,7,null,"维修后可用"]
[43,"配电柜","电源进线柜+母联柜","5000A",3,null,"维修后可用"]
[44,"配电柜","检修电源+照明电源柜",null,6,null,"维修后可用"]
[45,"配电柜","软起+变频柜",null,5,null,"维修后可用"]
[46,"配电柜","电源出线柜 V1","3200A",3,null,"维修后可用"]
[47,"配电柜","电容柜",null,4,null,"维修后可用"]
[48,"配电柜","抽屉柜",null,7,null,"维修后可用"]