{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["江西晨鸣"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"江西晨鸣","index":0,"n_rows":14,"n_cols":9,"rows_kept":14,"merged":[[0,0,0,8]],"flags":["formulas_cached_only"]}
["江西晨鸣卸煤沟闲置设备清单"]
["序号","物料名称","规格型号","单位","数量","主要性能指标、参数","购入时间","购进厂家","设备现状"]
[1,"螺旋卸料机","LX-6.70","套",2,"型号LX-6.70 卸车能力400T/H 轨道距离6.7米 装机容量18.5KW 外形尺寸7*5.3*5M 整机质量20835KG 产品编号04-15-5  出厂日期04.12","04年",null,"已锈蚀"]
[2,"多管冲击式除尘器","JJDCC7-II","台",3,"型号JJDCC7-II 额定风量7200m3/H设备阻力150-200Pa 效率90％配套功率7.5KW 设备总重2753KG 出厂编号040904","04年",null,"已锈蚀"]
[3,"单级叶轮给煤机","300-600T/H","套",4,"生产能力300-600T/H 车轮直径380MM叶轮直径2680MM 行走速度3.74r/m 叶轮转速2.76-8.3r/min 转距1800MM","04年",null,"已锈蚀"]
[4,"DG系列电动推杆","50090MB","个",3,null,"04年",null,"已锈蚀"]
[5,"TD型斗式提升机短节","TD160","节",4,"提升高度1029m 电机型号 Y100L2","04年",null,"已锈蚀"]
[6,"螺旋装置",null,"套",8,null,"04年",null,"已锈蚀"]
[7,"手动梁式起重机",null,"台",2,null,"04年","江西东风起重机械有限公司","已锈蚀"]
[8,"行车主轨横梁",null,"件",4,null,"04年",null,"已锈蚀"]
[9,"交流低压抽出式开关柜","SEIKO","台",5,"频率50HZ，额定电压380V","04年","中日合资大连正兴控制有限公司","已锈蚀"]
[10,"电气控制柜","JJIB-30KW ","台",3,"JJIB-30KW 频率50HZ","04年","山东章丘","已锈蚀，内部元件缺失"]
[11,"工业自动化控制柜","XL-21B","台",4,"XL-21B","04年","长沙天宇智能电气厂制造","已锈蚀，内部元件缺失"]
[12,"配套设备钢件",null,"批",1,"托辊架、三角板、  支架、平台板","04年",null,"已锈蚀"]