{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":124,"n_cols":256,"rows_kept":124,"merged":[[0,0,0,7],[1,0,1,7],[2,0,2,7]],"flags":["formulas_cached_only"]}
["武汉晨鸣汉阳纸业股份有限公司"]
["脱墨浆车间主要设备参数表"]
[]
["序号","名称","型号或制造图号","规格及技术数据","电机功率","单位"," 数量","备注"]
[1,"转鼓式碎浆机","optislush  OSD750","（ONP/OMG）500-750 ADMTPD碎浆浓度15-20%、                             出口浓度4-5%、转速8-14rpm","3×250KW",null,1,"mesto"]
[2,"卸料浆泵",null,"Q=900m3/h、H=24m",null,null,2]
[3,"卸料浆池",null,"容积：560m3，直径：10.67m，高度：6.4m，钢制衬不锈钢",null,null,1,"非标槽罐自制"]
[null,"附：搅拌器（Agitator)","FR3-42","不锈钢制",null,null,2,"TBC供"]
[null,"电机（Motor)","y315S-4","150rpm  ，B3",110,null,2,"湘潭电机厂"]
[4,"立管",null,"容积：18.8m3，直径：2m，深度：6m，不锈钢制",null,null,1,"非标槽罐自制"]
[5,"浆泵","S350-470.6","Q=1680m3/h，H=49m，C=2.5-3.0%,不锈钢制",null,null,1]
[null,"Pulp pump",{"$nulls":5},"ANDRITZ-KENFLO"]
[null,"电机（Motor)","YKS450-4","1500rpm  10kv",315,null,1,"湘潭电机厂"]
[6,"25#高浓除渣器",null,"压力降:172kpa，锥体：陶瓷   连续排渣",null,null,2,"TBC供"]
[7,"浆泵","S250-430.6","Q=780m3/h，H=34m，C=2.0%,不锈钢制",null,null,1,"ANDRITZ-KENFLO"]
[null,"电机（Motor)","Y315S-4","150rpm  ，B3",110,null,1]
[8,"17#高浓除渣器",null,"压力降:172kpa，锥体：陶瓷   间歇排渣",null,null,2,"TBC供"]
[9,"一段粗筛","Ultra-V500","筛孔:φ1.3mm，筛鼓尺寸:φ900×1080mm,不锈钢316L",null,null,1,"TBC供"]
[null,"电机（Motor)","Y355L3-6","1000rpm     V5    轴头加长至210 mm",250,null,1,"湘潭电机厂"]
[10,"浆泵","S125-400","Q=295m3/h，H=30m，C=2.5-3.0%,不锈钢制",null,null,1,"ANDRITZ-KENFLO"]
[null,"Pulp pump"]
[null,"电机（Motor)","Y225S-4","150rpm  ，B3",37,null,1]
[11,"二段粗筛","Ultra-V500","筛孔:φ1.3mm，筛鼓尺寸:φ610×426mm,不锈钢316L",null,null,1,"TBC供"]
[null,"电机（Motor)","Y315S-6","1000rpm     V5    ",75,null,1,"湘潭电机厂"]
[12,"浆泵","S100-350","Q=85m3/h，H=30m，C=2.0%,不锈钢制",null,null,1,"ANDRITZ-KENFLO"]
[null,"电机（Motor)","Y160L-4","1500rpm  ，B3",15,null,1]
[13,"三段粗筛","Ultra-V500","筛孔:φ1.3mm，筛鼓尺寸:φ400×225mm,不锈钢316L",null,null,1,"TBC供"]
[null,"电机（Motor)","Y315S-6","1000rpm     B3   ",18.5,null,1,"TBC供"]
[14,"浆泵","S350-470","Q=1610m3/h，H=30m，C=2.0%,不锈钢制",null,null,1,"ANDRITZ-KENFLO"]
[null,"电机（Motor)","Y315L-4","1500rpm  ，B3",160,null,1]
[15,"一段精筛","Ultra-V500","筛孔:φ0.15mm，筛鼓尺寸:φ900×1080mm,不锈钢316L",null,null,2,"TBC供"]
[null,"电机（Motor)","Y355M1-6","1000rpm     V5    轴头加长至210 mm",160,null,2,"湘潭电机厂"]
[16,"一段精筛后浆泵","S200-380.6","Q=480m3/h，H=30m，C=2.0%,不锈钢制",null,null,1,"ANDRITZ-KENFLO"]
[null,"电机（Motor)","Y250M-4","1500rpm  ，B3",55,null,1]
[17,"二段精筛","Ultra-V400","筛孔:φ0.15mm，筛鼓尺寸:φ762×838mm,不锈钢316L",null,null,1,"TBC供"]
[null,"电机（Motor)","Y315M-6","1000rpm     V5   ",90,null,1,"湘潭电机厂"]
[null,"电机（Motor)","Y160L-4","1500rpm  ，B3",15,null,1]
[18,"三段精筛","Ultra-V100","筛孔:φ0.15mm，筛鼓尺寸:φ610×311mm,不锈钢316L",null,null,1,"TBC供"]
[null,"电机（Motor)","Y225M-6","1000rpm     V5   ",30,null,1,"湘潭电机厂"]
[19,"浆泵","S8-350-470","Q=1901m3/h，H=28m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",19,"浆泵","S8-350-470","Q=1901m3/h，H=28m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",19,"浆泵","S8-350-470","Q=1901m3/h，H=28m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",19,"浆泵","S8-350-470","Q=1901m3/h，H=28m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",19,"浆泵","S8-350-470","Q=1901m3/h，H=28m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",19,"浆泵","S8-350-470","Q=1901m3/h，H=28m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",19,"浆泵","S8-350-470","Q=1901m3/h，H=28m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",19,"浆泵","S8-350-470","Q=1901m3/h，H=28m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",19,"浆泵","S8-350-470","Q=1901m3/h，H=28m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",19,"浆泵","S8-350-470","Q=1901m3/h，H=28m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",19,"浆泵","S8-350-470","Q=1901m3/h，H=28m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",19,"浆泵","S8-350-470","Q=1901m3/h，H=28m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",19,"浆泵","S8-350-470","Q=1901m3/h，H=28m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",19,"浆泵","S8-350-470","Q=1901m3/h，H=28m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",19,"浆泵","S8-350-470","Q=1901m3/h，H=28m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",19,"浆泵","S8-350-470","Q=1901m3/h，H=28m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",19,"浆泵","S8-350-470","Q=1901m3/h，H=28m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",19,"浆泵","S8-350-470","Q=1901m3/h，H=28m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",19,"浆泵","S8-350-470","Q=1901m3/h，H=28m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",19,"浆泵","S8-350-470","Q=1901m3/h，H=28m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",19,"浆泵","S8-350-470","Q=1901m3/h，H=28m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",19,"浆泵","S8-350-470","Q=1901m3/h，H=28m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",19,"浆泵","S8-350-470","Q=1901m3/h，H=28m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",19,"浆泵","S8-350-470","Q=1901m3/h，H=28m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",19,"浆泵","S8-350-470","Q=1901m3/h，H=28m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",19,"浆泵","S8-350-470","Q=1901m3/h，H=28m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",19,"浆泵","S8-350-470","Q=1901m3/h，H=28m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",19,"浆泵","S8-350-470","Q=1901m3/h，H=28m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",19,"浆泵","S8-350-470","Q=1901m3/h，H=28m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",19,"浆泵","S8-350-470","Q=1901m3/h，H=28m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",19,"浆泵","S8-350-470","Q=1901m3/h，H=28m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",19,"浆泵","S8-350-470","Q=1901m3/h，H=28m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO"]
[null,"电机（Motor)","Y2315L2-4","1485rpm  ，B3",200,null,1,null,null,"电机（Motor)","Y2315L2-4","1485rpm  ，B3",200,null,1,null,null,"电机（Motor)","Y2315L2-4","1485rpm  ，B3",200,null,1,null,null,"电机（Motor)","Y2315L2-4","1485rpm  ，B3",200,null,1,null,null,"电机（Motor)","Y2315L2-4","1485rpm  ，B3",200,null,1,null,null,"电机（Motor)","Y2315L2-4","1485rpm  ，B3",200,null,1,null,null,"电机（Motor)","Y2315L2-4","1485rpm  ，B3",200,null,1,null,null,"电机（Motor)","Y2315L2-4","1485rpm  ，B3",200,null,1,null,null,"电机（Motor)","Y2315L2-4","1485rpm  ，B3",200,null,1,null,null,"电机（Motor)","Y2315L2-4","1485rpm  ，B3",200,null,1,null,null,"电机（Motor)","Y2315L2-4","1485rpm  ，B3",200,null,1,null,null,"电机（Motor)","Y2315L2-4","1485rpm  ，B3",200,null,1,null,null,"电机（Motor)","Y2315L2-4","1485rpm  ，B3",200,null,1,null,null,"电机（Motor)","Y2315L2-4","1485rpm  ，B3",200,null,1,null,null,"电机（Motor)","Y2315L2-4","1485rpm  ，B3",200,null,1,null,null,"电机（Motor)","Y2315L2-4","1485rpm  ，B3",200,null,1,null,null,"电机（Motor)","Y2315L2-4","1485rpm  ，B3",200,null,1,null,null,"电机（Motor)","Y2315L2-4","1485rpm  ，B3",200,null,1,null,null,"电机（Motor)","Y2315L2-4","1485rpm  ，B3",200,null,1,null,null,"电机（Motor)","Y2315L2-4","1485rpm  ，B3",200,null,1,null,null,"电机（Motor)","Y2315L2-4","1485rpm  ，B3",200,null,1,null,null,"电机（Motor)","Y2315L2-4","1485rpm  ，B3",200,null,1,null,null,"电机（Motor)","Y2315L2-4","1485rpm  ，B3",200,null,1,null,null,"电机（Motor)","Y2315L2-4","1485rpm  ，B3",200,null,1,null,null,"电机（Motor)","Y2315L2-4","1485rpm  ，B3",200,null,1,null,null,"电机（Motor)","Y2315L2-4","1485rpm  ，B3",200,null,1,null,null,"电机（Motor)","Y2315L2-4","1485rpm  ，B3",200,null,1,null,null,"电机（Motor)","Y2315L2-4","1485rpm  ，B3",200,null,1,null,null,"电机（Motor)","Y2315L2-4","1485rpm  ，B3",200,null,1,null,null,"电机（Motor)","Y2315L2-4","1485rpm  ，B3",200,null,1,null,null,"电机（Motor)","Y2315L2-4","1485rpm  ，B3",200,null,1,null,null,"电机（Motor)","Y2315L2-4","1485rpm  ，B3",200,null,1]
[20,"前浮选槽","SFL4DD","长*宽:4004*5460mm*5，高度:2500mm,入口射流器:4组,不锈钢316L",null,null,1,"ANDRITZ",20,"前浮选槽","SFL4DD","长*宽:4004*5460mm*5，高度:2500mm,入口射流器:4组,不锈钢316L",null,null,1,"ANDRITZ",20,"前浮选槽","SFL4DD","长*宽:4004*5460mm*5，高度:2500mm,入口射流器:4组,不锈钢316L",null,null,1,"ANDRITZ",20,"前浮选槽","SFL4DD","长*宽:4004*5460mm*5，高度:2500mm,入口射流器:4组,不锈钢316L",null,null,1,"ANDRITZ",20,"前浮选槽","SFL4DD","长*宽:4004*5460mm*5，高度:2500mm,入口射流器:4组,不锈钢316L",null,null,1,"ANDRITZ",20,"前浮选槽","SFL4DD","长*宽:4004*5460mm*5，高度:2500mm,入口射流器:4组,不锈钢316L",null,null,1,"ANDRITZ",20,"前浮选槽","SFL4DD","长*宽:4004*5460mm*5，高度:2500mm,入口射流器:4组,不锈钢316L",null,null,1,"ANDRITZ",20,"前浮选槽","SFL4DD","长*宽:4004*5460mm*5，高度:2500mm,入口射流器:4组,不锈钢316L",null,null,1,"ANDRITZ",20,"前浮选槽","SFL4DD","长*宽:4004*5460mm*5，高度:2500mm,入口射流器:4组,不锈钢316L",null,null,1,"ANDRITZ",20,"前浮选槽","SFL4DD","长*宽:4004*5460mm*5，高度:2500mm,入口射流器:4组,不锈钢316L",null,null,1,"ANDRITZ",20,"前浮选槽","SFL4DD","长*宽:4004*5460mm*5，高度:2500mm,入口射流器:4组,不锈钢316L",null,null,1,"ANDRITZ",20,"前浮选槽","SFL4DD","长*宽:4004*5460mm*5，高度:2500mm,入口射流器:4组,不锈钢316L",null,null,1,"ANDRITZ",20,"前浮选槽","SFL4DD","长*宽:4004*5460mm*5，高度:2500mm,入口射流器:4组,不锈钢316L",null,null,1,"ANDRITZ",20,"前浮选槽","SFL4DD","长*宽:4004*5460mm*5，高度:2500mm,入口射流器:4组,不锈钢316L",null,null,1,"ANDRITZ",20,"前浮选槽","SFL4DD","长*宽:4004*5460mm*5，高度:2500mm,入口射流器:4组,不锈钢316L",null,null,1,"ANDRITZ",20,"前浮选槽","SFL4DD","长*宽:4004*5460mm*5，高度:2500mm,入口射流器:4组,不锈钢316L",null,null,1,"ANDRITZ",20,"前浮选槽","SFL4DD","长*宽:4004*5460mm*5，高度:2500mm,入口射流器:4组,不锈钢316L",null,null,1,"ANDRITZ",20,"前浮选槽","SFL4DD","长*宽:4004*5460mm*5，高度:2500mm,入口射流器:4组,不锈钢316L",null,null,1,"ANDRITZ",20,"前浮选槽","SFL4DD","长*宽:4004*5460mm*5，高度:2500mm,入口射流器:4组,不锈钢316L",null,null,1,"ANDRITZ",20,"前浮选槽","SFL4DD","长*宽:4004*5460mm*5，高度:2500mm,入口射流器:4组,不锈钢316L",null,null,1,"ANDRITZ",20,"前浮选槽","SFL4DD","长*宽:4004*5460mm*5，高度:2500mm,入口射流器:4组,不锈钢316L",null,null,1,"ANDRITZ",20,"前浮选槽","SFL4DD","长*宽:4004*5460mm*5，高度:2500mm,入口射流器:4组,不锈钢316L",null,null,1,"ANDRITZ",20,"前浮选槽","SFL4DD","长*宽:4004*5460mm*5，高度:2500mm,入口射流器:4组,不锈钢316L",null,null,1,"ANDRITZ",20,"前浮选槽","SFL4DD","长*宽:4004*5460mm*5，高度:2500mm,入口射流器:4组,不锈钢316L",null,null,1,"ANDRITZ",20,"前浮选槽","SFL4DD","长*宽:4004*5460mm*5，高度:2500mm,入口射流器:4组,不锈钢316L",null,null,1,"ANDRITZ",20,"前浮选槽","SFL4DD","长*宽:4004*5460mm*5，高度:2500mm,入口射流器:4组,不锈钢316L",null,null,1,"ANDRITZ",20,"前浮选槽","SFL4DD","长*宽:4004*5460mm*5，高度:2500mm,入口射流器:4组,不锈钢316L",null,null,1,"ANDRITZ",20,"前浮选槽","SFL4DD","长*宽:4004*5460mm*5，高度:2500mm,入口射流器:4组,不锈钢316L",null,null,1,"ANDRITZ",20,"前浮选槽","SFL4DD","长*宽:4004*5460mm*5，高度:2500mm,入口射流器:4组,不锈钢316L",null,null,1,"ANDRITZ",20,"前浮选槽","SFL4DD","长*宽:4004*5460mm*5，高度:2500mm,入口射流器:4组,不锈钢316L",null,null,1,"ANDRITZ",20,"前浮选槽","SFL4DD","长*宽:4004*5460mm*5，高度:2500mm,入口射流器:4组,不锈钢316L",null,null,1,"ANDRITZ",20,"前浮选槽","SFL4DD","长*宽:4004*5460mm*5，高度:2500mm,入口射流器:4组,不锈钢316L",null,null,1,"ANDRITZ"]
[null,"附:前浮选良浆槽",null,"容积:10m3",null,null,1,null,null,"附:前浮选良浆槽",null,"容积:10m3",null,null,1,null,null,"附:前浮选良浆槽",null,"容积:10m3",null,null,1,null,null,"附:前浮选良浆槽",null,"容积:10m3",null,null,1,null,null,"附:前浮选良浆槽",null,"容积:10m3",null,null,1,null,null,"附:前浮选良浆槽",null,"容积:10m3",null,null,1,null,null,"附:前浮选良浆槽",null,"容积:10m3",null,null,1,null,null,"附:前浮选良浆槽",null,"容积:10m3",null,null,1,null,null,"附:前浮选良浆槽",null,"容积:10m3",null,null,1,null,null,"附:前浮选良浆槽",null,"容积:10m3",null,null,1,null,null,"附:前浮选良浆槽",null,"容积:10m3",null,null,1,null,null,"附:前浮选良浆槽",null,"容积:10m3",null,null,1,null,null,"附:前浮选良浆槽",null,"容积:10m3",null,null,1,null,null,"附:前浮选良浆槽",null,"容积:10m3",null,null,1,null,null,"附:前浮选良浆槽",null,"容积:10m3",null,null,1,null,null,"附:前浮选良浆槽",null,"容积:10m3",null,null,1,null,null,"附:前浮选良浆槽",null,"容积:10m3",null,null,1,null,null,"附:前浮选良浆槽",null,"容积:10m3",null,null,1,null,null,"附:前浮选良浆槽",null,"容积:10m3",null,null,1,null,null,"附:前浮选良浆槽",null,"容积:10m3",null,null,1,null,null,"附:前浮选良浆槽",null,"容积:10m3",null,null,1,null,null,"附:前浮选良浆槽",null,"容积:10m3",null,null,1,null,null,"附:前浮选良浆槽",null,"容积:10m3",null,null,1,null,null,"附:前浮选良浆槽",null,"容积:10m3",null,null,1,null,null,"附:前浮选良浆槽",null,"容积:10m3",null,null,1,null,null,"附:前浮选良浆槽",null,"容积:10m3",null,null,1,null,null,"附:前浮选良浆槽",null,"容积:10m3",null,null,1,null,null,"附:前浮选良浆槽",null,"容积:10m3",null,null,1,null,null,"附:前浮选良浆槽",null,"容积:10m3",null,null,1,null,null,"附:前浮选良浆槽",null,"容积:10m3",null,null,1,null,null,"附:前浮选良浆槽",null,"容积:10m3",null,null,1,null,null,"附:前浮选良浆槽",null,"容积:10m3",null,null,1]
[21,"二段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",21,"二段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",21,"二段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",21,"二段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",21,"二段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",21,"二段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",21,"二段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",21,"二段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",21,"二段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",21,"二段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",21,"二段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",21,"二段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",21,"二段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",21,"二段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",21,"二段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",21,"二段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",21,"二段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",21,"二段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",21,"二段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",21,"二段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",21,"二段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",21,"二段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",21,"二段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",21,"二段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",21,"二段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",21,"二段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",21,"二段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",21,"二段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",21,"二段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",21,"二段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",21,"二段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",21,"二段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO"]
[null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1]
[22,"三段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",22,"三段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",22,"三段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",22,"三段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",22,"三段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",22,"三段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",22,"三段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",22,"三段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",22,"三段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",22,"三段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",22,"三段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",22,"三段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",22,"三段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",22,"三段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",22,"三段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",22,"三段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",22,"三段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",22,"三段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",22,"三段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",22,"三段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",22,"三段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",22,"三段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",22,"三段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",22,"三段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",22,"三段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",22,"三段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",22,"三段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",22,"三段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",22,"三段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",22,"三段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",22,"三段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",22,"三段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO"]
[null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1]
[23,"四段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",23,"四段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",23,"四段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",23,"四段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",23,"四段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",23,"四段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",23,"四段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",23,"四段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",23,"四段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",23,"四段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",23,"四段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",23,"四段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",23,"四段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",23,"四段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",23,"四段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",23,"四段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",23,"四段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",23,"四段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",23,"四段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",23,"四段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",23,"四段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",23,"四段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",23,"四段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",23,"四段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",23,"四段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",23,"四段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",23,"四段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",23,"四段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",23,"四段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",23,"四段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",23,"四段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",23,"四段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO"]
[null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1]
[24,"五段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",24,"五段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",24,"五段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",24,"五段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",24,"五段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",24,"五段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",24,"五段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",24,"五段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",24,"五段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",24,"五段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",24,"五段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",24,"五段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",24,"五段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",24,"五段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",24,"五段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",24,"五段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",24,"五段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",24,"五段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",24,"五段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",24,"五段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",24,"五段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",24,"五段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",24,"五段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",24,"五段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",24,"五段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",24,"五段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",24,"五段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",24,"五段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",24,"五段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",24,"五段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",24,"五段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO",24,"五段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=16m，C=1.3%,不锈钢制",null,null,1,"ANDRITZ-KENFLO"]
[null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1,null,null,"电机（Motor)","Y2355M1-6","990rpm  ，B3",160,null,1]
[25,"一段锥形除砂器浆泵","S500-600.6","Q=2570m3/h，H=36m，C=1.0,不锈钢制",null,null,1,"ANDRITZ-KENFLO"]
[null,"电机（Motor)","YKS450-6","1000rpm  ，10KV   B3",315,null,1,"湘潭电机厂"]
[26,"一段锥形除砂器",null,"不锈钢, 80支,600l/min/支",null,null,80,"山东高新"]
[27,"前多盘进浆立管",null,"容积：25m3，直径：2.5m，深度：5m，不锈钢制",null,null,1,"非标槽罐自制"]
[28,"浆泵","S500-600","Q=2800m3/h，H=15m，C=1.0-2.0%,不锈钢制",null,null,1,"ANDRITZ-KENFLO"]
[null,"电机（Motor)","Y355M1-6","1000rpm  ，B3",160,null,1]
[29,"一段精筛泵",null,"Q=2700m3/h，H=28m，C=1.0%"]
[30,"一段精筛","MAX-1300、Screen","缝宽0.12mm，转子速度16m/s","90kw、8p",null,2,"日本相川"]
[{"$nulls":3},"筛筐：φ1500×1500,筛选面积：4.8m2,开口面积：0.1957m2,C：1%"]
[31,"前多圆盘浓缩机","DF-520  14/16","圆盘直径:5.2m,浓滤液:400mmg/l,清滤液100mg/l,清浊比:75/25,不锈钢316L",null,null,1,"TBC/Kvaemer"]
[null,"附:主电机(Main moto)","Y160M-4","1500rpm  ，Frequency  control   B3",11,null,1,"湘潭电机厂"]
[null,"附:出料螺旋电机(Motor)","Y160-4","1500rpm  ， B3",15,null,1,"湘潭电机厂"]
[null,"附:喷水管电机(Shower  motor)",null,"1500rpm  ",1.5,null,1,"TBC/Kvaemer"]
[32,"中浓泵","MPC20/10","Q=140m3/h，浓度:10.-12%,不锈钢",null,null,1,"TBC/Kvaemer"]
[null,"MC-Pump",null,"parts in contact with pulp:ss329"]
[null,"电机(Motor)变频","Y280M-2","3000rpm  ，Frequency  control   B3",90,null,1,"湘潭电机厂"]
[null,"附:立管(Standpipe)",null,"不锈钢制",null,null,1,"非标槽罐自制"]
[33,"1#螺旋压榨机","SP150L","进浆浓度:3-12%,出浆浓度:30%,不锈钢316L",null,null,1,"TBC/Kvaemer"]
[null,"电机(Motor)变频","Y355L2-4","1500rpm  ，280V, B3,Frequency  control   ",315,null,1,"湘潭电机厂"]
[34,"快速加热螺旋","PMAS36","加热时间:10-20S,转速:300-400rpm ,不锈钢316L",null,null,1,"TBC/Kvaemer"]
[null,"电机（Motor)","Y355M3-6","1000rpm  ，B3",200,null,1,"湘潭电机厂"]
[35,"1#热分散机","KRD110-HC","进浆浓度:30%,出浆浓度:28%,比能:80-85kwh/t",null,null,1]
[null,"电机（Motor)","YKS560-6","1000rpm  ,10kv,B3",1400,null,1,"湘潭电机厂"]
[null,"喂料电机(Feeding gear moror)","Y255M-6","1000rpm  ，B3",30,null,1,"湘潭电机厂"]
[null,"液压电机(Hydraulic  drive  moror)",null,"1500rpm  ",1.5,null,1,"TBC/Kvaemer"]
[36,"高浓漂白塔",null,"高度:10.5m,直径:4.4m，容积:1960m3,停留时间:90min,钢制内衬不锈钢",null,null,1,"非标槽罐自制"]
[null,"附:搅拌器(Agitator)","FR3-42","不锈钢制",null,null,1,"TBC供"]
[null,"电机（Motor)","Y280S-4","1500rpm  ,B3",75,null,1,"湘潭电机厂"]
[null,"附稀释水环",{"$nulls":4},1]
[37,"后浮选浆泵","S8-350-470","Q=1901m3/h，H=22m，C=1.1%,不锈钢制",null,null,1,"ANDRITZ-KENFLO"]
[null,"电机（Motor)","Y2315M2-4","1485rpm  ，B3",160,null,1]
[38,"后浮选槽","SFL4DD","长*宽:4004*5460mm*5，高度:2500mm,入口射流器:4组,不锈钢316L",null,null,1,"ANDRITZ"]
[null,"附:前浮选良浆槽",null,"容积:10m3",null,null,1]
[39,"二段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=12m，C=1.1%,不锈钢制",null,null,1,"ANDRITZ-KENFLO"]
[null,"电机（Motor)","Y2315M3-6","990rpm  ，B3",132,null,1]
[40,"三段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=12m，C=1.1%,不锈钢制",null,null,1,"ANDRITZ-KENFLO"]
[null,"电机（Motor)","Y2315M3-6","990rpm  ，B3",132,null,1]
[41,"四段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=12m，C=1.1%,不锈钢制",null,null,1,"ANDRITZ-KENFLO"]
[null,"电机（Motor)","Y2315M3-6","990rpm  ，B3",132,null,1]
[42,"五段浮选浆泵","S8-500-600","Q=2097.6m3/h，H=12m，C=1.1%,不锈钢制",null,null,1,"ANDRITZ-KENFLO"]
[null,"电机（Motor)","Y2315M3-6","990rpm  ，B3",132,null,1]
[43,"后多盘进浆立管",null,"容积：15m3，直径：2m，高度：5m，不锈钢制",null,null,1,"非标槽罐自制"]
[44,"浆泵","S350-470","Q=1380m3/h，H=15m，C=1.0-2.0%,不锈钢制",null,null,1,"ANDRITZ-KENFLO"]
[null,"电机（Motor)","Y315S-6","1000rpm  ，B3",75,null,1]
[45,"后多圆盘浓缩机","DF-520  8/9","圆盘直径:5.2m,浓滤液:300mmg/l,清滤液100ppm,清浊比:75/25,进浆浓:1.17%,出浆浓:10-12%,浆接触部分为不锈钢316L",null,null,1,"TBC/Kvaemer"]
[null,"附:主电机(Main moto)变频","Y132M-4","1500rpm  ，Frequency  control   ",7.5,null,1,"湘潭电机厂"]
[null,"附:输料螺旋电机(Motor)","Y160M-4","1500rpm  ， B3",11,null,1,"湘潭电机厂"]
[null,"附:喷水管电机(Shower  motor)",null,"1500rpm  ",1.5,null,1,"TBC/Kvaemer"]
[46,"中浓泵","MPC20/10","进浆浓度:10-12%,不锈钢",null,null,1,"TBC/Kvaemer"]
[{"$nulls":3},"parts in contact with pulp:ss329"]
[null,"电机(Motor)变频","Y280M-2","3000rpm  ，Frequency  control   B3",90,null,1,"湘潭电机厂"]
[null,"附:立管(Standpipe)",null,"不锈钢制",null,null,1,"非标槽罐自制"]
[47,"高浓贮浆塔",null,"V=1000m3,φ9.8×17.5m,浓度:10%,钢制内衬不锈钢",null,null,1,"非标槽罐自制"]
[null,"附:搅拌器(Agitator)","FR3-42","不锈钢制",null,null,1,"TBC供"]
[null,"电机（Motor)","Y315S-4","1500rpm  ,B3",110,null,1,"湘潭电机厂"]
[null,"附稀释水环",{"$nulls":4},1]
[48,"2#螺旋压榨机","SHX-1350×800L","1350×8000mm,0.7-7.5r/min,500kpa,进浆浓度:10%,出浆浓度:30%",null,null,1,"METSO"]
[null,"电机(变频)",null,null,315,null,1]
[null,"电机",null,null,3,null,1]
[49,"加热螺旋",null,"D600×5000mm,500BDT/d,浓度:30%",null,null,1]
[null,"电机",null,null,15,null,1]
[50,"2#热分散机","DFD-150","浆料接触部分采用316L不锈钢",null,null,1,"METSO"]
[null,"电机",null,null,1600,null,1]
[null,"润滑系统电机",null,null,0.75,null,1]
[null,"装料装置",null,null,0.55,null,1]
[51,"2#中浓泵","DSHM125-280","进浆浓度:10~12%,不锈钢",null,null,1,"ANDRITZ"]
[null,"电机(变频)",null,null,90,null,1]
[null,"调制器","ZR500PH",{"$nulls":3},1]
[null,"电机",null,"1500rpm",30,null,1]
[null,"真空泵","AKV220-0",{"$nulls":3},1,"ANDRIZ"]
[null,"电机",null,"1500rpm",5.5,null,1]
[null,"动态蒸汽加热器","dshm-3-125-280",{"$nulls":3},1]
[52,"在线还原漂白管",null,"D2500×12700mm",null,null,1]