{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["闲置设备清单","重点设备","Sheet2"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"闲置设备清单","index":0,"n_rows":579,"n_cols":17,"rows_kept":579,"merged":[[0,0,0,16],[578,1,578,8]],"flags":["formulas_cached_only"]}
["吉林晨鸣闲置脱墨浆线主要单体设备统计表"]
["序号","公司","工厂","物料名称","规格型号","资产编号","单位","数量","主要性能指标、参数","购入时间","购进厂家","库存地点","资产原值","现账面净值","闲置原因","设备状况","产能"]
[1,"吉林晨鸣","制浆分厂","散包机","BO1500",2000000819,"台",1,"\n长×宽×高：5700×3500×8000mm，变频调速，1500rpm，380V，B5，IP55  正反转（5台)                                \n\n\n",2013.9,"VOITH  供货 ","脱墨浆车间",{"v":686637.84,"d":"686,637.84"},{"v":534719.23,"d":"534,719.23"},"脱墨浆停产","良好"]
[2,"吉林晨鸣","制浆分厂","匀整辊","RTR1500/3000",2000000822,"台",1,"转鼓直径φ3000mm，宽度：1380mm",2013.9,"VOITH  供货 ","脱墨浆车间",{"v":246027.95,"d":"246,027.95"},{"v":191594.25,"d":"191,594.25"},"脱墨浆停产","良好"]
[3,"吉林晨鸣","制浆分厂","二段高浓泵","S8-150-330.3",2000000830,"台",1,"Q=250m3/h H=18m C=1.17%",2013.9,"苏尔寿","脱墨浆车间",{"v":73075.54,"d":"73,075.54"},{"v":56907.57,"d":"56,907.57"},"脱墨浆停产","良好"]
[4,"吉林晨鸣","制浆分厂","二段高浓重质除砂器","HCC400-2.1",2000000831,"台",1,"通过量：70L/s 进料浓度：1.16%",2013.9,"VOITH  供货 ","脱墨浆车间",{"v":194728.51,"d":"194,728.51"},{"v":151644.84,"d":"151,644.84"},"脱墨浆停产","良好"]
[5,"吉林晨鸣","制浆分厂","复合筛进浆槽搅拌器","40SKPT-AAA",2000000838,"台",1,"45KW",2013.9,"安德里兹","脱墨浆车间",{"v":97992.41,"d":"97,992.41"},{"v":76311.58,"d":"76,311.58"},"脱墨浆停产","良好"]
[6,"吉林晨鸣","制浆分厂","复合筛泵","S8-150-330.3",2000000839,"台",1," Q=350m3/h  H=30m C=1.88%   无缠绕式",2013.9,"苏尔寿","脱墨浆车间",{"v":71923.92,"d":"71,923.92"},{"v":56010.73,"d":"56,010.73"},"脱墨浆停产","良好"]
[7,"吉林晨鸣","制浆分厂","复合筛","CSM22B",2000000840,"台",1,"进浆浓度：1.88％  筛板孔径：2.0mm ，筛鼓孔径：2.2mm",2013.9,"VOITH  供货 ","脱墨浆车间",{"v":278252.38,"d":"278,252.38"},{"v":216689.03,"d":"216,689.03"},"脱墨浆停产","良好"]
[8,"吉林晨鸣","制浆分厂","高浓除渣器","HCC170-83S",2000000841,"台",1,"最大进浆压力：3.0bar   正常压降：1.3bar",2013.9,"VOITH  供货 ","脱墨浆车间",{"v":268013.43,"d":"268,013.43"},{"v":208715.47,"d":"208,715.47"},"脱墨浆停产","良好"]
[9,"吉林晨鸣","制浆分厂","一段重质除砂器","HCL5-IB3.48",2000000843,"台",48,"  最大进浆压力：4.0bar   正常压降：1.2-2.0bar",2013.9,"VOITH  供货 ","脱墨浆车间",{"v":228230.18,"d":"228,230.18"},{"v":177734.24,"d":"177,734.24"},"脱墨浆停产","良好"]
[10,"吉林晨鸣","制浆分厂","二段重质进浆泵","S8-150-330.3",2000000844,"台",1,"  Q=350m3/h    H=22m    C=1.55%",2013.9,"安德里兹","脱墨浆车间",{"v":68887.83,"d":"68,887.83"},{"v":53646.41,"d":"53,646.41"},"脱墨浆停产","良好"]
[11,"吉林晨鸣","制浆分厂","二段重质除砂器","HCL5-IB2.12",2000000845,"台",12,"  最大进浆压力：3.0bar   正常压降：1.3bar",2013.9,"VOITH  供货 ","脱墨浆车间",{"v":175768.65,"d":"175,768.65"},{"v":136879.83,"d":"136,879.83"},"脱墨浆停产","良好"]
[12,"吉林晨鸣","制浆分厂","三段重质进浆泵","S8-125-400.3",2000000846,"台",1,"  Q=130m3/h    H=35m    C=0.93%",2013.9,"安德里兹","脱墨浆车间",{"v":68469.06,"d":"68,469.06"},{"v":53320.27,"d":"53,320.27"},"脱墨浆停产","良好"]
[13,"吉林晨鸣","制浆分厂","三、四段重质除砂器","HGH5-IS6.1",2000000847,"台",4,"  最大进浆压力：4.0bar   正常压降：1.3bar",2013.9,"VOITH  供货 ","脱墨浆车间",{"v":207291.64,"d":"207,291.64"},{"v":161428.38,"d":"161,428.38"},"脱墨浆停产","良好"]
[14,"吉林晨鸣","制浆分厂","二段中浓筛泵","S8-150-330.3",2000000850,"台",1,"Q=350m3/h  H=20m C=1.50%",2013.9,"安德里兹","脱墨浆车间",{"v":68887.83,"d":"68,887.83"},{"v":53646.41,"d":"53,646.41"},"脱墨浆停产","良好"]
[15,"吉林晨鸣","制浆分厂","二段中浓预精筛","GFF800",2000000851,"台",1,"进浆浓度：1.5％  缝宽：0.2mm ",2013.9,"VOITH  供货 ","脱墨浆车间",{"v":198916.22,"d":"198,916.22"},{"v":154906.01,"d":"154,906.01"},"脱墨浆停产","良好"]
[16,"吉林晨鸣","制浆分厂","三段中浓筛泵","S8-100-265.3",2000000852,"台",1," Q=160m3/h  H=20m  C=0.88%",2013.9,"安德里兹","脱墨浆车间",{"v":49100.9,"d":"49,100.90"},{"v":38237.32,"d":"38,237.32"},"脱墨浆停产","良好"]
[17,"吉林晨鸣","制浆分厂","三段中浓筛","GFR600",2000000853,"台",1,"进浆浓度：0.88％   缝宽：0.20mm ",2013.9,"VOITH  供货 ","脱墨浆车间",{"v":173580.57,"d":"173,580.57"},{"v":135175.86,"d":"135,175.86"},"脱墨浆停产","良好"]
[18,"吉林晨鸣","制浆分厂","前浮选一段1#喂料泵","S8-500-600.3",2000000854,"台",1,"Q=1800m3/h  H=10m C=1.31%",2013.9,"苏尔寿","脱墨浆车间",{"v":177977.67,"d":"177,977.67"},{"v":138600.11,"d":"138,600.11"},"脱墨浆停产","良好"]
[19,"吉林晨鸣","制浆分厂","一段前浮选槽","ECC4/44P",2000000855,"台",1,"  进浆量：26312l/min   进浆浓度：1.31％",2013.9,"VOITH  供货 ","脱墨浆车间",{"v":1778465.91,"d":"1,778,465.91"},{"v":1384980.31,"d":"1,384,980.31"},"脱墨浆停产","良好"]
[20,"吉林晨鸣","制浆分厂","前浮选一段2#喂料泵","APP54-500/O",2000000856,"台",1,"Q=1800m3/h  H=10m C=1.31%",2013.9,"苏尔寿","脱墨浆车间",{"v":324547.51,"d":"324,547.51"},{"v":252741.36,"d":"252,741.36"},"脱墨浆停产","良好"]
[21,"吉林晨鸣","制浆分厂","前浮选一段3#喂料泵","APP54-500/O",2000000857,"台",1,"Q=1800m3/h  H=10m C=1.31%",2013.9,"苏尔寿","脱墨浆车间",{"v":324547.51,"d":"324,547.51"},{"v":252741.36,"d":"252,741.36"},"脱墨浆停产","良好"]
[22,"吉林晨鸣","制浆分厂","前浮选一段4#喂料泵","APP54-500/O",2000000858,"台",1,"Q=1800m3/h  H=10m C=1.31%",2013.9,"苏尔寿","脱墨浆车间",{"v":324547.51,"d":"324,547.51"},{"v":252741.36,"d":"252,741.36"},"脱墨浆停产","良好"]
[23,"吉林晨鸣","制浆分厂","前浮选一段5#喂料泵","APP54-500/O",2000000859,"台",1,"Q=1800m3/h  H=10m C=1.31%",2013.9,"苏尔寿","脱墨浆车间",{"v":324547.51,"d":"324,547.51"},{"v":252741.36,"d":"252,741.36"},"脱墨浆停产","良好"]
[24,"吉林晨鸣","制浆分厂","1#泡沫击碎器","FE3",2000000860,"台",1,"转子直径：1660mm  转速：279rpm",2013.9,"安德里兹","脱墨浆车间",{"v":56664.95,"d":"56,664.95"},{"v":44127.84,"d":"44,127.84"},"脱墨浆停产","良好"]
[25,"吉林晨鸣","制浆分厂","前浮选二段1#喂料泵","S8-200-380.3",2000000862,"台",1,"Q=500m3/h  H=25m  C=0.91%",2013.9,"安德里兹","脱墨浆车间",{"v":124060.9,"d":"124,060.90"},{"v":96612.42,"d":"96,612.42"},"脱墨浆停产","良好"]
[26,"吉林晨鸣","制浆分厂","前浮选二段槽","SFL5DD",2000000863,"台",1,"进浆量：7560l/min   进浆浓度：0.91％",2013.9,"安德里兹","脱墨浆车间",{"v":1778465.91,"d":"1,778,465.91"},{"v":1384980.31,"d":"1,384,980.31"},"脱墨浆停产","良好"]
[27,"吉林晨鸣","制浆分厂","前浮选二段2#喂料泵","APP43-250/O",2000000864,"台",1,"Q=500m3/h H=10m C=0.91%",2013.9,"苏尔寿","脱墨浆车间",{"v":129366.73,"d":"129,366.73"},{"v":100744.35,"d":"100,744.35"},"脱墨浆停产","良好"]
[28,"吉林晨鸣","制浆分厂","前浮选二段3#喂料泵","APP43-250/O",2000000865,"台",1,"Q=500m3/h H=10m C=0.91%",2013.9,"苏尔寿","脱墨浆车间",{"v":129366.73,"d":"129,366.73"},{"v":100744.35,"d":"100,744.35"},"脱墨浆停产","良好"]
[29,"吉林晨鸣","制浆分厂","前浮选一段良浆泵","S8-500-600.3",2000000866,"台",1,"Q=2200m3/h H=32m C=0.98%",2013.9,"苏尔寿","脱墨浆车间",{"v":177977.67,"d":"177,977.67"},{"v":138600.11,"d":"138,600.11"},"脱墨浆停产","良好"]
[30,"吉林晨鸣","制浆分厂","一段精筛","GFF-1200",2000000867,"台",1,"进浆浓度：0.98％  缝宽：0.15mm ",2013.9,"日本相川","脱墨浆车间",{"v":385269.3,"d":"385,269.30"},{"v":300028.46,"d":"300,028.46"},"脱墨浆停产","良好"]
[31,"吉林晨鸣","制浆分厂","二段精筛进浆泵","S8-200-380.3",2000000868,"台",1,"Q=700m3/h  H=24m  C=0.80%",2013.9,"苏尔寿","脱墨浆车间",{"v":124060.9,"d":"124,060.90"},{"v":96612.42,"d":"96,612.42"},"脱墨浆停产","良好"]
[32,"吉林晨鸣","制浆分厂","二段精筛","GFF-1000",2000000869,"台",1,"进浆浓度：0.80％ 缝宽：0.15mm ",2013.9,"日本相川","脱墨浆车间",{"v":311984.38,"d":"311,984.38"},{"v":242957.82,"d":"242,957.82"},"脱墨浆停产","良好"]
[33,"吉林晨鸣","制浆分厂","三段精筛进浆泵","S8-150-330.3",2000000870,"台",1,"Q=250m3/h  H=24m  C=0.65%",2013.9,"苏尔寿","脱墨浆车间",{"v":73075.54,"d":"73,075.54"},{"v":56907.57,"d":"56,907.57"},"脱墨浆停产","良好"]
[34,"吉林晨鸣","制浆分厂","四段精筛进浆泵","S8-100-265.3",2000000872,"台",1,"Q=140m3/h  H=24m  C=0.50%",2013.9,"苏尔寿","脱墨浆车间",{"v":59570.17,"d":"59,570.17"},{"v":46390.25,"d":"46,390.25"},"脱墨浆停产","良好"]
[35,"吉林晨鸣","制浆分厂","四段精筛","FH-400R",2000000873,"台",1,"进浆浓度：0.50％  缝宽：0.12mm ",2013.9,"日本相川","脱墨浆车间",{"v":186353.09,"d":"186,353.09"},{"v":145122.46,"d":"145,122.46"},"脱墨浆停产","良好"]
[36,"吉林晨鸣","制浆分厂","1#快速加热器","PMAS36",2000000878,"台",1,"进浆28-30%，出浆30%,  良浆能力：386 BDT/D",2013.9," VOITH","脱墨浆车间",{"v":939093.92,"d":"939,093.92"},{"v":731319.37,"d":"731,319.37"},"脱墨浆停产","良好"]
[37,"吉林晨鸣","制浆分厂","1#热分散机","KRD-110HC",2000000879,"台",1,"进浆浓度30%，出浆28%，能力：386 BDT/D",2013.9," VOITH","脱墨浆车间",{"v":4876588.06,"d":"4,876,588.06"},{"v":3797642.96,"d":"3,797,642.96"},"脱墨浆停产","良好"]
[38,"吉林晨鸣","制浆分厂","氧化漂白塔","HTC500-114",2000000880,"台",1,"计量140m3，直径φ5000X8800mm",2013.9,"VOITH  ","脱墨浆车间",{"v":314078.24,"d":"314,078.24"},{"v":244588.43,"d":"244,588.43"},"脱墨浆停产","良好"]
[39,"吉林晨鸣","制浆分厂","氧化漂白塔顶部散浆器","TES 100-7/40",2000000881,"台",1,"1500rpm  380V   B5   IP54  变频调速",2013.9,"VOITH  ","脱墨浆车间",{"v":121234.2,"d":"121,234.20"},{"v":94411.12,"d":"94,411.12"},"脱墨浆停产","良好"]
[40,"吉林晨鸣","制浆分厂","氧化漂白塔搅拌器","SLF-100.30D",2000000882,"台",3,"1500rpm  380V   B5   IP54",2013.9,"VOITH  ","脱墨浆车间",{"v":157039.12,"d":"157,039.12"},{"v":122294.22,"d":"122,294.22"},"脱墨浆停产","良好"]
[41,"吉林晨鸣","制浆分厂","漂白塔卸料泵","S8-250-430.3",2000000883,"台",1,"Q=550m3/h    H=12m    C=3.5%",2013.9,"苏尔寿","脱墨浆车间",{"v":164158.22,"d":"164,158.22"},{"v":127838.21,"d":"127,838.21"},"脱墨浆停产","良好"]
[42,"吉林晨鸣","制浆分厂","后浮选一段1#喂料泵","S8-350-470.3",2000000884,"台",1,"Q=1700m3/h  H=25m C=1.2%",2013.9,"苏尔寿","脱墨浆车间",{"v":172743.03,"d":"172,743.03"},{"v":134523.62,"d":"134,523.62"},"脱墨浆停产","良好"]
[43,"吉林晨鸣","制浆分厂","后浮选槽一段","ECC4/44P",2000000885,"台",1,"  进浆量：25376 l/min   进浆浓度：1.20％",2013.9,"VOITH  ","脱墨浆车间",{"v":2093854.9,"d":"2,093,854.90"},{"v":1630589.51,"d":"1,630,589.51"},"脱墨浆停产","良好"]
[44,"吉林晨鸣","制浆分厂","后浮选一段2#喂料泵","APP54-500/O",2000000886,"台",1,"Q=1700m3/h H=10m C=1.20%",2013.9,"苏尔寿","脱墨浆车间",{"v":324547.51,"d":"324,547.51"},{"v":252741.36,"d":"252,741.36"},"脱墨浆停产","良好"]
[45,"吉林晨鸣","制浆分厂","后浮选一段3#喂料泵","APP54-500/O",2000000887,"台",1,"Q=1700m3/h H=10m C=1.20%",2013.9,"苏尔寿","脱墨浆车间",{"v":324547.51,"d":"324,547.51"},{"v":252741.36,"d":"252,741.36"},"脱墨浆停产","良好"]
[46,"吉林晨鸣","制浆分厂","后浮选一段4#喂料泵","APP54-500/O",2000000888,"台",1,"Q=1700m3/h H=10m C=1.20%",2013.9,"苏尔寿","脱墨浆车间",{"v":324547.51,"d":"324,547.51"},{"v":252741.36,"d":"252,741.36"},"脱墨浆停产","良好"]
[47,"吉林晨鸣","制浆分厂","2#泡器击碎器","FE3",2000000889,"台",1,"    转子直径：1660mm  转速：279rpm",2013.9,"安德里兹","脱墨浆车间",{"v":56664.95,"d":"56,664.95"},{"v":44127.84,"d":"44,127.84"},"脱墨浆停产","良好"]
[48,"吉林晨鸣","制浆分厂","后浮选二段1#喂料泵","S8-150-330.3",2000000891,"台",1,"   Q=420m3/h  H=24m  C=1.0%",2013.9,"安德里兹","脱墨浆车间",{"v":93176.54,"d":"93,176.54"},{"v":72561.24,"d":"72,561.24"},"脱墨浆停产","良好"]
[49,"吉林晨鸣","制浆分厂","二段后浮选槽","SFL4DD",2000000892,"台",1,"  进浆量：6040l/min   进浆浓度：0.87％",2013.9,"安德里兹","脱墨浆车间",{"v":2093854.9,"d":"2,093,854.90"},{"v":1630589.51,"d":"1,630,589.51"},"脱墨浆停产","良好"]
[50,"吉林晨鸣","制浆分厂","后浮选二段2#喂料泵","S8-150-330.3",2000000893,"台",1,"Q=420m3/h H=10m C=0.87%",2013.9,"安德里兹","脱墨浆车间",{"v":83754.2,"d":"83,754.20"},{"v":65223.57,"d":"65,223.57"},"脱墨浆停产","良好"]
[51,"吉林晨鸣","制浆分厂","后浮选二段3#喂料泵","APP43-250/O",2000000894,"台",1,"Q=420m3/h H=10m C=0.87%",2013.9,"安德里兹","脱墨浆车间",{"v":131399.86,"d":"131,399.86"},{"v":102327.66,"d":"102,327.66"},"脱墨浆停产","良好"]
[52,"吉林晨鸣","制浆分厂","后浮选一段良浆泵","S8-350-470.3",2000000895,"台",1,"Q=1500m3/h H=24m C=1.22%",2013.9,"苏尔寿","脱墨浆车间",{"v":142172.75,"d":"142,172.75"},{"v":110717.04,"d":"110,717.04"},"脱墨浆停产","良好"]
[53,"吉林晨鸣","制浆分厂","后浮选二段良浆泵","S8-150-330.3",2000000896,"台",1,"Q=300m3/h H=10m C=0.69%",2013.9,"安德里兹","脱墨浆车间",837.54,652.23,"脱墨浆停产","良好"]
[54,"吉林晨鸣","制浆分厂","后多盘浓缩机","VDF5.2-16/15-325",2000000897,"台",1,"滤盘直径：5200mm    16盘  过滤面积：489m2",2013.9,"G&LV","脱墨浆车间",{"v":6051240.66,"d":"6,051,240.66"},{"v":4712403.66,"d":"4,712,403.66"},"脱墨浆停产","良好"]
[55,"吉林晨鸣","制浆分厂","输送斜螺旋","XWD6-17-11 中高：200MM",2000000898,"台",2,"处理量187BDT/D，11KW",2013.9,null,"脱墨浆车间",{"v":188446.94,"d":"188,446.94"},{"v":146753.07,"d":"146,753.07"},"脱墨浆停产","良好"]
[56,"吉林晨鸣","制浆分厂","2#3#螺旋挤浆机","SHX-900X5500",2000000899,"台",2,"螺旋直径：φ900mm， 螺旋长度：5500mm",2013.9,"日本相川","脱墨浆车间",{"v":1758838.12,"d":"1,758,838.12"},{"v":1369695.17,"d":"1,369,695.17"},"脱墨浆停产","良好"]
[57,"吉林晨鸣","制浆分厂","收集螺旋",null,2000000900,"台",1,"处理量373BDT/D，22KW",2013.9,null,"脱墨浆车间",{"v":117255.87,"d":"117,255.87"},{"v":91313.02,"d":"91,313.02"},"脱墨浆停产","良好"]
[58,"吉林晨鸣","制浆分厂","2#快速加热器","PMAS30",2000000901,"台",1,"处理浓浆28-30%， 入口温度45℃，出口温度90℃",2013.9,"VOITH  ","脱墨浆车间",{"v":123537.44,"d":"123,537.44"},{"v":96204.78,"d":"96,204.78"},"脱墨浆停产","良好"]
[59,"吉林晨鸣","制浆分厂","后热分散机","KRD85XLC",2000000902,"台",1,"进浆浓度30%，出浆28%, 能力410 BDt/d，浆温≤90℃",2013.9,"VOITH  ","脱墨浆车间",{"v":4899620.47,"d":"4,899,620.47"},{"v":3815579.45,"d":"3,815,579.45"},"脱墨浆停产","良好"]
[60,"吉林晨鸣","制浆分厂","2#中浓泵","LCE21-100V",2000000904,"台",1,"Q=180m3/h    H=70m    C=10%",2013.9,"苏尔寿","脱墨浆车间",{"v":374800.03,"d":"374,800.03"},{"v":291875.53,"d":"291,875.53"},"脱墨浆停产","良好"]
[61,"吉林晨鸣","制浆分厂","2-3bar 调浓白水泵","S8-200-380.3",2000000914,"台",1,"Q=500m3/h    H=30m    C=0.05%",2013.9,"安德里兹","脱墨浆车间",{"v":102598.89,"d":"102,598.89"},{"v":79898.89,"d":"79,898.89"},"脱墨浆停产","良好"]
[62,"吉林晨鸣","制浆分厂","冲洗白水泵","S8-150-400.3",2000000916,"台",1,"Q=300m3/h    H=50m    C=0.01%",2013.9,"苏尔寿","脱墨浆车间",{"v":58627.94,"d":"58,627.94"},{"v":45656.49,"d":"45,656.49"},"脱墨浆停产","良好"]
[63,"吉林晨鸣","制浆分厂","稀释白水泵","S8-150-400.3",2000000917,"台",1,"Q=360m3/h    H=40m    C=0.01%",2013.9,"安德里兹","脱墨浆车间",{"v":57581.01,"d":"57,581.01"},{"v":44841.2,"d":"44,841.20"},"脱墨浆停产","良好"]
[64,"吉林晨鸣","制浆分厂","开机冲洗白水泵","S8-200-470.3",2000000922,"台",1,"Q=400m3/h  H=60m",2013.9,"苏尔寿","脱墨浆车间",{"v":120396.66,"d":"120,396.66"},{"v":93758.89,"d":"93,758.89"},"脱墨浆停产","良好"]
[65,"吉林晨鸣","制浆分厂","开机补充白水泵","S8-500-600.3",2000000923,"台",1,"Q=1800m3/h  H=12m",2013.9,"苏尔寿","脱墨浆车间",{"v":186353.09,"d":"186,353.09"},{"v":145122.46,"d":"145,122.46"},"脱墨浆停产","良好"]
[66,"吉林晨鸣","制浆分厂","白水加热循环泵","S8-125-350.3",2000000924,"台",1,"Q=150m3/h  H=24m",2013.9,"苏尔寿","脱墨浆车间",{"v":81660.34,"d":"81,660.34"},{"v":63592.98,"d":"63,592.98"},"脱墨浆停产","良好"]
[67,"吉林晨鸣","制浆分厂","蒸汽喷射器",null,2000000925,"台",1,"白水流量：150m3/h，进水温度45℃，出水温度90℃；",2013.9,null,"脱墨浆车间",{"v":101028.5,"d":"101,028.50"},{"v":78675.96,"d":"78,675.96"},"脱墨浆停产","良好"]
[68,"吉林晨鸣","制浆分厂","2#高压喷淋白水泵","APP32-80/O",2000000928,"台",1,"Q=165m3/h    H=120m    C=0.01%",2013.9,"苏尔寿","脱墨浆车间",{"v":70353.52,"d":"70,353.52"},{"v":54787.8,"d":"54,787.80"},"脱墨浆停产","良好"]
[69,"吉林晨鸣","制浆分厂","4-5bar白水泵","APP33-125/C",2000000929,"台",1," Q=310m3/h    H=50m    C=0.01%",2013.9,"苏尔寿","脱墨浆车间",{"v":82183.8,"d":"82,183.80"},{"v":64000.64,"d":"64,000.64"},"脱墨浆停产","良好"]
[70,"吉林晨鸣","制浆分厂","调浓白水泵","S8-350-470.3",2000000930,"台",1,"Q=1500m3/h    H=30m    C=0.01%",2013.9,"安德里兹","脱墨浆车间",{"v":141335.21,"d":"141,335.21"},{"v":110064.8,"d":"110,064.80"},"脱墨浆停产","良好"]
[71,"吉林晨鸣","制浆分厂","补充白水泵","APP31-125/O",2000000931,"台",1,"Q=250m3/h    H=24m    C=0.01%",2013.9,"苏尔寿","脱墨浆车间",{"v":58627.94,"d":"58,627.94"},{"v":45656.49,"d":"45,656.49"},"脱墨浆停产","良好"]
[72,"吉林晨鸣","制浆分厂","1#气浮","CQJ-10",2000000932,"台",1,"处理水量：7650L/min，Φ10000mm  ",2013.9,"无锡沪东","脱墨浆车间",{"v":565340.82,"d":"565,340.82"},{"v":440259.14,"d":"440,259.14"},"脱墨浆停产","良好"]
[73,"吉林晨鸣","制浆分厂","1#气浮溶气泵",null,2000000933,"台",1,"Q=150 m3/h ,  H=70m,过流部分不锈钢 ",2013.9,"安德里兹","脱墨浆车间",{"v":51822.91,"d":"51,822.91"},{"v":40357.1,"d":"40,357.10"},"脱墨浆停产","良好"]
[74,"吉林晨鸣","制浆分厂","2#污泥泵","APP22-40/O",2000000935,"台",1," Q=20m3/h  H=15m C=1.0-2.0%",2013.9,"苏尔寿","脱墨浆车间",{"v":51194.75,"d":"51,194.75"},{"v":39867.93,"d":"39,867.93"},"脱墨浆停产","良好"]
[75,"吉林晨鸣","制浆分厂","1#污泥泵","APP42-150/O",2000000937,"台",1,"Q=300 m3/h, H=30m ,C=1.90% ，",2013.9,"安德里兹","脱墨浆车间",{"v":88988.83,"d":"88,988.83"},{"v":69300.03,"d":"69,300.03"},"脱墨浆停产","良好"]
[76,"吉林晨鸣","制浆分厂","重力床"," BD3XL",2000000938,"台",1,"工作面宽：3150mm,网案长度：10200mm，面积25.4m2",2013.9,"VOITH   ","脱墨浆车间",{"v":361189.97,"d":"361,189.97"},{"v":281276.68,"d":"281,276.68"},"脱墨浆停产","良好"]
[77,"吉林晨鸣","制浆分厂","污泥压榨螺旋","RSP-80",2000000939,"台",2,"能力:120 绝干t/d，进口浓度10-15%，出口浓度50%-60%",2013.9,"VOITH   ","脱墨浆车间",{"v":4187709.8,"d":"4,187,709.80"},{"v":3261179.01,"d":"3,261,179.01"},"脱墨浆停产","良好"]
[78,"吉林晨鸣","制浆分厂","滤液泵","APP31-125/O",2000000941,"台",1,"Q=250m3/h , H=25m",2013.9,"安德里兹","脱墨浆车间",{"v":73075.54,"d":"73,075.54"},{"v":56907.57,"d":"56,907.57"},"脱墨浆停产","良好"]
[79,"吉林晨鸣","制浆分厂","2#气浮","CQJ-10",2000000942,"台",1,"处理水量：5200L/min，Φ8000mm  ",2013.9,"无锡沪东","脱墨浆车间",{"v":565340.82,"d":"565,340.82"},{"v":440259.14,"d":"440,259.14"},"脱墨浆停产","良好"]
[80,"吉林晨鸣","制浆分厂","提渣机",null,2000000943,"台",1,"最大进料浓度6.0%，最大固体负荷1.72BDT/D",2013.9,"VOITH   ","脱墨浆车间",{"v":117674.65,"d":"117,674.65"},{"v":91639.13,"d":"91,639.13"},"脱墨浆停产","良好"]
[81,"吉林晨鸣","制浆分厂","DAF2滤液槽",null,2000000944,"台",1,"V=60m3 ,  不锈钢制    1.5~2.5%",2013.9,null,"脱墨浆车间",{"v":93176.54,"d":"93,176.54"},{"v":72561.24,"d":"72,561.24"},"脱墨浆停产","良好"]
[82,"吉林晨鸣","制浆分厂","滤液泵","APP22-65/C",2000000945,"台",1,"Q=60m3/h , H=15m",2013.9,"安德里兹","脱墨浆车间",{"v":58627.94,"d":"58,627.94"},{"v":45656.49,"d":"45,656.49"},"脱墨浆停产","良好"]
[83,"吉林晨鸣","制浆分厂","Na2SiO3卸料泵","IJ65-50-125",2000000950,"台",1,"Q=500 L/min ，H＝20m，316L不锈钢",2013.9,"杭州碱泵","脱墨浆车间",{"v":16332.07,"d":"16,332.07"},{"v":12718.61,"d":"12,718.61"},"脱墨浆停产","良好"]
[84,"吉林晨鸣","制浆分厂","Na2SiO3贮存槽",null,2000000951,"台",1,"V=60m3 ,浓度30%，,φ4000×5000mm",2013.9,null,"脱墨浆车间",{"v":68050.28,"d":"68,050.28"},{"v":52994.16,"d":"52,994.16"},"脱墨浆停产","良好"]
[85,"吉林晨鸣","制浆分厂","Na2SiO3计量泵","IJ25-25-130",2000000952,"台",1,"Q=15 L/min    H=40m   316L不锈钢",2013.9,"杭州碱泵","脱墨浆车间",{"v":12039.67,"d":"12,039.67"},{"v":9375.89,"d":"9,375.89"},"脱墨浆停产","良好"]
[86,"吉林晨鸣","制浆分厂","Na2SiO3计量泵","IJ25-25-160",2000000953,"台",1,"Q=15 L/min    H=40m  316L不锈钢",2013.9,"杭州碱泵","脱墨浆车间",{"v":12039.67,"d":"12,039.67"},{"v":9375.89,"d":"9,375.89"},"脱墨浆停产","良好"]
[87,"吉林晨鸣","制浆分厂","DTPA卸料泵",null,2000000957,"台",1,"Q=150 L/min ，H＝40m，316L不锈钢",2013.9,null,"脱墨浆车间",{"v":12039.67,"d":"12,039.67"},{"v":9375.89,"d":"9,375.89"},"脱墨浆停产","良好"]
[88,"吉林晨鸣","制浆分厂","DTPA贮存槽",null,2000000958,"台",1,"V=20m3 ,浓度30%，,φ2800×3750mm",2013.9,null,"脱墨浆车间",{"v":33501.68,"d":"33,501.68"},{"v":26089.43,"d":"26,089.43"},"脱墨浆停产","良好"]
[89,"吉林晨鸣","制浆分厂","DTPA计量泵",null,2000000959,"台",2,"Q=2 L/min    H=40m  316L不锈钢",2013.9,"大连红珊瑚","脱墨浆车间",{"v":12563.13,"d":"12,563.13"},{"v":9783.54,"d":"9,783.54"},"脱墨浆停产","良好"]
[90,"吉林晨鸣","制浆分厂","脱墨剂卸料泵",null,2000000960,"台",1,"Q=150 L/min ，H＝20m，316L不锈钢",2013.9,null,"脱墨浆车间",{"v":14133.52,"d":"14,133.52"},{"v":11006.47,"d":"11,006.47"},"脱墨浆停产","良好"]
[91,"吉林晨鸣","制浆分厂","脱墨剂贮存槽",null,2000000961,"台",1,"V=20m3 ,浓度30%，,φ3000×3750mm",2013.9,null,"脱墨浆车间",{"v":33501.68,"d":"33,501.68"},{"v":26089.43,"d":"26,089.43"},"脱墨浆停产","良好"]
[92,"吉林晨鸣","制浆分厂","脱墨剂计量泵",null,2000000962,"台",2,"Q=1.5 L/min    H=40m    316L不锈钢",2013.9,null,"脱墨浆车间",{"v":21985.48,"d":"21,985.48"},{"v":17121.18,"d":"17,121.18"},"脱墨浆停产","良好"]
[93,"吉林晨鸣","制浆分厂","硫酸卸料泵","IJ80-65-125",2000000963,"台",1,"Q=150 L/min ，H＝20m，316L不锈钢",2013.9,"杭州碱泵","脱墨浆车间",{"v":12039.67,"d":"12,039.67"},{"v":9375.89,"d":"9,375.89"},"脱墨浆停产","良好"]
[94,"吉林晨鸣","制浆分厂","硫酸贮存槽",null,2000000964,"台",1,"V=10m3 ,浓度98%，,φ2300×3000mm",2013.9,null,"脱墨浆车间",{"v":21985.48,"d":"21,985.48"},{"v":17121.18,"d":"17,121.18"},"脱墨浆停产","良好"]
[95,"吉林晨鸣","制浆分厂","硫酸计量泵",null,2000000965,"台",2,"Q=1.0 L/min    H=40m  316L不锈钢",2013.9,"大连红珊瑚","脱墨浆车间",{"v":24079.33,"d":"24,079.33"},{"v":18751.77,"d":"18,751.77"},"脱墨浆停产","良好"]
[96,"吉林晨鸣","制浆分厂","PAC卸料泵","IFK80-65-125",2000000966,"台",1,"Q=150 L/min ，H＝20m，316L不锈钢",2013.9,"杭州碱泵","脱墨浆车间",{"v":17274.3,"d":"17,274.30"},{"v":13452.37,"d":"13,452.37"},"脱墨浆停产","良好"]
[97,"吉林晨鸣","制浆分厂","PAC贮存槽",null,2000000967,"台",1,"V=10m3 ,浓度98%，,φ2300×3000mm",2013.9,null,"脱墨浆车间",{"v":10259.89,"d":"10,259.89"},{"v":7989.89,"d":"7,989.89"},"脱墨浆停产","良好"]
[98,"吉林晨鸣","制浆分厂","PAC计量泵","IJ25-25-160",2000000968,"台",2,"Q=1.5 L/min    H=40m  316L不锈钢",2013.9,"杭州碱泵","脱墨浆车间",{"v":11725.59,"d":"11,725.59"},{"v":9131.31,"d":"9,131.31"},"脱墨浆停产","良好"]
[99,"吉林晨鸣","制浆分厂","钠皂溶解槽",null,2000000969,"台",1,"V=5.0m3  φ1800×2000mm",2013.9,null,"脱墨浆车间",{"v":21985.48,"d":"21,985.48"},{"v":17121.18,"d":"17,121.18"},"脱墨浆停产","良好"]
[100,"吉林晨鸣","制浆分厂","卸料泵","IJ65-50-125",2000000970,"台",1,"Q=500 L/min ，H＝20m，316L不锈钢",2013.9,"杭州碱泵","脱墨浆车间",{"v":15494.53,"d":"15,494.53"},{"v":12066.38,"d":"12,066.38"},"脱墨浆停产","良好"]
[101,"吉林晨鸣","制浆分厂","钠皂贮存槽",null,2000000971,"台",1,"V=10m3    φ2300×3500mm",2013.9,null,"脱墨浆车间",{"v":33501.68,"d":"33,501.68"},{"v":26089.43,"d":"26,089.43"},"脱墨浆停产","良好"]
[102,"吉林晨鸣","制浆分厂","浮选钠皂计量泵","IJ40-25-200",2000000972,"台",1,"额定流量为50 L/min  H＝40 m",2013.9,"杭州碱泵","脱墨浆车间",{"v":11725.59,"d":"11,725.59"},{"v":9131.31,"d":"9,131.31"},"脱墨浆停产","良好"]
[103,"吉林晨鸣","制浆分厂","转鼓钠皂计量泵","IJ25-25-160",2000000973,"台",1,"额定流量为40 L/min  H＝40 m",2013.9,"杭州碱泵","脱墨浆车间",{"v":10259.89,"d":"10,259.89"},{"v":7989.89,"d":"7,989.89"},"脱墨浆停产","良好"]
[104,"吉林晨鸣","制浆分厂","F.A.S加料斗",null,2000000974,"台",1,"V=3m3， 不锈钢制    φ1500×1790mm",2013.9,null,"脱墨浆车间",{"v":10364.58,"d":"10,364.58"},{"v":8071.4,"d":"8,071.40"},"脱墨浆停产","良好"]
[105,"吉林晨鸣","制浆分厂","F.A.S贮存槽",null,2000000975,"台",1,"V=3m3， 不锈钢制     φ1500×2200mm",2013.9,null,"脱墨浆车间",{"v":10364.58,"d":"10,364.58"},{"v":8071.4,"d":"8,071.40"},"脱墨浆停产","良好"]
[106,"吉林晨鸣","制浆分厂","FAS计量泵","IJ25-25-160",2000000976,"台",2,"额定流量Q=30 L/min    H＝50m",2013.9,"杭州碱泵","脱墨浆车间",{"v":10259.89,"d":"10,259.89"},{"v":7989.89,"d":"7,989.89"},"脱墨浆停产","良好"]
[107,"吉林晨鸣","制浆分厂","低分子阳离子絮凝剂溶解槽",null,2000000977,"台",1,"V=5m3， 不锈钢制     φ1800×2000mm",2013.9,null,"脱墨浆车间",{"v":12563.13,"d":"12,563.13"},{"v":9783.54,"d":"9,783.54"},"脱墨浆停产","良好"]
[108,"吉林晨鸣","制浆分厂","阳离子卸料泵","IJ65-50-125",2000000978,"台",1,"Q=500 L/min ，H＝20m，316L不锈钢",2013.9,"杭州碱泵","脱墨浆车间",{"v":15913.3,"d":"15,913.30"},{"v":12392.47,"d":"12,392.47"},"脱墨浆停产","良好"]
[109,"吉林晨鸣","制浆分厂","低分子阳离子絮凝剂贮存槽",null,2000000979,"台",1,"V=10m3， 不锈钢制     φ2000×3000mm",2013.9,null,"脱墨浆车间",{"v":24602.8,"d":"24,602.80"},{"v":19159.42,"d":"19,159.42"},"脱墨浆停产","良好"]
[110,"吉林晨鸣","制浆分厂","低分子阳离子絮凝剂计量泵",null,2000000980,"台",2,"额定流量Q=30 L/min    H＝40m",2013.9,"杭州碱泵","脱墨浆车间",{"v":11516.2,"d":"11,516.20"},{"v":8968.24,"d":"8,968.24"},"脱墨浆停产","良好"]
[111,"吉林晨鸣","制浆分厂","高分子阴离子絮凝剂溶解槽",null,2000000981,"台",1,"V=5m3， 不锈钢制     φ1800×2000mm",2013.9,null,"脱墨浆车间",{"v":12563.13,"d":"12,563.13"},{"v":9783.54,"d":"9,783.54"},"脱墨浆停产","良好"]
[112,"吉林晨鸣","制浆分厂","高分子阴离子絮凝剂卸料泵","IJ65-50-125",2000000982,"台",1,"Q=500 L/min ，H＝20m，316L不锈钢",2013.9,"杭州碱泵","脱墨浆车间",{"v":15913.3,"d":"15,913.30"},{"v":12392.47,"d":"12,392.47"},"脱墨浆停产","良好"]
[113,"吉林晨鸣","制浆分厂","阴离子絮凝剂贮存槽",null,2000000983,"台",1,"V=10m3， 不锈钢制     φ2300×3000mm",2013.9,null,"脱墨浆车间",{"v":24602.8,"d":"24,602.80"},{"v":19159.42,"d":"19,159.42"},"脱墨浆停产","良好"]
[114,"吉林晨鸣","制浆分厂","阴离子计量泵","IJ25-25-200",2000000984,"台",2,"额定流量Q=30 L/min    H＝50m",2013.9,"杭州碱泵","脱墨浆车间",{"v":26173.19,"d":"26,173.19"},{"v":20382.39,"d":"20,382.39"},"脱墨浆停产","良好"]
[115,"吉林晨鸣","制浆分厂","凝结剂溶解槽",null,2000000985,"台",1,"V=5m3， 不锈钢制     φ1800×2000mm",2013.9,null,"脱墨浆车间",{"v":12563.13,"d":"12,563.13"},{"v":9783.54,"d":"9,783.54"},"脱墨浆停产","良好"]
[116,"吉林晨鸣","制浆分厂","凝结剂卸料泵","IJ65-50-125",2000000986,"台",1,"Q=500 L/min ，H＝20m，316L不锈钢",2013.9,"杭州碱泵","脱墨浆车间",{"v":15913.3,"d":"15,913.30"},{"v":12392.47,"d":"12,392.47"},"脱墨浆停产","良好"]
[117,"吉林晨鸣","制浆分厂","凝结剂贮存槽",null,2000000987,"台",1,"V=10m3， 不锈钢制     φ2300×3000mm",2013.9,null,"脱墨浆车间",{"v":24602.8,"d":"24,602.80"},{"v":19159.42,"d":"19,159.42"},"脱墨浆停产","良好"]
[118,"吉林晨鸣","制浆分厂","凝结剂计量泵","IJ25-25-200",2000000988,"台",2,"额定流量Q=30 L/min    H＝50m",2013.9,"杭州碱泵","脱墨浆车间",{"v":26173.19,"d":"26,173.19"},{"v":20382.39,"d":"20,382.39"},"脱墨浆停产","良好"]
[119,"吉林晨鸣","制浆分厂","减温装置",null,2000000991,"台",1,"入口蒸汽压力：0.7MPa(绝压），温度：250℃（过热蒸汽）出口蒸汽压力：0.7MPa（绝压），温度：165℃（饱和蒸汽）蒸汽量：15t/h",2013.9,null,"脱墨浆车间",{"v":152642.02,"d":"152,642.02"},{"v":118869.97,"d":"118,869.97"},"脱墨浆停产","良好"]
[120,"吉林晨鸣","制浆分厂","重力床喷淋水泵","CDLF16-82-7.5",2000000993,"台",1,"Q=30m3/h,H=80m",2013.9,"南方泵业","脱墨浆车间",{"v":10050.5,"d":"10,050.50"},{"v":7826.84,"d":"7,826.84"},"脱墨浆停产","良好"]
[121,"吉林晨鸣","制浆分厂","压滤机供料泵","S3-80-265DD",2000000996,"台",1,"Q=72m3/h    H=40m ",2013.9,"安德里兹","脱墨浆车间",{"v":54544.92,"d":"54,544.92"},{"v":42476.86,"d":"42,476.86"},"脱墨浆停产","良好"]
[122,"吉林晨鸣","制浆分厂","4#低浓除砂器供料泵","S3-80-265DD",2000000997,"台",1,"Q=72m3/h    H=40m ",2013.9,"安德里兹","脱墨浆车间",{"v":54544.92,"d":"54,544.92"},{"v":42476.86,"d":"42,476.86"},"脱墨浆停产","需维修"]
[123,"吉林晨鸣","制浆分厂","压滤机","CPN-NS2500S6",2000000998,"台",1,"外型：5.5*3.62*2.3",2013.9,"绿昇环保工程","脱墨浆车间",{"v":366424.61,"d":"366,424.61"},{"v":285353.15,"d":"285,353.15"},"脱墨浆停产","良好"]
[124,"吉林晨鸣","制浆分厂","2#泡沫槽",null,2000000890,"台",1,null,"2014-03-31",null,null,{"v":104692.75,"d":"104,692.75"},{"v":81529.49,"d":"81,529.49"},"脱墨浆停产","良好"]
[125,"吉林晨鸣","制浆分厂","中浓立管",null,2000000903,"台",1,null,"2014-03-31",null,null,{"v":1046927.45,"d":"1,046,927.45"},{"v":815294.75,"d":"815,294.75"},"脱墨浆停产","良好"]
[126,"吉林晨鸣","制浆分厂","蒸汽喷射器",null,2000000905,"台",1,null,"2014-03-31",null,null,{"v":38212.85,"d":"38,212.85"},{"v":29758.24,"d":"29,758.24"},"脱墨浆停产","良好"]
[127,"吉林晨鸣","制浆分厂","清白水槽",null,2000000913,"台",1,null,"2014-03-31",null,null,{"v":104692.75,"d":"104,692.75"},{"v":81529.49,"d":"81,529.49"},"脱墨浆停产","良好"]
[128,"吉林晨鸣","制浆分厂","浊白水槽",null,2000000926,"台",1,null,"2014-03-31",null,null,{"v":103645.82,"d":"103,645.82"},{"v":80714.19,"d":"80,714.19"},"脱墨浆停产","良好"]
[129,"吉林晨鸣","制浆分厂","清白水槽",null,2000000927,"台",1,null,"2014-03-31",null,null,{"v":104692.75,"d":"104,692.75"},{"v":81529.49,"d":"81,529.49"},"脱墨浆停产","良好"]
[130,"吉林晨鸣","制浆分厂","2#污泥槽",null,2000000934,"台",1,null,"2014-03-31",null,null,{"v":120396.66,"d":"120,396.66"},{"v":93758.89,"d":"93,758.89"},"脱墨浆停产","良好"]
[131,"吉林晨鸣","制浆分厂","1#污泥槽",null,2000000936,"台",1,null,"2014-03-31",null,null,{"v":104692.75,"d":"104,692.75"},{"v":81529.49,"d":"81,529.49"},"脱墨浆停产","良好"]
[132,"吉林晨鸣","制浆分厂","滤液槽",null,2000000940,"台",1,null,"2014-03-31",null,null,{"v":104692.75,"d":"104,692.75"},{"v":81529.49,"d":"81,529.49"},"脱墨浆停产","良好"]
[133,"吉林晨鸣","制浆分厂","跳筛","2㎡",2000000999,"台",1,null,"2014-03-31",null,null,{"v":44494.42,"d":"44,494.42"},{"v":34650.02,"d":"34,650.02"},"脱墨浆停产","良好"]
[134,"吉林晨鸣","制浆分厂","一体化温度变送器","STT25H-0-EN0-000-000-000",2000001007,"台",1,"0-100℃ M27X2","2014-03-31","霍尼韦尔",null,{"v":1732.35,"d":"1,732.35"},{"v":1349.06,"d":"1,349.06"},"脱墨浆停产","良好"]
[135,"吉林晨鸣","制浆分厂","一体化温度变送器","STT25H-0-EN0-000-000-000",2000001008,"台",1,"0-100℃ M27X2","2014-03-31","霍尼韦尔",null,{"v":1732.35,"d":"1,732.35"},{"v":1349.06,"d":"1,349.06"},"脱墨浆停产","良好"]
[136,"吉林晨鸣","制浆分厂","一体化温度变送器","STT25H-0-EN0-000-000-000",2000001009,"台",1,"0-100℃ M27X2","2014-03-31","霍尼韦尔",null,{"v":1732.35,"d":"1,732.35"},{"v":1349.06,"d":"1,349.06"},"脱墨浆停产","良好"]
[137,"吉林晨鸣","制浆分厂","一体化温度变送器","STT25H-0-EN0-000-000-000",2000001010,"台",1,"0-100℃ M27X2","2014-03-31","霍尼韦尔",null,{"v":1732.35,"d":"1,732.35"},{"v":1349.06,"d":"1,349.06"},"脱墨浆停产","良好"]
[138,"吉林晨鸣","制浆分厂","一体化温度变送器","STT25H-0-EN0-000-000-000",2000001011,"台",1,"0-100℃ M27X2","2014-03-31","霍尼韦尔",null,{"v":1732.35,"d":"1,732.35"},{"v":1349.06,"d":"1,349.06"},"脱墨浆停产","良好"]
[139,"吉林晨鸣","制浆分厂","一体化温度变送器","STT25H-0-EN0-000-000-000",2000001012,"台",1,"0-100℃ M27X2","2014-03-31","霍尼韦尔",null,{"v":1732.35,"d":"1,732.35"},{"v":1349.06,"d":"1,349.06"},"脱墨浆停产","良好"]
[140,"吉林晨鸣","制浆分厂","一体化温度变送器","STT25H-0-EN0-000-000-000",2000001013,"台",1,"0-100℃ M27X2","2014-03-31","霍尼韦尔",null,{"v":1732.35,"d":"1,732.35"},{"v":1349.06,"d":"1,349.06"},"脱墨浆停产","报废"]
[141,"吉林晨鸣","制浆分厂","一体化温度变送器","STT25H-0-EN0-000-000-000",2000001014,"台",1,"0-100℃ M27X2","2014-03-31","霍尼韦尔",null,{"v":1732.35,"d":"1,732.35"},{"v":1349.06,"d":"1,349.06"},"脱墨浆停产","报废"]
[142,"吉林晨鸣","制浆分厂","一体化温度变送器","STT25H-0-EN0-000-000-000",2000001015,"台",1,"0-100℃ M27X2","2014-03-31","霍尼韦尔",null,{"v":1732.35,"d":"1,732.35"},{"v":1349.06,"d":"1,349.06"},"脱墨浆停产","报废"]
[143,"吉林晨鸣","制浆分厂","一体化温度变送器","STT25H-0-EN0-000-000-000",2000001016,"台",1,"0-100℃ M27X2","2014-03-31","霍尼韦尔",null,{"v":1732.35,"d":"1,732.35"},{"v":1349.06,"d":"1,349.06"},"脱墨浆停产","报废"]
[144,"吉林晨鸣","制浆分厂","pH/温度","TB82PH",2000001017,"台",1,"插入式探头 0-14   盘柜安装支架","2014-03-31","ABB",null,{"v":6468.65,"d":"6,468.65"},{"v":5037.45,"d":"5,037.45"},"脱墨浆停产","报废"]
[145,"吉林晨鸣","制浆分厂","气动开关闸板阀","MV-E-600-P-TY-2ILS-SV-EC",2000001022,"台",1,"DN600 PN16","2014-03-31","依博罗",null,{"v":65009.94,"d":"65,009.94"},{"v":50626.47,"d":"50,626.47"},"脱墨浆停产","良好"]
[146,"吉林晨鸣","制浆分厂","气动开关闸板阀","MV-E-450-P-TY-2ILS-SV-EC",2000001023,"台",1,"DN450 PN16","2014-03-31","依博罗",null,{"v":32978.21,"d":"32,978.21"},{"v":25681.77,"d":"25,681.77"},"脱墨浆停产","良好"]
[147,"吉林晨鸣","制浆分厂","气动开关闸板阀","MV-E-250-P-TY-2ILS-SV-EC",2000001024,"台",1,"DN250 PN16","2014-03-31","依博罗",null,{"v":22711.47,"d":"22,711.47"},{"v":17686.54,"d":"17,686.54"},"脱墨浆停产","良好"]
[148,"吉林晨鸣","制浆分厂","气动开关闸板阀","MV-E-450-P-TY-2ILS-SV-EC",2000001025,"台",1,"DN450 PN16","2014-03-31","依博罗",null,{"v":32978.21,"d":"32,978.21"},{"v":25681.77,"d":"25,681.77"},"脱墨浆停产","良好"]
[149,"吉林晨鸣","制浆分厂","气动开关闸板阀","MV-E-500-P-TY-2ILS-SV-EC",2000001026,"台",1,"DN500 PN16","2014-03-31","依博罗",null,{"v":42925.96,"d":"42,925.96"},{"v":33428.58,"d":"33,428.58"},"脱墨浆停产","良好"]
[150,"吉林晨鸣","制浆分厂","气动开关闸板阀","MV-E-400-P-TY-2ILS-SV-EC",2000001027,"台",1,"DN400 PN16","2014-03-31","依博罗",null,{"v":25395.92,"d":"25,395.92"},{"v":19777.05,"d":"19,777.05"},"脱墨浆停产","良好"]
[151,"吉林晨鸣","制浆分厂","气动开关闸板阀","HG-E-400-PV-TY-2ILS-SV-E",2000001028,"台",1,"DN400 PN16","2014-03-31","依博罗",null,{"v":25395.92,"d":"25,395.92"},{"v":19777.05,"d":"19,777.05"},"脱墨浆停产","报废"]
[152,"吉林晨鸣","制浆分厂","气动开关闸板阀","HG-E-400-PV-TY-2ILS-SV-E",2000001029,"台",1,"DN400 PN16","2014-03-31","依博罗",null,{"v":25395.92,"d":"25,395.92"},{"v":19777.05,"d":"19,777.05"},"脱墨浆停产","报废"]
[153,"吉林晨鸣","制浆分厂","气动开关闸板阀","HG-E-400-PV-TY-2ILS-SV-E",2000001030,"台",1,"DN400 PN16","2014-03-31","依博罗",null,{"v":25395.92,"d":"25,395.92"},{"v":19777.05,"d":"19,777.05"},"脱墨浆停产","良好"]
[154,"吉林晨鸣","制浆分厂","气动开关闸板阀","MV-E-400-P-TY-2ILS-SV-EC",2000001031,"台",1,"DN400 PN16","2014-03-31","依博罗",null,{"v":25395.92,"d":"25,395.92"},{"v":19777.05,"d":"19,777.05"},"脱墨浆停产","良好"]
[155,"吉林晨鸣","制浆分厂","气动开关闸板阀","MV-E-400-P-TY-2ILS-SV-EC",2000001033,"台",1,"DN400 PN16","2014-03-31","依博罗",null,{"v":25395.92,"d":"25,395.92"},{"v":19777.05,"d":"19,777.05"},"脱墨浆停产","良好"]
[156,"吉林晨鸣","制浆分厂","气动开关闸板阀","MV-E-400-P-TY-2ILS-SV-EC",2000001034,"台",1,"DN400 PN16","2014-03-31","依博罗",null,{"v":25395.92,"d":"25,395.92"},{"v":19777.05,"d":"19,777.05"},"脱墨浆停产","良好"]
[157,"吉林晨鸣","制浆分厂","气动开关闸板阀","MV-E-400-P-TY-2ILS-SV-EC",2000001036,"台",1,"DN400 PN16","2014-03-31","依博罗",null,{"v":25395.92,"d":"25,395.92"},{"v":19777.05,"d":"19,777.05"},"脱墨浆停产","良好"]
[158,"吉林晨鸣","制浆分厂","气动开关闸板阀","MV-E-450-P-TY-2ILS-SV-EC",2000001037,"台",1,"DN450 PN16","2014-03-31","依博罗",null,{"v":32978.21,"d":"32,978.21"},{"v":25681.77,"d":"25,681.77"},"脱墨浆停产","良好"]
[159,"吉林晨鸣","制浆分厂","气动开关闸板阀","MV-E-350-P-TY-2ILS-SV-EC",2000001038,"台",1,"DN350 PN16","2014-03-31","依博罗",null,{"v":20959.59,"d":"20,959.59"},{"v":16322.28,"d":"16,322.28"},"脱墨浆停产","良好"]
[160,"吉林晨鸣","制浆分厂","气动开关闸板阀","MV-E-100-P-TY-2ILS-SV-EC",2000001039,"台",1,"DN100 PN16","2014-03-31","依博罗",null,{"v":4922.64,"d":"4,922.64"},{"v":3833.5,"d":"3,833.50"},"脱墨浆停产","良好"]
[161,"吉林晨鸣","制浆分厂","液体音叉限位开关","7ML5747-2DB52-1AA0-Z Y01",2000001040,"台",1,"插入式 螺纹连接 水介质","2014-03-31","西门子",null,{"v":5479.89,"d":"5,479.89"},{"v":4267.46,"d":"4,267.46"},"脱墨浆停产","报废"]
[162,"吉林晨鸣","制浆分厂","液体音叉限位开关","7ML5747-2DB52-1AA0-Z Y01",2000001041,"台",1,"插入式 螺纹连接 水介质","2014-03-31","西门子",null,{"v":5479.89,"d":"5,479.89"},{"v":4267.46,"d":"4,267.46"},"脱墨浆停产","报废"]
[163,"吉林晨鸣","制浆分厂","电容式料位开关","7ML5630-0AN00-0DA0-Z Y01",2000001042,"台",1,null,"2014-03-31",null,null,{"v":5479.89,"d":"5,479.89"},{"v":4267.46,"d":"4,267.46"},"脱墨浆停产","良好"]
[164,"吉林晨鸣","制浆分厂","电容式料位开关","7ML5630-0AN00-0DA0-Z Y01",2000001043,"台",1,null,"2014-03-31",null,null,{"v":5479.89,"d":"5,479.89"},{"v":4267.46,"d":"4,267.46"},"脱墨浆停产","良好"]
[165,"吉林晨鸣","制浆分厂","电容式料位开关","7ML5630-0AN00-0DA0-Z Y01",2000001044,"台",1,null,"2014-03-31",null,null,{"v":5479.89,"d":"5,479.89"},{"v":4267.46,"d":"4,267.46"},"脱墨浆停产","良好"]
[166,"吉林晨鸣","制浆分厂","电容式料位开关","7ML5630-0AN00-0DA0-Z Y01",2000001045,"台",1,null,"2014-03-31",null,null,{"v":5479.89,"d":"5,479.89"},{"v":4267.46,"d":"4,267.46"},"脱墨浆停产","良好"]
[167,"吉林晨鸣","制浆分厂","电容式料位开关","7ML5630-0AM00-0HA0-Z Y01",2000001046,"台",1,null,"2014-03-31",null,null,{"v":5479.89,"d":"5,479.89"},{"v":4267.46,"d":"4,267.46"},"脱墨浆停产","良好"]
[168,"吉林晨鸣","制浆分厂","电磁流量计","OPTIFLUX4100W(15)1144102",2000001086,"台",1,"DN15 PN16","2014-03-31","科隆",null,{"v":4483,"d":"4,483.00"},{"v":3491.14,"d":"3,491.14"},"脱墨浆停产","良好"]
[169,"吉林晨鸣","制浆分厂","电磁流量计","OPTIFLUX4100W(15)1144102",2000001087,"台",1,"DN15 PN16","2014-03-31","科隆",null,{"v":4483,"d":"4,483.00"},{"v":3491.14,"d":"3,491.14"},"脱墨浆停产","良好"]
[170,"吉林晨鸣","制浆分厂","电磁流量计","OPTIFLUX4100W(32)1164102",2000001088,"台",1,"DN32 PN16","2014-03-31","科隆",null,{"v":4711.17,"d":"4,711.17"},{"v":3668.84,"d":"3,668.84"},"脱墨浆停产","良好"]
[171,"吉林晨鸣","制浆分厂","电磁流量计","OPTIFLUX4100W(32)1164102",2000001089,"台",1,"DN32 PN16","2014-03-31","科隆",null,{"v":4711.17,"d":"4,711.17"},{"v":3668.84,"d":"3,668.84"},"脱墨浆停产","良好"]
[172,"吉林晨鸣","制浆分厂","电磁流量计","OPTIFLUX4100W(32)1164102",2000001090,"台",1,"DN32 PN16","2014-03-31","科隆",null,{"v":4711.17,"d":"4,711.17"},{"v":3668.84,"d":"3,668.84"},"脱墨浆停产","良好"]
[173,"吉林晨鸣","制浆分厂","电磁流量计","OPTIFLUX4100W(40)1164102",2000001091,"台",1,"DN40 PN16","2014-03-31","科隆",null,{"v":4837.5,"d":"4,837.50"},{"v":3767.19,"d":"3,767.19"},"脱墨浆停产","良好"]
[174,"吉林晨鸣","制浆分厂","电磁流量计","OPTIFLUX4100W(32)1164102",2000001098,"台",1,"DN32 PN16","2014-03-31","科隆",null,{"v":4711.17,"d":"4,711.17"},{"v":3668.84,"d":"3,668.84"},"脱墨浆停产","良好"]
[175,"吉林晨鸣","制浆分厂","电磁流量计","OPTIFLUX4100W(32)1164102",2000001099,"台",1,"DN32 PN16","2014-03-31","科隆",null,{"v":4711.17,"d":"4,711.17"},{"v":3668.84,"d":"3,668.84"},"脱墨浆停产","良好"]
[176,"吉林晨鸣","制浆分厂","涡街流量计","AE225",2000001101,"台",1,"DN250 PN16","2014-03-31","横河",null,{"v":9527.04,"d":"9,527.04"},{"v":7419.17,"d":"7,419.17"},"脱墨浆停产","良好"]
[177,"吉林晨鸣","制浆分厂","平衡流量计"," AKPPD006P24MAMBSWABCDJ",2000001102,"台",1,"引压式 带三阀组","2014-03-31","科隆",null,{"v":38924.23,"d":"38,924.23"},{"v":30312.25,"d":"30,312.25"},"脱墨浆停产","良好"]
[178,"吉林晨鸣","制浆分厂","平衡流量计"," AKPPD006P24MAMBSWABCDJ",2000001103,"台",1,"引压式 带三阀组","2014-03-31","科隆",null,{"v":38924.23,"d":"38,924.23"},{"v":30312.25,"d":"30,312.25"},"脱墨浆停产","良好"]
[179,"吉林晨鸣","制浆分厂","电磁流量计","OPTIFLUX4100W(32)1164102",2000001104,"台",1,"DN32 PN16","2014-03-31","科隆",null,{"v":4711.17,"d":"4,711.17"},{"v":3668.84,"d":"3,668.84"},"脱墨浆停产","良好"]
[180,"吉林晨鸣","制浆分厂","气动V型调节球阀","ZSSV-16TK15YPD2LP",2000001139,"台",1,"DN15 PN16","2014-03-31","力诺",null,{"v":2222.85,"d":"2,222.85"},{"v":1731.04,"d":"1,731.04"},"脱墨浆停产","良好"]
[181,"吉林晨鸣","制浆分厂","气动V型调节球阀","ZSSV-16TK50YPD2LP",2000001140,"台",1,"DN50 PN16","2014-03-31","力诺",null,{"v":3365.09,"d":"3,365.09"},{"v":2620.56,"d":"2,620.56"},"脱墨浆停产","良好"]
[182,"吉林晨鸣","制浆分厂","气动V型调节球阀","ZSSV-16TK50YPD2LP",2000001141,"台",1,"DN50 PN16","2014-03-31","力诺",null,{"v":3365.09,"d":"3,365.09"},{"v":2620.56,"d":"2,620.56"},"脱墨浆停产","良好"]
[183,"吉林晨鸣","制浆分厂","气动V型调节球阀","ZSSV-16TK15YPD2LP",2000001142,"台",1,"DN15 PN16","2014-03-31","力诺",null,{"v":2222.85,"d":"2,222.85"},{"v":1731.04,"d":"1,731.04"},"脱墨浆停产","良好"]
[184,"吉林晨鸣","制浆分厂","气动V型调节球阀","ZSSV-16TK15YPD2LP",2000001143,"台",1,"DN15 PN16","2014-03-31","力诺",null,{"v":2222.85,"d":"2,222.85"},{"v":1731.04,"d":"1,731.04"},"脱墨浆停产","良好"]
[185,"吉林晨鸣","制浆分厂","气动V型调节球阀","ZSSV-16TK15YPD2LP",2000001144,"台",1,"DN15 PN16","2014-03-31","力诺",null,{"v":2222.85,"d":"2,222.85"},{"v":1731.04,"d":"1,731.04"},"脱墨浆停产","良好"]
[186,"吉林晨鸣","制浆分厂","气动V型调节球阀","ZSSV-16TK25YPD2LP",2000001145,"台",1,"DN25 PN16","2014-03-31","力诺",null,{"v":3846.67,"d":"3,846.67"},{"v":2995.59,"d":"2,995.59"},"脱墨浆停产","良好"]
[187,"吉林晨鸣","制浆分厂","气动V型调节球阀","ZSSV-16TK40YPD2LP",2000001146,"台",1,"DN40 PN16","2014-03-31","力诺",null,{"v":3846.67,"d":"3,846.67"},{"v":2995.59,"d":"2,995.59"},"脱墨浆停产","良好"]
[188,"吉林晨鸣","制浆分厂","气动V型调节球阀","ZSSV-16TK40YPD2LP",2000001147,"台",1,"DN40 PN16","2014-03-31","力诺",null,{"v":3846.67,"d":"3,846.67"},{"v":2995.59,"d":"2,995.59"},"脱墨浆停产","良好"]
[189,"吉林晨鸣","制浆分厂","气动V型调节球阀","ZSSV-16TK40YPD2LP",2000001148,"台",1,"DN40 PN16","2014-03-31","力诺",null,{"v":3846.67,"d":"3,846.67"},{"v":2995.59,"d":"2,995.59"},"脱墨浆停产","良好"]
[190,"吉林晨鸣","制浆分厂","气动V型调节球阀","ZSSV-16TK32YPD2LP",2000001149,"台",1,"DN32 PN16","2014-03-31","力诺",null,{"v":3846.67,"d":"3,846.67"},{"v":2995.59,"d":"2,995.59"},"脱墨浆停产","良好"]
[191,"吉林晨鸣","制浆分厂","气动V型调节球阀","ZSSV-16TK40YPD2LP",2000001150,"台",1,"DN40 PN16","2014-03-31","力诺",null,{"v":3846.67,"d":"3,846.67"},{"v":2995.59,"d":"2,995.59"},"脱墨浆停产","良好"]
[192,"吉林晨鸣","制浆分厂","气动V型调节球阀","ZSSV-16TK65YPD2LP",2000001157,"台",1,"DN65 PN16","2014-03-31","力诺",null,{"v":1637.5,"d":"1,637.50"},{"v":1275.19,"d":"1,275.19"},"脱墨浆停产","良好"]
[193,"吉林晨鸣","制浆分厂","气动V型调节球阀","ZSSV-16TK65YPD2LP",2000001158,"台",1,"DN65 PN16","2014-03-31","力诺",null,{"v":1637.5,"d":"1,637.50"},{"v":1275.19,"d":"1,275.19"},"脱墨浆停产","良好"]
[194,"吉林晨鸣","制浆分厂","气动V型调节球阀","ZSSV-16TK40YPD2LP",2000001159,"台",1,"DN40 PN16","2014-03-31","力诺",null,{"v":1637.5,"d":"1,637.50"},{"v":1275.19,"d":"1,275.19"},"脱墨浆停产","良好"]
[195,"吉林晨鸣","制浆分厂","气动V型调节球阀","ZSSV-16TK40YPD2LP",2000001160,"台",1,"DN40 PN16","2014-03-31","力诺",null,{"v":1637.5,"d":"1,637.50"},{"v":1275.19,"d":"1,275.19"},"脱墨浆停产","良好"]
[196,"吉林晨鸣","制浆分厂","气动V型调节球阀","ZSSV-16TK125YPD2LP",2000001161,"台",1,"DN125 PN16","2014-03-31","力诺",null,{"v":3509.34,"d":"3,509.34"},{"v":2732.9,"d":"2,732.90"},"脱墨浆停产","良好"]
[197,"吉林晨鸣","制浆分厂","气动V型调节球阀","ZSSV-16TK100YPD2LP",2000001162,"台",1,"DN100 PN16","2014-03-31","力诺",null,{"v":2013.35,"d":"2,013.35"},{"v":1567.9,"d":"1,567.90"},"脱墨浆停产","良好"]
[198,"吉林晨鸣","制浆分厂","气动O型开关球阀","ZSSR-16EK32YPD4BLP",2000001163,"台",1,"DN32 PN16","2014-03-31","力诺",null,{"v":1387.56,"d":"1,387.56"},{"v":1080.56,"d":"1,080.56"},"脱墨浆停产","良好"]
[199,"吉林晨鸣","制浆分厂","气动O型开关球阀","ZSSR-16EK65YPD4BLP",2000001164,"台",1,"DN65 PN16","2014-03-31","力诺",null,{"v":1637.5,"d":"1,637.50"},{"v":1275.19,"d":"1,275.19"},"脱墨浆停产","良好"]
[200,"吉林晨鸣","制浆分厂","气动O型开关球阀","ZSSR-16EK25YPD4BLP",2000001165,"台",1,"DN25 PN16","2014-03-31","力诺",null,{"v":2222.85,"d":"2,222.85"},{"v":1731.04,"d":"1,731.04"},"脱墨浆停产","良好"]
[201,"吉林晨鸣","制浆分厂","气动O型开关球阀","ZSSR-16EK40YPD4BLP",2000001166,"台",1,"DN40 PN16","2014-03-31","力诺",null,{"v":2222.85,"d":"2,222.85"},{"v":1731.04,"d":"1,731.04"},"脱墨浆停产","良好"]
[202,"吉林晨鸣","制浆分厂","气动O型开关球阀","ZSSR-16EK25YPD4BLP",2000001167,"台",1,"DN25 PN16","2014-03-31","力诺",null,{"v":3846.67,"d":"3,846.67"},{"v":2995.59,"d":"2,995.59"},"脱墨浆停产","良好"]
[203,"吉林晨鸣","制浆分厂","气动O型开关球阀","ZSSR-16EK50YPD4BLP",2000001168,"台",1,"DN50 PN16","2014-03-31","力诺",null,{"v":3846.67,"d":"3,846.67"},{"v":2995.59,"d":"2,995.59"},"脱墨浆停产","良好"]
[204,"吉林晨鸣","制浆分厂","气动O型开关球阀","ZSSR-16ESB32YPD4BLP",2000001169,"台",1,"DN32 PN16","2014-03-31","力诺",null,{"v":3846.67,"d":"3,846.67"},{"v":2995.59,"d":"2,995.59"},"脱墨浆停产","良好"]
[205,"吉林晨鸣","制浆分厂","气动O型开关球阀","ZSSR-16EK25YPD4BLP",2000001170,"台",1,"DN25 PN16","2014-03-31","力诺",null,{"v":3846.67,"d":"3,846.67"},{"v":2995.59,"d":"2,995.59"},"脱墨浆停产","良好"]
[206,"吉林晨鸣","制浆分厂","气动O型开关球阀","ZSSR-16EK25YPD4BLP",2000001171,"台",1,"DN25 PN16","2014-03-31","力诺",null,{"v":3846.67,"d":"3,846.67"},{"v":2995.59,"d":"2,995.59"},"脱墨浆停产","良好"]
[207,"吉林晨鸣","制浆分厂","气动O型开关球阀","ZSSR-16EK20YPD4BLP",2000001172,"台",1,"DN20 PN16","2014-03-31","力诺",null,{"v":3846.67,"d":"3,846.67"},{"v":2995.59,"d":"2,995.59"},"脱墨浆停产","良好"]
[208,"吉林晨鸣","制浆分厂","气动O型开关球阀","ZSSR-16EK32YPD4BLP",2000001173,"台",1,"DN32 PN16","2014-03-31","力诺",null,{"v":4899.83,"d":"4,899.83"},{"v":3815.75,"d":"3,815.75"},"脱墨浆停产","良好"]
[209,"吉林晨鸣","制浆分厂","气动O型开关球阀","ZSSR-16ESB40YPD4BLP",2000001174,"台",1,"DN40 PN16","2014-03-31","力诺",null,{"v":1637.5,"d":"1,637.50"},{"v":1275.19,"d":"1,275.19"},"脱墨浆停产","良好"]
[210,"吉林晨鸣","制浆分厂","气动O型开关球阀","ZSSR-16ESB50YPD4BLP",2000001175,"台",1,"DN50 PN16","2014-03-31","力诺",null,{"v":3509.34,"d":"3,509.34"},{"v":2732.9,"d":"2,732.90"},"脱墨浆停产","良好"]
[211,"吉林晨鸣","制浆分厂","气动O型开关球阀","ZSSR-16EK50YPD4BLP",2000001176,"台",1,"DN50 PN16","2014-03-31","力诺",null,{"v":1637.5,"d":"1,637.50"},{"v":1275.19,"d":"1,275.19"},"脱墨浆停产","良好"]
[212,"吉林晨鸣","制浆分厂","气动O型开关球阀","ZSSR-16EK150YPD4BLP",2000001177,"台",1,"DN150 PN16","2014-03-31","力诺",null,{"v":1637.5,"d":"1,637.50"},{"v":1275.19,"d":"1,275.19"},"脱墨浆停产","良好"]
[213,"吉林晨鸣","制浆分厂","气动O型开关球阀","ZSSR-16EK50YPD4BLP",2000001189,"台",1,"DN50 PN16","2014-03-31","力诺",null,{"v":4413.52,"d":"4,413.52"},{"v":3437.02,"d":"3,437.02"},"脱墨浆停产","良好"]
[214,"吉林晨鸣","制浆分厂","气动O型开关球阀","ZSSR-16EK50YPD4BLP",2000001190,"台",1,"DN50 PN16","2014-03-31","力诺",null,{"v":4413.52,"d":"4,413.52"},{"v":3437.02,"d":"3,437.02"},"脱墨浆停产","良好"]
[215,"吉林晨鸣","制浆分厂","气动开关蝶阀","ZSSW-16EK150MPD4BLP",2000001191,"台",1,"DN150 PN16","2014-03-31","力诺",null,{"v":4413.52,"d":"4,413.52"},{"v":3437.02,"d":"3,437.02"},"脱墨浆停产","良好"]
[216,"吉林晨鸣","制浆分厂","气动开关蝶阀","ZSSW-16EK150MPD4BLP",2000001192,"台",1,"DN150 PN16","2014-03-31","力诺",null,{"v":4413.52,"d":"4,413.52"},{"v":3437.02,"d":"3,437.02"},"脱墨浆停产","良好"]
[217,"吉林晨鸣","制浆分厂","气动V型调节球阀","ZSSR-16ESB15YPD4BLP",2000001193,"台",1,"DN15 PN16","2014-03-31","力诺",null,{"v":4413.52,"d":"4,413.52"},{"v":3437.02,"d":"3,437.02"},"脱墨浆停产","良好"]
[218,"吉林晨鸣","制浆分厂","气动开关蝶阀","ZSSW-16EK200MPD4BLP",2000001194,"台",1,"DN200 PN16","2014-03-31","力诺",null,{"v":3060.27,"d":"3,060.27"},{"v":2383.2,"d":"2,383.20"},"脱墨浆停产","良好"]
[219,"吉林晨鸣","制浆分厂","气动O型开关球阀","ZSSR-16EK32YPD4BLP",2000001195,"台",1,"DN32 PN16","2014-03-31","力诺",null,{"v":4899.83,"d":"4,899.83"},{"v":3815.75,"d":"3,815.75"},"脱墨浆停产","良好"]
[220,"吉林晨鸣","制浆分厂","气动O型开关球阀","ZSSR-16EK65YPD4BLP",2000001196,"台",1,"DN65 PN16","2014-03-31","力诺",null,{"v":1637.5,"d":"1,637.50"},{"v":1275.19,"d":"1,275.19"},"脱墨浆停产","良好"]
[221,"吉林晨鸣","制浆分厂","气动O型开关球阀","ZSSR-16EK50YPD4BLP",2000001197,"台",1,"DN50 PN16","2014-03-31","力诺",null,{"v":3509.34,"d":"3,509.34"},{"v":2732.9,"d":"2,732.90"},"脱墨浆停产","良好"]
[222,"吉林晨鸣","制浆分厂","气动开关蝶阀","ZSSW-16EK200MPD4BLP",2000001198,"台",1,"DN200 PN16","2014-03-31","力诺",null,{"v":3060.27,"d":"3,060.27"},{"v":2383.2,"d":"2,383.20"},"脱墨浆停产","良好"]
[223,"吉林晨鸣","制浆分厂","气动O型开关球阀","ZSSR-16EK40YPD4BLP",2000001199,"台",1,"DN40 PN16","2014-03-31","力诺",null,{"v":3060.27,"d":"3,060.27"},{"v":2383.2,"d":"2,383.20"},"脱墨浆停产","良好"]
[224,"吉林晨鸣","制浆分厂","气动O型开关球阀","ZSSR-16EK40YPD4BLP",2000001200,"台",1,"DN40 PN16","2014-03-31","力诺",null,{"v":2013.35,"d":"2,013.35"},{"v":1567.9,"d":"1,567.90"},"脱墨浆停产","良好"]
[225,"吉林晨鸣","制浆分厂","气动O型开关球阀","ZSSR-16EK40YPD4BLP",2000001201,"台",1,"DN40 PN16","2014-03-31","力诺",null,{"v":4413.52,"d":"4,413.52"},{"v":3437.02,"d":"3,437.02"},"脱墨浆停产","良好"]
[226,"吉林晨鸣","制浆分厂","气动O型开关球阀","ZSSR-16EK40YPD4BLP",2000001202,"台",1,"DN40 PN16","2014-03-31","力诺",null,{"v":3509.34,"d":"3,509.34"},{"v":2732.9,"d":"2,732.90"},"脱墨浆停产","良好"]
[227,"吉林晨鸣","制浆分厂","气动V型调节球阀","REKA400AJJST-B1CU20-ND91",2000001206,"台",1,"DN400 PN16","2014-03-31","美卓",null,{"v":26943.35,"d":"26,943.35"},{"v":20982.13,"d":"20,982.13"},"脱墨浆停产","良好"]
[228,"吉林晨鸣","制浆分厂","气动V型调节球阀","REKA500AJJST-B1CU25-ND91",2000001207,"台",1,"DN500 PN16","2014-03-31","美卓",null,{"v":26943.35,"d":"26,943.35"},{"v":20982.13,"d":"20,982.13"},"脱墨浆停产","良好"]
[229,"吉林晨鸣","制浆分厂","气动V型调节球阀","REKA400AJJST-B1CU20-ND91",2000001208,"台",1,"DN400 PN16","2014-03-31","美卓",null,{"v":26943.35,"d":"26,943.35"},{"v":20982.13,"d":"20,982.13"},"脱墨浆停产","良好"]
[230,"吉林晨鸣","制浆分厂","气动V型调节球阀","REKA400AJJST-B1CU20-ND91",2000001209,"台",1,"DN400 PN16","2014-03-31","美卓",null,{"v":26943.35,"d":"26,943.35"},{"v":20982.13,"d":"20,982.13"},"脱墨浆停产","良好"]
[231,"吉林晨鸣","制浆分厂","气动V型调节球阀","REKA300AJJST-B1CU17-ND91",2000001210,"台",1,"DN300 PN16","2014-03-31","美卓",null,{"v":38303.66,"d":"38,303.66"},{"v":29828.98,"d":"29,828.98"},"脱墨浆停产","良好"]
[232,"吉林晨鸣","制浆分厂","气动V型调节球阀","RAA200AS-B1CU11-ND9103HN",2000001232,"台",1,"DN200 PN16","2014-03-31","美卓",null,{"v":65521.85,"d":"65,521.85"},{"v":51025.16,"d":"51,025.16"},"脱墨浆停产","良好"]
[233,"吉林晨鸣","制浆分厂","气动V型调节球阀","REKA300AJJST-B1CU17-ND91",2000001233,"台",1,"DN300 PN16","2014-03-31","美卓",null,{"v":39361.58,"d":"39,361.58"},{"v":30652.84,"d":"30,652.84"},"脱墨浆停产","良好"]
[234,"吉林晨鸣","制浆分厂","气动V型调节球阀","REKA300AJJST-B1CU17-ND91",2000001234,"台",1,"DN300 PN16","2014-03-31","美卓",null,{"v":39361.58,"d":"39,361.58"},{"v":30652.84,"d":"30,652.84"},"脱墨浆停产","良好"]
[235,"吉林晨鸣","制浆分厂","气动开关蝶阀","L12A500AA/K-B1CU25-SR33B",2000001235,"台",1,null,"2014-03-31","美卓",null,{"v":39361.58,"d":"39,361.58"},{"v":30652.84,"d":"30,652.84"},"脱墨浆停产","良好"]
[236,"吉林晨鸣","制浆分厂","气动O型开关球阀","1'4AB3600XTB2-VPVL100DAB",2000001236,"台",1,"1'4AB3600XTB2-VPVL100DAB","2014-03-31","美卓",null,{"v":39361.58,"d":"39,361.58"},{"v":30652.84,"d":"30,652.84"},"脱墨浆停产","良好"]
[237,"吉林晨鸣","制浆分厂","气动O型开关球阀","3/4'4AB3600XTB2-VPVL100D",2000001237,"台",1,"3/4'4AB3600XTB2-VPVL100D","2014-03-31","美卓",null,{"v":48051.16,"d":"48,051.16"},{"v":37419.85,"d":"37,419.85"},"脱墨浆停产","良好"]
[238,"吉林晨鸣","制浆分厂","气动O型开关球阀","3/4'4AB3600XTB2-VPVL100D",2000001238,"台",1,"3/4'4AB3600XTB2-VPVL100D","2014-03-31","美卓",null,{"v":48051.16,"d":"48,051.16"},{"v":37419.85,"d":"37,419.85"},"脱墨浆停产","良好"]
[239,"吉林晨鸣","制浆分厂","气动O型开关球阀","M1KA250AP-B1CU25-SV3-SR3",2000001239,"台",1,"M1KA250AP-B1CU25-SV3-SR3","2014-03-31","美卓",null,{"v":48051.16,"d":"48,051.16"},{"v":37419.85,"d":"37,419.85"},"脱墨浆停产","良好"]
[240,"吉林晨鸣","制浆分厂","气动O型开关球阀","M1KA250AP-B1CU25-SV3-SR3",2000001240,"台",1,"M1KA250AP-B1CU25-SV3-SR3","2014-03-31","美卓",null,{"v":48051.16,"d":"48,051.16"},{"v":37419.85,"d":"37,419.85"},"脱墨浆停产","良好"]
[241,"吉林晨鸣","制浆分厂","气动V型开关球阀","1'1/44AB3600XTB2-VPVL200",2000001241,"台",1,"1'1/44AB3600XTB2-VPVL200","2014-03-31","美卓",null,{"v":48051.16,"d":"48,051.16"},{"v":37419.85,"d":"37,419.85"},"脱墨浆停产","良好"]
[242,"吉林晨鸣","制浆分厂","气动O型开关球阀","1'4AB3600XTB2-VPVL100DAB",2000001242,"台",1,"1'4AB3600XTB2-VPVL100DAB","2014-03-31","美卓",null,{"v":48051.16,"d":"48,051.16"},{"v":37419.85,"d":"37,419.85"},"脱墨浆停产","良好"]
[243,"吉林晨鸣","制浆分厂","气动O型开关球阀","1'4AB3600XTB2-VPVL100DAB",2000001243,"台",1,"1'4AB3600XTB2-VPVL100DAB","2014-03-31","美卓",null,{"v":48051.16,"d":"48,051.16"},{"v":37419.85,"d":"37,419.85"},"脱墨浆停产","良好"]
[244,"吉林晨鸣","制浆分厂","气动开关蝶阀","L12A500AA/K-B1CU25-SR33B",2000001244,"台",1,"L12A500AA/K-B1CU25-SR33B","2014-03-31","美卓",null,{"v":48051.16,"d":"48,051.16"},{"v":37419.85,"d":"37,419.85"},"脱墨浆停产","良好"]
[245,"吉林晨鸣","制浆分厂","气动开关蝶阀","L12A350AA-B1CU17-SR33B5H",2000001245,"台",1,"L12A350AA-B1CU17-SR33B5H","2014-03-31","美卓",null,{"v":48051.16,"d":"48,051.16"},{"v":37419.85,"d":"37,419.85"},"脱墨浆停产","良好"]
[246,"吉林晨鸣","制浆分厂","气动V型开关球阀","3/4'4AB3600XTB2-VPVL100D",2000001246,"台",1,"3/4'4AB3600XTB2-VPVL100D","2014-03-31","美卓",null,{"v":48051.16,"d":"48,051.16"},{"v":37419.85,"d":"37,419.85"},"脱墨浆停产","良好"]
[247,"吉林晨鸣","制浆分厂","气动V型开关球阀","1'4AB3600XTB2-VPVL100DAB",2000001247,"台",1,"1'4AB3600XTB2-VPVL100DAB","2014-03-31","美卓",null,{"v":48051.16,"d":"48,051.16"},{"v":37419.85,"d":"37,419.85"},"脱墨浆停产","良好"]
[248,"吉林晨鸣","制浆分厂","气动V型开关球阀","1-1/2''4AB3600XTB2",2000001248,"台",1,"1-1/2''4AB3600XTB2","2014-03-31","美卓",null,{"v":48051.16,"d":"48,051.16"},{"v":37419.85,"d":"37,419.85"},"脱墨浆停产","良好"]
[249,"吉林晨鸣","制浆分厂","气动V型开关球阀","1-1/2''4AB3600XTB2",2000001249,"台",1,"1-1/2''4AB3600XTB2","2014-03-31","美卓",null,{"v":48051.16,"d":"48,051.16"},{"v":37419.85,"d":"37,419.85"},"脱墨浆停产","良好"]
[250,"吉林晨鸣","制浆分厂","气动V型开关球阀","RAA080AS-B1CU6-SR33B5HDN",2000001250,"台",1,"DN80 PN16","2014-03-31","美卓",null,{"v":48051.16,"d":"48,051.16"},{"v":37419.85,"d":"37,419.85"},"脱墨浆停产","良好"]
[251,"吉林晨鸣","制浆分厂","气动V型开关球阀","RAA080AS-B1CU6-SR33B5HDN",2000001251,"台",1,"DN80 PN16","2014-03-31","美卓",null,{"v":48051.16,"d":"48,051.16"},{"v":37419.85,"d":"37,419.85"},"脱墨浆停产","良好"]
[252,"吉林晨鸣","制浆分厂","气动V型开关球阀","1-1/2''4AB3600XTB2",2000001252,"台",1,"1-1/2''4AB3600XTB2","2014-03-31","美卓",null,{"v":48051.16,"d":"48,051.16"},{"v":37419.85,"d":"37,419.85"},"脱墨浆停产","良好"]
[253,"吉林晨鸣","制浆分厂","气动V型开关球阀","RAA080AS-B1CU6-SR33B5HDN",2000001253,"台",1,"RAA080AS-B1CU6-SR33B5HDN","2014-03-31","美卓",null,{"v":48051.16,"d":"48,051.16"},{"v":37419.85,"d":"37,419.85"},"脱墨浆停产","良好"]
[254,"吉林晨鸣","制浆分厂","气动V型开关球阀","1-1/2''4AB3600XTB2",2000001254,"台",1,"1-1/2''4AB3600XTB2","2014-03-31","美卓",null,{"v":48051.16,"d":"48,051.16"},{"v":37419.85,"d":"37,419.85"},"脱墨浆停产","良好"]
[255,"吉林晨鸣","制浆分厂","气动V型开关球阀","1-1/2''4AB3600XTB2",2000001255,"台",1,"1-1/2''4AB3600XTB2","2014-03-31","美卓",null,{"v":48051.16,"d":"48,051.16"},{"v":37419.85,"d":"37,419.85"},"脱墨浆停产","良好"]
[256,"吉林晨鸣","制浆分厂","真空压力变送器","STA92L-E1G-00000-H6,SM,S",2000001303,"台",1,"负100KPA-100KPA","2014-03-31","霍尼韦尔",null,{"v":3392.93,"d":"3,392.93"},{"v":2642.25,"d":"2,642.25"},"脱墨浆停产","报废"]
[257,"吉林晨鸣","制浆分厂","真空压力变送器","STA92L-E1G-00000-H6,SM,S",2000001304,"台",1,"负100KPA-100KPA","2014-03-31","霍尼韦尔",null,{"v":3392.93,"d":"3,392.93"},{"v":2642.25,"d":"2,642.25"},"脱墨浆停产","报废"]
[258,"吉林晨鸣","制浆分厂","压力变送器","STG94L-E1G-00000-H6,SM,S",2000001347,"台",1,"0-100KPA","2014-03-31","霍尼韦尔",null,{"v":2770.33,"d":"2,770.33"},{"v":2157.39,"d":"2,157.39"},"脱墨浆停产","良好"]
[259,"吉林晨鸣","制浆分厂","静压投入式液位计","ST600",2000001348,"台",1,null,"2014-03-31",null,null,{"v":1382.39,"d":"1,382.39"},{"v":1076.52,"d":"1,076.52"},"脱墨浆停产","已报废"]
[260,"吉林晨鸣","制浆分厂","静压投入式液位计","ST600",2000001349,"台",1,null,"2014-03-31",null,null,{"v":1382.39,"d":"1,382.39"},{"v":1076.52,"d":"1,076.52"},"脱墨浆停产","已报废"]
[261,"吉林晨鸣","制浆分厂","远传压力变送器","STR94G-11A-1Y0EFMEA8020-",2000001356,"台",1,"0-100KPA","2014-03-31","霍尼韦尔",null,{"v":3794.4,"d":"3,794.40"},{"v":2954.88,"d":"2,954.88"},"脱墨浆停产","良好"]
[262,"吉林晨鸣","制浆分厂","法兰式差压变送器","STF932-S1A-0K5C0-H6,SM,1",2000001357,"台",1,"0-100KPA","2014-03-31","霍尼韦尔",null,{"v":3846.74,"d":"3,846.74"},{"v":2995.66,"d":"2,995.66"},"脱墨浆停产","良好"]
[263,"吉林晨鸣","制浆分厂","隔膜密封式压力变送器","STR94G-11A-1Y0EFMEA8020-",2000001358,"台",1,"0-100KPA","2014-03-31","霍尼韦尔",null,{"v":3365.6,"d":"3,365.60"},{"v":2620.97,"d":"2,620.97"},"脱墨浆停产","良好"]
[264,"吉林晨鸣","制浆分厂","真空压力变送器","STA92L-E1G-00000-H6,SM,S",2000001359,"台",1,"0-100KPA","2014-03-31","霍尼韦尔",null,{"v":3392.93,"d":"3,392.93"},{"v":2642.25,"d":"2,642.25"},"脱墨浆停产","良好"]
[265,"吉林晨鸣","制浆分厂","真空压力变送器","STA92L-E1G-00000-H6,SM,S",2000001388,"台",1,"0-100KPA","2014-03-31","霍尼韦尔",null,{"v":3392.93,"d":"3,392.93"},{"v":2642.25,"d":"2,642.25"},"脱墨浆停产","报废"]
[266,"吉林晨鸣","制浆分厂"," 压力变送器","STR94G-11D-120AFMAA21A0-",2000001389,"台",1,"0-100KPA","2014-03-31","霍尼韦尔",null,{"v":2770.33,"d":"2,770.33"},{"v":2157.39,"d":"2,157.39"},"脱墨浆停产","良好"]
[267,"吉林晨鸣","制浆分厂"," 压力变送器","STR94G-11D-120AFMAA21A0-",2000001390,"台",1,"0-100KPA","2014-03-31","霍尼韦尔",null,{"v":2770.33,"d":"2,770.33"},{"v":2157.39,"d":"2,157.39"},"脱墨浆停产","良好"]
[268,"吉林晨鸣","制浆分厂"," 压力变送器","STR94G-11D-120AFMAA21A0-",2000001391,"台",1,"0-100KPA","2014-03-31","霍尼韦尔",null,{"v":2770.33,"d":"2,770.33"},{"v":2157.39,"d":"2,157.39"},"脱墨浆停产","良好"]
[269,"吉林晨鸣","制浆分厂","单远传隔膜压力变送器","STF924-R1A-0K5C0-H6,SM,1",2000001392,"台",1,"0-100KPA","2014-03-31","霍尼韦尔",null,{"v":2770.33,"d":"2,770.33"},{"v":2157.39,"d":"2,157.39"},"脱墨浆停产","良好"]
[270,"吉林晨鸣","制浆分厂","1#气浮撇泥电机","1.5KW—4级",2000001589,"台",1,null,"2014-03-31",null,null,{"v":33956.79,"d":"33,956.79"},{"v":26443.84,"d":"26,443.84"},"脱墨浆停产","良好"]
[271,"吉林晨鸣","制浆分厂","1#气浮驱动电机","3KW—4级",2000001590,"台",1,null,"2014-03-31",null,null,{"v":34318.39,"d":"34,318.39"},{"v":26725.43,"d":"26,725.43"},"脱墨浆停产","良好"]
[272,"吉林晨鸣","制浆分厂","后多盘分浆主电机","11KW—4级",2000001591,"台",1,null,"2014-03-31",null,null,{"v":34576.68,"d":"34,576.68"},{"v":26926.59,"d":"26,926.59"},"脱墨浆停产","良好"]
[273,"吉林晨鸣","制浆分厂","泡沫泵电机","11KW—6级",2000001592,"台",1,null,"2014-03-31",null,null,{"v":34680,"d":"34,680.00"},{"v":27007.05,"d":"27,007.05"},"脱墨浆停产","良好"]
[274,"吉林晨鸣","制浆分厂","泡沫泵电机","11KW—6级",2000001593,"台",1,null,"2014-03-31",null,null,{"v":34680,"d":"34,680.00"},{"v":27007.05,"d":"27,007.05"},"脱墨浆停产","良好"]
[275,"吉林晨鸣","制浆分厂","污泥混合槽入口絮凝剂流量显示调节","气动V型调节阀 ZSSV—16T",2000001596,"台",1,null,"2014-03-31",null,null,{"v":35597.03,"d":"35,597.03"},{"v":27721.17,"d":"27,721.17"},"脱墨浆停产","良好"]
[276,"吉林晨鸣","制浆分厂","后多盘喷水白臂电机","8.75KW—6级",2000001597,"台",1,null,"2014-03-31",null,null,{"v":35609.85,"d":"35,609.85"},{"v":27731.19,"d":"27,731.19"},"脱墨浆停产","良好"]
[277,"吉林晨鸣","制浆分厂","中浓除渣器上部排放口阀门遥控","气动刀闸阀 336D—C DN100",2000001598,"台",1,null,"2014-03-31",null,null,{"v":35728.87,"d":"35,728.87"},{"v":27823.85,"d":"27,823.85"},"脱墨浆停产","良好"]
[278,"吉林晨鸣","制浆分厂","前多盘清白水池高压水阀门遥控","气动通断球阀 ZSSR—16E D",2000001599,"台",1,null,"2014-03-31",null,null,{"v":35728.87,"d":"35,728.87"},{"v":27823.85,"d":"27,823.85"},"脱墨浆停产","良好"]
[279,"吉林晨鸣","制浆分厂","前多盘清白水池高压水阀门遥控","气动通断球阀 ZSSR—16E D",2000001600,"台",1,null,"2014-03-31",null,null,{"v":35728.87,"d":"35,728.87"},{"v":27823.85,"d":"27,823.85"},"脱墨浆停产","良好"]
[280,"吉林晨鸣","制浆分厂","前多盘稀释水流量显示调节","气动V型调节阀 ZSSV—16T",2000001601,"台",1,null,"2014-03-31",null,null,{"v":35728.87,"d":"35,728.87"},{"v":27823.85,"d":"27,823.85"},"脱墨浆停产","良好"]
[281,"吉林晨鸣","制浆分厂","前多盘清白水池高压水阀门遥控","气动通断球阀 ZSSR—16E D",2000001602,"台",1,null,"2014-03-31",null,null,{"v":35728.87,"d":"35,728.87"},{"v":27823.85,"d":"27,823.85"},"脱墨浆停产","良好"]
[282,"吉林晨鸣","制浆分厂","三段压力精筛排渣口阀门遥控","气动刀闸阀 336D—C DN100",2000001603,"台",1,null,"2014-03-31",null,null,{"v":35729.11,"d":"35,729.11"},{"v":27824.04,"d":"27,824.04"},"脱墨浆停产","良好"]
[283,"吉林晨鸣","制浆分厂","螺旋输送电机","22KW—4级",2000001605,"台",1,null,"2014-03-31",null,null,{"v":36126.43,"d":"36,126.43"},{"v":28133.45,"d":"28,133.45"},"脱墨浆停产","良好"]
[284,"吉林晨鸣","制浆分厂","三精筛电机","22KW—6级",2000001606,"台",1,null,"2014-03-31",null,null,{"v":36643.02,"d":"36,643.02"},{"v":28535.74,"d":"28,535.74"},"脱墨浆停产","良好"]
[285,"吉林晨鸣","制浆分厂","漂白塔浊白水出口阀门遥控","气动插板阀 ZSLDC—16E DN",2000001607,"台",1,null,"2014-03-31",null,null,{"v":37660,"d":"37,660.00"},{"v":29327.72,"d":"29,327.72"},"脱墨浆停产","良好"]
[286,"吉林晨鸣","制浆分厂","1#后浮选槽液位指使调节","气动V型调节阀 ZSSV—16T",2000001608,"台",1,null,"2014-03-31",null,null,{"v":37660,"d":"37,660.00"},{"v":29327.72,"d":"29,327.72"},"脱墨浆停产","良好"]
[287,"吉林晨鸣","制浆分厂","二段精筛电机","37KW—6级",2000001609,"台",1,null,"2014-03-31",null,null,{"v":37676.18,"d":"37,676.18"},{"v":29340.32,"d":"29,340.32"},"脱墨浆停产","良好"]
[288,"吉林晨鸣","制浆分厂","二段精筛电机","22KW—4级",2000001610,"台",1,null,"2014-03-31",null,null,{"v":37676.18,"d":"37,676.18"},{"v":29340.32,"d":"29,340.32"},"脱墨浆停产","良好"]
[289,"吉林晨鸣","制浆分厂","后多盘直搅龙减速机","15KW—4级",2000001611,"台",1,null,"2014-03-31",null,null,{"v":37676.18,"d":"37,676.18"},{"v":29340.32,"d":"29,340.32"},"脱墨浆停产","良好"]
[290,"吉林晨鸣","制浆分厂","2#气浮泵电机","37KW—2级",2000001612,"台",1,null,"2014-03-31",null,null,{"v":37676.18,"d":"37,676.18"},{"v":29340.32,"d":"29,340.32"},"脱墨浆停产","良好"]
[291,"吉林晨鸣","制浆分厂","P—4泵出口压力调节","气动O型调节阀 ZSSV—16T",2000001613,"台",1,null,"2014-03-31",null,null,{"v":37981.01,"d":"37,981.01"},{"v":29577.7,"d":"29,577.70"},"脱墨浆停产","良好"]
[292,"吉林晨鸣","制浆分厂","1、2段粗筛冲洗水阀门遥控","气动通断球阀 ZSSR—16E D",2000001614,"台",1,null,"2014-03-31",null,null,{"v":37981.01,"d":"37,981.01"},{"v":29577.7,"d":"29,577.70"},"脱墨浆停产","良好"]
[293,"吉林晨鸣","制浆分厂","快速加热器温度指示调节","气动V型调节阀 ZSSV—16T",2000001615,"台",1,null,"2014-03-31",null,null,{"v":37981.01,"d":"37,981.01"},{"v":29577.7,"d":"29,577.70"},"脱墨浆停产","良好"]
[294,"吉林晨鸣","制浆分厂","二精筛电机","45KW—8级",2000001616,"台",1,null,"2014-03-31",null,null,{"v":38192.77,"d":"38,192.77"},{"v":29742.62,"d":"29,742.62"},"脱墨浆停产","良好"]
[295,"吉林晨鸣","制浆分厂","一段精筛电机","90KW—8级",2000001617,"台",1,null,"2014-03-31",null,null,{"v":38192.77,"d":"38,192.77"},{"v":29742.62,"d":"29,742.62"},"脱墨浆停产","良好"]
[296,"吉林晨鸣","制浆分厂","热分散油泵电机","1.5KW—4级",2000001618,"台",1,null,"2014-03-31",null,null,{"v":38192.77,"d":"38,192.77"},{"v":29742.62,"d":"29,742.62"},"脱墨浆停产","良好"]
[297,"吉林晨鸣","制浆分厂","高浓除渣器出口压力调节","气动V型调节阀 ZSSV—16T",2000001619,"台",1,null,"2014-03-31",null,null,{"v":38343.41,"d":"38,343.41"},{"v":29859.94,"d":"29,859.94"},"脱墨浆停产","良好"]
[298,"吉林晨鸣","制浆分厂","碎浆机密封水阀门遥控","PILOT式双口活塞驱动阀AP1",2000001620,"台",1,null,"2014-03-31",null,null,{"v":38709.35,"d":"38,709.35"},{"v":30144.91,"d":"30,144.91"},"脱墨浆停产","良好"]
[299,"吉林晨鸣","制浆分厂","计量槽排放口阀门遥控","气动通断球阀 ZSSR—16E D",2000001621,"台",1,null,"2014-03-31",null,null,{"v":38709.35,"d":"38,709.35"},{"v":30144.91,"d":"30,144.91"},"脱墨浆停产","良好"]
[300,"吉林晨鸣","制浆分厂","计量槽排放口阀门遥控","气动通断球阀 ZSSR—16E D",2000001622,"台",1,null,"2014-03-31",null,null,{"v":38709.35,"d":"38,709.35"},{"v":30144.91,"d":"30,144.91"},"脱墨浆停产","良好"]
[301,"吉林晨鸣","制浆分厂","计量槽排放口阀门遥控","气动通断球阀 ZSSR—16E D",2000001623,"台",1,null,"2014-03-31",null,null,{"v":38709.35,"d":"38,709.35"},{"v":30144.91,"d":"30,144.91"},"脱墨浆停产","良好"]
[302,"吉林晨鸣","制浆分厂","计量槽排放口阀门遥控","气动通断球阀 ZSSR—16E D",2000001624,"台",1,null,"2014-03-31",null,null,{"v":38709.35,"d":"38,709.35"},{"v":30144.91,"d":"30,144.91"},"脱墨浆停产","良好"]
[303,"吉林晨鸣","制浆分厂","计量槽排放口阀门遥控","气动通断球阀 ZSSR—16E D",2000001625,"台",1,null,"2014-03-31",null,null,{"v":38709.35,"d":"38,709.35"},{"v":30144.91,"d":"30,144.91"},"脱墨浆停产","良好"]
[304,"吉林晨鸣","制浆分厂","三段压力粗筛稀释水阀门遥控","扭矩气缸式球阀 AW13—E01",2000001626,"台",1,null,"2014-03-31",null,null,{"v":38709.35,"d":"38,709.35"},{"v":30144.91,"d":"30,144.91"},"脱墨浆停产","良好"]
[305,"吉林晨鸣","制浆分厂","三段压力精筛入口阀门遥控","刀闸阀 336D—C DN125",2000001627,"台",1,null,"2014-03-31",null,null,{"v":38709.35,"d":"38,709.35"},{"v":30144.91,"d":"30,144.91"},"脱墨浆停产","良好"]
[306,"吉林晨鸣","制浆分厂","三段压力精筛稀释水阀门遥控","刀闸阀 336D—C DN125",2000001628,"台",1,null,"2014-03-31",null,null,{"v":38709.35,"d":"38,709.35"},{"v":30144.91,"d":"30,144.91"},"脱墨浆停产","良好"]
[307,"吉林晨鸣","制浆分厂","1#预浮选槽入口压力调节","气动V型调节阀 ZSSV—16T",2000001629,"台",1,null,"2014-03-31",null,null,{"v":38709.35,"d":"38,709.35"},{"v":30144.91,"d":"30,144.91"},"脱墨浆停产","良好"]
[308,"吉林晨鸣","制浆分厂","1#预浮选槽放空阀门遥控","气动通断球阀 ZSSR—16E D",2000001630,"台",1,null,"2014-03-31",null,null,{"v":38709.35,"d":"38,709.35"},{"v":30144.91,"d":"30,144.91"},"脱墨浆停产","良好"]
[309,"吉林晨鸣","制浆分厂","2#预浮选槽放空阀门遥控","气动通断球阀 ZSSR—16E D",2000001631,"台",1,null,"2014-03-31",null,null,{"v":38709.35,"d":"38,709.35"},{"v":30144.91,"d":"30,144.91"},"脱墨浆停产","良好"]
[310,"吉林晨鸣","制浆分厂","1#预浮泡沫分离器进水阀门遥控","气动通断球阀 ZSSR—16E D",2000001632,"台",1,null,"2014-03-31",null,null,{"v":38709.35,"d":"38,709.35"},{"v":30144.91,"d":"30,144.91"},"脱墨浆停产","良好"]
[311,"吉林晨鸣","制浆分厂","2#预浮泡沫分离器进水阀门遥控","气动通断球阀 ZSSR—16E D",2000001633,"台",1,null,"2014-03-31",null,null,{"v":38709.35,"d":"38,709.35"},{"v":30144.91,"d":"30,144.91"},"脱墨浆停产","良好"]
[312,"吉林晨鸣","制浆分厂","1#后浮选槽放空阀门遥控","气动通断球阀 ZSSR—16E D",2000001634,"台",1,null,"2014-03-31",null,null,{"v":38709.35,"d":"38,709.35"},{"v":30144.91,"d":"30,144.91"},"脱墨浆停产","良好"]
[313,"吉林晨鸣","制浆分厂","2#后浮选槽放空阀门遥控","气动通断球阀 ZSSR—16E D",2000001635,"台",1,null,"2014-03-31",null,null,{"v":38709.35,"d":"38,709.35"},{"v":30144.91,"d":"30,144.91"},"脱墨浆停产","良好"]
[314,"吉林晨鸣","制浆分厂","1#后浮泡沫分离器进水阀门遥控","气动通断球阀 ZSSR—16E D",2000001636,"台",1,null,"2014-03-31",null,null,{"v":38709.35,"d":"38,709.35"},{"v":30144.91,"d":"30,144.91"},"脱墨浆停产","良好"]
[315,"吉林晨鸣","制浆分厂","2#后浮泡沫分离器进水阀门遥控","气动通断球阀 ZSSR—16E D",2000001637,"台",1,null,"2014-03-31",null,null,{"v":38709.35,"d":"38,709.35"},{"v":30144.91,"d":"30,144.91"},"脱墨浆停产","良好"]
[316,"吉林晨鸣","制浆分厂","重力脱水机进水口阀门遥控","气动通断球阀 ZSSR—16E D",2000001638,"台",1,null,"2014-03-31",null,null,{"v":38709.35,"d":"38,709.35"},{"v":30144.91,"d":"30,144.91"},"脱墨浆停产","良好"]
[317,"吉林晨鸣","制浆分厂","高浓除渣器上部排放口阀门遥控","气动刀闸阀 336D—C DN100",2000001639,"台",1,null,"2014-03-31",null,null,{"v":39122.13,"d":"39,122.13"},{"v":30466.34,"d":"30,466.34"},"脱墨浆停产","良好"]
[318,"吉林晨鸣","制浆分厂","P—80泵出口压力调节","气动V型调节阀 ZSSV—16T",2000001640,"台",1,null,"2014-03-31",null,null,{"v":39122.13,"d":"39,122.13"},{"v":30466.34,"d":"30,466.34"},"脱墨浆停产","良好"]
[319,"吉林晨鸣","制浆分厂","1#气浮清水池液位调节","气动通断球阀 ZSSR—16E D",2000001642,"台",1,null,"2014-03-31",null,null,{"v":39122.13,"d":"39,122.13"},{"v":30466.34,"d":"30,466.34"},"脱墨浆停产","良好"]
[320,"吉林晨鸣","制浆分厂","P—18泵出口压力调节","气动通断球阀 ZSSR—16E D",2000001643,"台",1,null,"2014-03-31",null,null,{"v":39122.13,"d":"39,122.13"},{"v":30466.34,"d":"30,466.34"},"脱墨浆停产","良好"]
[321,"吉林晨鸣","制浆分厂","清水泵出口压力调节","气动O型调节阀 ZSSR—16T",2000001644,"台",1,null,"2014-03-31",null,null,{"v":39122.13,"d":"39,122.13"},{"v":30466.34,"d":"30,466.34"},"脱墨浆停产","良好"]
[322,"吉林晨鸣","制浆分厂","中浓浆泵出口阀门调节控制","气动V型调节球阀 ZSSV—16",2000001645,"台",1,null,"2014-03-31",null,null,{"v":39122.13,"d":"39,122.13"},{"v":30466.34,"d":"30,466.34"},"脱墨浆停产","良好"]
[323,"吉林晨鸣","制浆分厂","原有中浓浆泵出口阀门调节控制","气动V型调节球阀 ZSSV—16",2000001646,"台",1,null,"2014-03-31",null,null,{"v":39122.13,"d":"39,122.13"},{"v":30466.34,"d":"30,466.34"},"脱墨浆停产","良好"]
[324,"吉林晨鸣","制浆分厂","二段精筛电机","55KW—8级",2000001647,"台",1,null,"2014-03-31",null,null,{"v":39225.93,"d":"39,225.93"},{"v":30547.17,"d":"30,547.17"},"脱墨浆停产","良好"]
[325,"吉林晨鸣","制浆分厂","1#气浮泵电机","55KW—2级",2000001648,"台",1,null,"2014-03-31",null,null,{"v":39225.93,"d":"39,225.93"},{"v":30547.17,"d":"30,547.17"},"脱墨浆停产","良好"]
[326,"吉林晨鸣","制浆分厂","二段粗筛供料池液位显示调节","气动O型调节阀 ZSSR—16T",2000001649,"台",1,null,"2014-03-31",null,null,{"v":39742.51,"d":"39,742.51"},{"v":30949.49,"d":"30,949.49"},"脱墨浆停产","良好"]
[327,"吉林晨鸣","制浆分厂","二段压力粗筛出口阀门遥控","气动V型调节阀 ZSSV—16T",2000001650,"台",1,null,"2014-03-31",null,null,{"v":39742.51,"d":"39,742.51"},{"v":30949.49,"d":"30,949.49"},"脱墨浆停产","良好"]
[328,"吉林晨鸣","制浆分厂","二段精筛供料池液位指示调节报警","气动O型调节阀 ZSSR—16T",2000001651,"台",1,null,"2014-03-31",null,null,{"v":39742.51,"d":"39,742.51"},{"v":30949.49,"d":"30,949.49"},"脱墨浆停产","良好"]
[329,"吉林晨鸣","制浆分厂","二段压力精筛出口阀门遥控","气动V型调节阀 ZSSV—16T",2000001652,"台",1,null,"2014-03-31",null,null,{"v":39742.51,"d":"39,742.51"},{"v":30949.49,"d":"30,949.49"},"脱墨浆停产","良好"]
[330,"吉林晨鸣","制浆分厂","后多盘清白水池高压水阀门遥控","气动通断球阀 ZSSR—16E D",2000001653,"台",1,null,"2014-03-31",null,null,{"v":39742.51,"d":"39,742.51"},{"v":30949.49,"d":"30,949.49"},"脱墨浆停产","良好"]
[331,"吉林晨鸣","制浆分厂","后多盘清白水池高压水阀门遥控","气动通断球阀 ZSSR—16E D",2000001654,"台",1,null,"2014-03-31",null,null,{"v":39742.51,"d":"39,742.51"},{"v":30949.49,"d":"30,949.49"},"脱墨浆停产","良好"]
[332,"吉林晨鸣","制浆分厂","四段精筛供料槽液位指示调节","气动V型调节球阀 ZSSV—16",2000001655,"台",1,null,"2014-03-31",null,null,{"v":39742.51,"d":"39,742.51"},{"v":30949.49,"d":"30,949.49"},"脱墨浆停产","良好"]
[333,"吉林晨鸣","制浆分厂","1#气浮刮渣机减速机","F15-Y1.5-BW18-59",2000001656,"台",1,null,"2014-03-31",null,null,{"v":40069.93,"d":"40,069.93"},{"v":31204.44,"d":"31,204.44"},"脱墨浆停产","良好"]
[334,"吉林晨鸣","制浆分厂","1#气浮螺旋减速机","RWO27",2000001657,"台",1,null,"2014-03-31",null,null,{"v":40069.93,"d":"40,069.93"},{"v":31204.44,"d":"31,204.44"},"脱墨浆停产","良好"]
[335,"吉林晨鸣","制浆分厂","2#气浮刮渣机减速机","F15-Y1.1-BW15-59",2000001658,"台",1,null,"2014-03-31",null,null,{"v":40069.93,"d":"40,069.93"},{"v":31204.44,"d":"31,204.44"},"脱墨浆停产","良好"]
[336,"吉林晨鸣","制浆分厂","高浓除渣器下部排放口阀门遥控","气动刀闸阀 336D—C DN200",2000001659,"台",1,null,"2014-03-31",null,null,{"v":40259.1,"d":"40,259.10"},{"v":31351.77,"d":"31,351.77"},"脱墨浆停产","良好"]
[337,"吉林晨鸣","制浆分厂","中浓除渣器下部排放口阀门遥控","气动刀闸阀 336D—C DN200",2000001660,"台",1,null,"2014-03-31",null,null,{"v":40259.1,"d":"40,259.10"},{"v":31351.77,"d":"31,351.77"},"脱墨浆停产","良好"]
[338,"吉林晨鸣","制浆分厂","1#预浮选槽液位指示调节","气动V型调节阀 ZSSV—16T",2000001661,"台",1,null,"2014-03-31",null,null,{"v":40259.1,"d":"40,259.10"},{"v":31351.77,"d":"31,351.77"},"脱墨浆停产","良好"]
[339,"吉林晨鸣","制浆分厂","1#预浮选槽进水阀门遥控","气动通断球阀 ZSSR—16E D",2000001662,"台",1,null,"2014-03-31",null,null,{"v":40259.1,"d":"40,259.10"},{"v":31351.77,"d":"31,351.77"},"脱墨浆停产","良好"]
[340,"吉林晨鸣","制浆分厂","1#后浮选槽进水阀门遥控","气动通断球阀 ZSSR—16E D",2000001663,"台",1,null,"2014-03-31",null,null,{"v":40259.1,"d":"40,259.10"},{"v":31351.77,"d":"31,351.77"},"脱墨浆停产","良好"]
[341,"吉林晨鸣","制浆分厂","粗选机渣浆排放A阀门遥控","气缸式刀闸阀 336D—C DN4",2000001664,"台",1,null,"2014-03-31",null,null,{"v":40459.2,"d":"40,459.20"},{"v":31507.62,"d":"31,507.62"},"脱墨浆停产","良好"]
[342,"吉林晨鸣","制浆分厂","粗选机输出阀门遥控","气缸式刀闸阀 336D—C DN6",2000001665,"台",1,null,"2014-03-31",null,null,{"v":40459.2,"d":"40,459.20"},{"v":31507.62,"d":"31,507.62"},"脱墨浆停产","良好"]
[343,"吉林晨鸣","制浆分厂","粗选机渣浆排放B阀门遥控","气缸式刀闸阀 336D—C DN1",2000001666,"台",1,null,"2014-03-31",null,null,{"v":40459.2,"d":"40,459.20"},{"v":31507.62,"d":"31,507.62"},"脱墨浆停产","良好"]
[344,"吉林晨鸣","制浆分厂","2#气浮螺旋减速机","F2.2-Y2.2-BW2.2-71",2000001667,"台",1,null,"2014-03-31",null,null,{"v":40586.51,"d":"40,586.51"},{"v":31606.76,"d":"31,606.76"},"脱墨浆停产","良好"]
[345,"吉林晨鸣","制浆分厂","二清白水池供料泵电机","110KW—2级",2000001668,"台",1,null,"2014-03-31",null,null,{"v":41292.26,"d":"41,292.26"},{"v":32156.36,"d":"32,156.36"},"脱墨浆停产","良好"]
[346,"吉林晨鸣","制浆分厂","成浆塔泵电机","132KW—2级",2000001669,"台",1,null,"2014-03-31",null,null,{"v":41292.26,"d":"41,292.26"},{"v":32156.36,"d":"32,156.36"},"脱墨浆停产","良好"]
[347,"吉林晨鸣","制浆分厂","1#气浮供料泵电机","75KW—6级",2000001670,"台",1,null,"2014-03-31",null,null,{"v":41292.26,"d":"41,292.26"},{"v":32156.36,"d":"32,156.36"},"脱墨浆停产","良好"]
[348,"吉林晨鸣","制浆分厂","三段压力粗筛排渣口阀门遥控","扭矩气缸式球阀 AG13—E01",2000001671,"台",1,null,"2014-03-31",null,null,{"v":41292.26,"d":"41,292.26"},{"v":32156.36,"d":"32,156.36"},"脱墨浆停产","良好"]
[349,"吉林晨鸣","制浆分厂","1、2段精筛冲洗水阀门遥控","气动通断球阀 ZSSR—16E D",2000001672,"台",1,null,"2014-03-31",null,null,{"v":41374.53,"d":"41,374.53"},{"v":32220.43,"d":"32,220.43"},"脱墨浆停产","良好"]
[350,"吉林晨鸣","制浆分厂","1#预浮选槽进气阀门遥控","气动通断球阀 ZSSR—16E D",2000001673,"台",1,null,"2014-03-31",null,null,{"v":41374.53,"d":"41,374.53"},{"v":32220.43,"d":"32,220.43"},"脱墨浆停产","良好"]
[351,"吉林晨鸣","制浆分厂","2#预浮选槽液位指示调节","气动V型调节阀 ZSSV—16T",2000001674,"台",1,null,"2014-03-31",null,null,{"v":41374.53,"d":"41,374.53"},{"v":32220.43,"d":"32,220.43"},"脱墨浆停产","良好"]
[352,"吉林晨鸣","制浆分厂","2#预浮选槽入口压力调节","气动V型调节阀 ZSSV—16T",2000001675,"台",1,null,"2014-03-31",null,null,{"v":41374.53,"d":"41,374.53"},{"v":32220.43,"d":"32,220.43"},"脱墨浆停产","良好"]
[353,"吉林晨鸣","制浆分厂","2#预浮选槽进气阀门遥控","气动通断球阀 ZSSR—16E D",2000001676,"台",1,null,"2014-03-31",null,null,{"v":41374.53,"d":"41,374.53"},{"v":32220.43,"d":"32,220.43"},"脱墨浆停产","良好"]
[354,"吉林晨鸣","制浆分厂","链板机1#减速机",null,2000001677,"台",1,null,"2014-03-31",null,null,{"v":41619.68,"d":"41,619.68"},{"v":32411.32,"d":"32,411.32"},"脱墨浆停产","良好"]
[355,"吉林晨鸣","制浆分厂","一段精筛电机","90KW—8级",2000001679,"台",1,null,"2014-03-31",null,null,{"v":42842.01,"d":"42,842.01"},{"v":33363.21,"d":"33,363.21"},"脱墨浆停产","良好"]
[356,"吉林晨鸣","制浆分厂","螺旋压榨挤浆电机","90KW—4级",2000001680,"台",1,null,"2014-03-31",null,null,{"v":42842.01,"d":"42,842.01"},{"v":33363.21,"d":"33,363.21"},"脱墨浆停产","良好"]
[357,"吉林晨鸣","制浆分厂","螺旋压榨挤浆电机","90KW—4级",2000001681,"台",1,null,"2014-03-31",null,null,{"v":42842.01,"d":"42,842.01"},{"v":33363.21,"d":"33,363.21"},"脱墨浆停产","良好"]
[358,"吉林晨鸣","制浆分厂","粗选机排气阀门遥控","扭矩气缸式球阀AG13—E010",2000001682,"台",1,null,"2014-03-31",null,null,{"v":43437.91,"d":"43,437.91"},{"v":33827.26,"d":"33,827.26"},"脱墨浆停产","良好"]
[359,"吉林晨鸣","制浆分厂","三段粗筛供料池液位显示调节","气动O型调节阀 ZSSV—16T",2000001683,"台",1,null,"2014-03-31",null,null,{"v":43875.18,"d":"43,875.18"},{"v":34167.81,"d":"34,167.81"},"脱墨浆停产","良好"]
[360,"吉林晨鸣","制浆分厂","三段压力粗筛入口阀门遥控","扭矩气缸式球阀 AW13—E01",2000001684,"台",1,null,"2014-03-31",null,null,{"v":43875.18,"d":"43,875.18"},{"v":34167.81,"d":"34,167.81"},"脱墨浆停产","良好"]
[361,"吉林晨鸣","制浆分厂","前多盘喷水管",null,2000001685,"台",1,null,"2014-03-31",null,null,{"v":44719.18,"d":"44,719.18"},{"v":34825.08,"d":"34,825.08"},"脱墨浆停产","良好"]
[362,"吉林晨鸣","制浆分厂","前多盘浓缩机减速机","M4PHT60",2000001686,"台",1,null,"2014-03-31",null,null,{"v":44719.18,"d":"44,719.18"},{"v":34825.08,"d":"34,825.08"},"脱墨浆停产","良好"]
[363,"吉林晨鸣","制浆分厂","前多盘喷水管减速机",null,2000001687,"台",1,null,"2014-03-31",null,null,{"v":44719.18,"d":"44,719.18"},{"v":34825.08,"d":"34,825.08"},"脱墨浆停产","良好"]
[364,"吉林晨鸣","制浆分厂","后多盘浓缩机减速机","M4PHT60",2000001688,"台",1,null,"2014-03-31",null,null,{"v":44719.18,"d":"44,719.18"},{"v":34825.08,"d":"34,825.08"},"脱墨浆停产","良好"]
[365,"吉林晨鸣","制浆分厂","后多盘喷水管减速机",null,2000001689,"台",1,null,"2014-03-31",null,null,{"v":44719.18,"d":"44,719.18"},{"v":34825.08,"d":"34,825.08"},"脱墨浆停产","良好"]
[366,"吉林晨鸣","制浆分厂","后多盘浊白水池液位指使调节","气动O型调节阀 ZSSR—16T",2000001690,"台",1,null,"2014-03-31",null,null,{"v":44719.18,"d":"44,719.18"},{"v":34825.08,"d":"34,825.08"},"脱墨浆停产","良好"]
[367,"吉林晨鸣","制浆分厂","前多盘破碎螺旋","AM160",2000001691,"台",1,null,"2014-03-31",null,null,{"v":45752.34,"d":"45,752.34"},{"v":35629.63,"d":"35,629.63"},"脱墨浆停产","良好"]
[368,"吉林晨鸣","制浆分厂","计量槽排放口阀门遥控","气动通断球阀 ZSSV—16T D",2000001692,"台",1,null,"2014-03-31",null,null,{"v":45906.61,"d":"45,906.61"},{"v":35749.76,"d":"35,749.76"},"脱墨浆停产","良好"]
[369,"吉林晨鸣","制浆分厂","一精筛电机","110KW—8级",2000001693,"台",1,null,"2014-03-31",null,null,{"v":45941.51,"d":"45,941.51"},{"v":35776.94,"d":"35,776.94"},"脱墨浆停产","良好"]
[370,"吉林晨鸣","制浆分厂","前多盘破碎螺旋减速机","AM160",2000001694,"台",1,null,"2014-03-31",null,null,{"v":47302.09,"d":"47,302.09"},{"v":36836.51,"d":"36,836.51"},"脱墨浆停产","良好"]
[371,"吉林晨鸣","制浆分厂","后多盘破碎螺旋减速机","AM160",2000001695,"台",1,null,"2014-03-31",null,null,{"v":47302.09,"d":"47,302.09"},{"v":36836.51,"d":"36,836.51"},"脱墨浆停产","良好"]
[372,"吉林晨鸣","制浆分厂","聚合铝溶解槽搅拌","XL06-35-5.5",2000001696,"台",1,null,"2014-03-31",null,null,{"v":47818.67,"d":"47,818.67"},{"v":37238.79,"d":"37,238.79"},"脱墨浆停产","良好"]
[373,"吉林晨鸣","制浆分厂","螺旋输送加汽电机","132KW—6级",2000001697,"台",1,null,"2014-03-31",null,null,{"v":49041.01,"d":"49,041.01"},{"v":38190.68,"d":"38,190.68"},"脱墨浆停产","良好"]
[374,"吉林晨鸣","制浆分厂","污泥压榨机减速机","MRP1744V-630",2000001698,"台",1,null,"2014-03-31",null,null,{"v":49885.01,"d":"49,885.01"},{"v":38847.94,"d":"38,847.94"},"脱墨浆停产","良好"]
[375,"吉林晨鸣","制浆分厂","后多盘喷水管",null,2000001699,"台",1,null,"2014-03-31",null,null,{"v":49885.01,"d":"49,885.01"},{"v":38847.94,"d":"38,847.94"},"脱墨浆停产","良好"]
[376,"吉林晨鸣","制浆分厂","三段压力精筛入口浆管阀门调节控制","气动V型调节球阀 ZSSV—16",2000001700,"台",1,null,"2014-03-31",null,null,{"v":50608.22,"d":"50,608.22"},{"v":39411.15,"d":"39,411.15"},"脱墨浆停产","良好"]
[377,"吉林晨鸣","制浆分厂","清水池液位指示调节","气动蝶型调节阀 ZSSW—16T",2000001705,"台",1,null,"2014-03-31",null,null,{"v":51623.92,"d":"51,623.92"},{"v":40202.11,"d":"40,202.11"},"脱墨浆停产","良好"]
[378,"吉林晨鸣","制浆分厂","二段压力精筛出口良浆流量指示调节","气动V型调节球阀 ZSSV—16",2000001706,"台",1,null,"2014-03-31",null,null,{"v":51623.92,"d":"51,623.92"},{"v":40202.11,"d":"40,202.11"},"脱墨浆停产","良好"]
[379,"吉林晨鸣","制浆分厂","进入中浓浆泵立管的清水阀门开关控制","气动O型切断阀 ZSSR—16E",2000001707,"台",1,null,"2014-03-31",null,null,{"v":54206.84,"d":"54,206.84"},{"v":42213.57,"d":"42,213.57"},"脱墨浆停产","良好"]
[380,"吉林晨鸣","制浆分厂","后多盘破碎螺旋","AM160",2000001709,"台",1,null,"2014-03-31",null,null,{"v":55050.84,"d":"55,050.84"},{"v":42870.83,"d":"42,870.83"},"脱墨浆停产","良好"]
[381,"吉林晨鸣","制浆分厂","前多盘螺旋输送机",null,2000001710,"台",1,null,"2014-03-31",null,null,{"v":55050.84,"d":"55,050.84"},{"v":42870.83,"d":"42,870.83"},"脱墨浆停产","良好"]
[382,"吉林晨鸣","制浆分厂","1#气浮螺旋","RWO27",2000001711,"台",1,null,"2014-03-31",null,null,{"v":55050.84,"d":"55,050.84"},{"v":42870.83,"d":"42,870.83"},"脱墨浆停产","良好"]
[383,"吉林晨鸣","制浆分厂","热分散主电机","1500KW—4级",2000001712,"台",1,null,"2014-03-31",null,null,{"v":56789.75,"d":"56,789.75"},{"v":44225.01,"d":"44,225.01"},"脱墨浆停产","良好"]
[384,"吉林晨鸣","制浆分厂","2#气浮刮渣机","F15-Y1.1-BW15-59",2000001713,"台",1,null,"2014-03-31",null,null,{"v":60216.67,"d":"60,216.67"},{"v":46893.73,"d":"46,893.73"},"脱墨浆停产","良好"]
[385,"吉林晨鸣","制浆分厂","二段压力精筛入口浆管阀门调节控制","气动V型调节球阀 ZSSV—16",2000001714,"台",1,null,"2014-03-31",null,null,{"v":60216.67,"d":"60,216.67"},{"v":46893.73,"d":"46,893.73"},"脱墨浆停产","良好"]
[386,"吉林晨鸣","制浆分厂","螺旋压榨机减速机","PX8110R4-RRH-250",2000001715,"台",1,null,"2014-03-31",null,null,{"v":65382.5,"d":"65,382.50"},{"v":50916.63,"d":"50,916.63"},"脱墨浆停产","良好"]
[387,"吉林晨鸣","制浆分厂","热分散机减速机","PX8110P2-LR-10",2000001716,"台",1,null,"2014-03-31",null,null,{"v":65382.5,"d":"65,382.50"},{"v":50916.63,"d":"50,916.63"},"脱墨浆停产","良好"]
[388,"吉林晨鸣","制浆分厂","后浮选槽供料泵","S350—470CD",2000001717,"台",1,null,"2014-03-31",null,null,{"v":78518.54,"d":"78,518.54"},{"v":61146.32,"d":"61,146.32"},"脱墨浆停产","良好"]
[389,"吉林晨鸣","制浆分厂","一段低浓除渣器供料泵","FP60—500C",2000001718,"台",1,null,"2014-03-31",null,null,{"v":80879.98,"d":"80,879.98"},{"v":62985.28,"d":"62,985.28"},"脱墨浆停产","良好"]
[390,"吉林晨鸣","制浆分厂","前多盘清水2#泵","S500—600CC",2000001719,"台",1,null,"2014-03-31",null,null,{"v":83684.37,"d":"83,684.37"},{"v":65169.19,"d":"65,169.19"},"脱墨浆停产","良好"]
[391,"吉林晨鸣","制浆分厂","一段中浓除渣器供料泵","S500—600CD",2000001720,"台",1,null,"2014-03-31",null,null,{"v":91211.64,"d":"91,211.64"},{"v":71031.08,"d":"71,031.08"},"脱墨浆停产","良好"]
[392,"吉林晨鸣","制浆分厂","一段中浓除渣器供料池","V=10M3",2000001721,"台",1,null,"2014-03-31",null,null,{"v":101543.3,"d":"101,543.30"},{"v":79076.83,"d":"79,076.83"},"脱墨浆停产","良好"]
[393,"吉林晨鸣","制浆分厂","1#气浮清水泵","S350—470CC",2000001722,"台",1,null,"2014-03-31",null,null,{"v":101543.3,"d":"101,543.30"},{"v":79076.83,"d":"79,076.83"},"脱墨浆停产","良好"]
[394,"吉林晨鸣","制浆分厂","卸料泵","BA400/350—48MKB",2000001723,"台",1,null,"2014-03-31",null,null,{"v":101543.3,"d":"101,543.30"},{"v":79076.83,"d":"79,076.83"},"脱墨浆停产","良好"]
[395,"吉林晨鸣","制浆分厂","污泥混合罐","V=30M3",2000001724,"台",1,null,"2014-03-31",null,null,{"v":163533.26,"d":"163,533.26"},{"v":127351.51,"d":"127,351.51"},"脱墨浆停产","良好"]
[396,"吉林晨鸣","制浆分厂","三段压力精筛","GFF-600",2000001725,"台",1,null,"2014-03-31",null,null,{"v":192754.39,"d":"192,754.39"},{"v":150107.47,"d":"150,107.47"},"脱墨浆停产","良好"]
[397,"吉林晨鸣","制浆分厂","二段压力精筛","GFF-800",2000001726,"台",1,null,"2014-03-31",null,null,{"v":194528.24,"d":"194,528.24"},{"v":151488.87,"d":"151,488.87"},"脱墨浆停产","良好"]
[398,"吉林晨鸣","制浆分厂","1#气浮澄清器","CAF-450",2000001727,"台",1,null,"2014-03-31",null,null,{"v":194528.24,"d":"194,528.24"},{"v":151488.87,"d":"151,488.87"},"脱墨浆停产","良好"]
[399,"吉林晨鸣","制浆分厂","螺旋压榨机","SHX-900X5500L",2000001728,"台",1,null,"2014-03-31",null,null,{"v":196265.21,"d":"196,265.21"},{"v":152841.54,"d":"152,841.54"},"脱墨浆停产","良好"]
[400,"吉林晨鸣","制浆分厂","二段粗筛供料池","V=100M3",2000001729,"台",1,null,"2014-03-31",null,null,{"v":246186.53,"d":"246,186.53"},{"v":191717.77,"d":"191,717.77"},"脱墨浆停产","良好"]
[401,"吉林晨鸣","制浆分厂","H2O2贮存槽","V=50M3",2000001730,"台",1,null,"2014-03-31",null,null,{"v":246186.53,"d":"246,186.53"},{"v":191717.77,"d":"191,717.77"},"脱墨浆停产","良好"]
[402,"吉林晨鸣","制浆分厂","螺旋压榨机","PX8110R4-RRH-250",2000001731,"台",1,null,"2014-03-31",null,null,{"v":246186.53,"d":"246,186.53"},{"v":191717.77,"d":"191,717.77"},"脱墨浆停产","良好"]
[403,"吉林晨鸣","制浆分厂","后多盘浓缩机","M4PHT60",2000001732,"台",1,null,"2014-03-31",null,null,{"v":246186.53,"d":"246,186.53"},{"v":191717.77,"d":"191,717.77"},"脱墨浆停产","良好"]
[404,"吉林晨鸣","制浆分厂","Na2SiO3贮存槽","V=50M3",2000001733,"台",1,null,"2014-03-31",null,null,{"v":287513.17,"d":"287,513.17"},{"v":223900.89,"d":"223,900.89"},"脱墨浆停产","良好"]
[405,"吉林晨鸣","制浆分厂","NaOH贮存槽","V=10M3",2000001734,"台",1,null,"2014-03-31",null,null,{"v":287513.17,"d":"287,513.17"},{"v":223900.89,"d":"223,900.89"},"脱墨浆停产","良好"]
[406,"吉林晨鸣","制浆分厂","后浮选槽","MACC114A-800",2000001735,"台",1,null,"2014-03-31",null,null,{"v":422495.79,"d":"422,495.79"},{"v":329018.6,"d":"329,018.60"},"脱墨浆停产","良好"]
[407,"吉林晨鸣","制浆分厂","清水罐","V=10M3",2000001736,"台",1,null,"2014-03-31",null,null,{"v":810791.95,"d":"810,791.95"},{"v":631404.22,"d":"631,404.22"},"脱墨浆停产","良好"]
[408,"吉林晨鸣","制浆分厂","二段中浓除渣器供料泵","S125—400CD",2000001737,"台",1,null,"2014-03-31",null,null,{"v":1090648.4,"d":"1,090,648.40"},{"v":849342.43,"d":"849,342.43"},"脱墨浆停产","良好"]
[409,"吉林晨鸣","制浆分厂","前多盘浓缩机","VDF5.2-10/12",2000001739,"台",1,null,"2014-03-31",null,null,{"v":1461376.27,"d":"1,461,376.27"},{"v":1138046.78,"d":"1,138,046.78"},"脱墨浆停产","良好"]
[410,"吉林晨鸣","制浆分厂","链板机","V=10M3",2000001740,"台",1,null,"2014-03-31",null,null,{"v":1550762.14,"d":"1,550,762.14"},{"v":1207655.99,"d":"1,207,655.99"},"脱墨浆停产","良好"]
[411,"吉林晨鸣","制浆分厂","密封水过滤器","FP-GLQ-200\n-1.0/80B",2000001742,"台",1,null,"2014-03-31",null,null,{"v":255814.31,"d":"255,814.31"},{"v":199215.41,"d":"199,215.41"},"脱墨浆停产","良好"]
[412,"吉林晨鸣","制浆分厂","空气压缩机","YL90L-2",2000001743,"台",1,null,"2014-03-31",null,null,{"v":1099.85,"d":"1,099.85"},856.52,"脱墨浆停产","良好"]
[413,"吉林晨鸣","制浆分厂","空气压缩机","YL90L-2",2000001744,"台",1,null,"2014-03-31",null,null,{"v":1237.59,"d":"1,237.59"},963.78,"脱墨浆停产","良好"]
[414,"吉林晨鸣","制浆分厂","直流氩弧机1",null,2000001745,"台",1,null,"2014-03-31",null,null,{"v":6159.78,"d":"6,159.78"},{"v":4796.93,"d":"4,796.93"},"脱墨浆停产","良好"]
[415,"吉林晨鸣","制浆分厂","直流氩弧机2",null,2000001746,"台",1,null,"2014-03-31",null,null,{"v":6159.78,"d":"6,159.78"},{"v":4796.93,"d":"4,796.93"},"脱墨浆停产","良好"]
[416,"吉林晨鸣","制浆分厂","直流氩弧机3",null,2000001747,"台",1,null,"2014-03-31",null,null,{"v":6159.78,"d":"6,159.78"},{"v":4796.93,"d":"4,796.93"},"脱墨浆停产","良好"]
[417,"吉林晨鸣","制浆分厂","三精筛电机","Y28M-8 380R 2BK 22007-88",2000001748,"台",1,null,"2014-03-31",null,null,{"v":6798.78,"d":"6,798.78"},{"v":5294.55,"d":"5,294.55"},"脱墨浆停产","良好"]
[418,"吉林晨鸣","制浆分厂","纸库CD电动葫芦1","10T-18M",2000001749,"台",1,null,"2014-03-31",null,null,{"v":12949.48,"d":"12,949.48"},{"v":10084.39,"d":"10,084.39"},"脱墨浆停产","良好"]
[419,"吉林晨鸣","制浆分厂","汽车队CD电动葫芦","10T-18M",2000001750,"台",1,null,"2014-03-31",null,null,{"v":12949.48,"d":"12,949.48"},{"v":10084.39,"d":"10,084.39"},"脱墨浆停产","良好"]
[420,"吉林晨鸣","制浆分厂","全自动过滤器","FP-GLQ-200-1.0/8013",2000001751,"台",1,null,"2014-03-31",null,null,{"v":35575.57,"d":"35,575.57"},{"v":27704.47,"d":"27,704.47"},"脱墨浆停产","良好"]
[421,"吉林晨鸣","制浆分厂","成浆泵现场按钮箱",null,2000001752,"台",1,null,"2014-03-31",null,null,79.11,61.61,"脱墨浆停产","良好"]
[422,"吉林晨鸣","制浆分厂","漂白液碱计量泵变频器","ATV313KW",2000001753,"台",1,null,"2014-03-31",null,null,{"v":2613.74,"d":"2,613.74"},{"v":2035.44,"d":"2,035.44"},"脱墨浆停产","良好"]
[423,"吉林晨鸣","制浆分厂","螺杆泵1","FG50-1",2000001754,"台",1,null,"2014-03-31",null,null,{"v":3557.33,"d":"3,557.33"},{"v":2770.27,"d":"2,770.27"},"脱墨浆停产","良好"]
[424,"吉林晨鸣","制浆分厂","螺杆泵2","FG50-1",2000001755,"台",1,null,"2014-03-31",null,null,{"v":3558.67,"d":"3,558.67"},{"v":2771.31,"d":"2,771.31"},"脱墨浆停产","良好"]
[425,"吉林晨鸣","制浆分厂","螺杆泵3","FG50-1",2000001756,"台",1,null,"2014-03-31",null,null,{"v":3559.45,"d":"3,559.45"},{"v":2771.92,"d":"2,771.92"},"脱墨浆停产","良好"]
[426,"吉林晨鸣","制浆分厂","螺杆泵","FG25-1",2000001757,"台",1,null,"2014-03-31",null,null,{"v":4111.12,"d":"4,111.12"},{"v":3201.54,"d":"3,201.54"},"脱墨浆停产","良好"]
[427,"吉林晨鸣","制浆分厂","空压机","W-1.6/10",2000001758,"台",1,null,"2014-03-31",null,null,{"v":4743.49,"d":"4,743.49"},{"v":3693.97,"d":"3,693.97"},"脱墨浆停产","良好"]
[428,"吉林晨鸣","制浆分厂","螺杆泵","FG30-1",2000001759,"台",1,null,"2014-03-31",null,null,{"v":6640.55,"d":"6,640.55"},{"v":5171.34,"d":"5,171.34"},"脱墨浆停产","良好"]
[429,"吉林晨鸣","制浆分厂","脱墨剂贮存罐不锈钢罐","直径2000*2000",2000001761,"台",1,null,"2014-03-31",null,null,{"v":22926.27,"d":"22,926.27"},{"v":17853.84,"d":"17,853.84"},"脱墨浆停产","良好"]
[430,"吉林晨鸣","制浆分厂","链板机2#减速机","UJ-8850",2000001762,"台",1,null,"2014-03-31",null,null,{"v":74521.62,"d":"74,521.62"},{"v":58033.73,"d":"58,033.73"},"脱墨浆停产","良好"]
[431,"吉林晨鸣","制浆分厂","链板机2#","UJ-8850",2000001763,"台",1,null,"2014-03-31",null,null,{"v":126319.53,"d":"126,319.53"},{"v":98371.32,"d":"98,371.32"},"脱墨浆停产","良好"]
[432,"吉林晨鸣","制浆分厂","耐腐蚀离心泵(B)","SC32-160A",2000001764,"台",1,null,"2014-03-31",null,null,{"v":23242.74,"d":"23,242.74"},{"v":18100.3,"d":"18,100.30"},"脱墨浆停产","良好"]
[433,"吉林晨鸣","制浆分厂","不锈钢罐","直径2800*2500",2000001765,"台",1,null,"2014-03-31",null,null,{"v":32413.26,"d":"32,413.26"},{"v":25241.81,"d":"25,241.81"},"脱墨浆停产","良好"]
[434,"吉林晨鸣","制浆分厂","浆泵S3-125-400CD","SMS/132KW",2000001766,"台",1,null,"2014-03-31",null,null,{"v":36370.82,"d":"36,370.82"},{"v":28323.76,"d":"28,323.76"},"脱墨浆停产","良好"]
[435,"吉林晨鸣","制浆分厂","后浮选供料泵控制柜","GGD配电柜",2000001767,"台",1,null,"2014-03-31",null,null,{"v":7510.24,"d":"7,510.24"},{"v":5848.6,"d":"5,848.60"},"脱墨浆停产","良好"]
[436,"吉林晨鸣","制浆分厂","二精搅拌器电机Y1603-L-6","11KW",2000001769,"台",1,null,"2014-03-31",null,null,{"v":1343.81,"d":"1,343.81"},{"v":1046.5,"d":"1,046.50"},"脱墨浆停产","良好"]
[437,"吉林晨鸣","制浆分厂","链板机电机Y225M-4/IP44/380V","45KW",2000001770,"台",1,null,"2014-03-31",null,null,{"v":3130.91,"d":"3,130.91"},{"v":2438.2,"d":"2,438.20"},"脱墨浆停产","良好"]
[438,"吉林晨鸣","制浆分厂","预浮选供料泵电机Y250M-4/V1","55KW",2000001771,"台",1,null,"2014-03-31",null,null,{"v":4190.24,"d":"4,190.24"},{"v":3263.15,"d":"3,263.15"},"脱墨浆停产","良好"]
[439,"吉林晨鸣","制浆分厂","高浓除渣器入口压力显示","CECYS-153BG22",2000001772,"台",1,null,"2014-03-31",null,null,{"v":4743.49,"d":"4,743.49"},{"v":3693.97,"d":"3,693.97"},"脱墨浆停产","良好"]
[440,"吉林晨鸣","制浆分厂","高浓除渣器出口压力显示","CECYS-153BG22",2000001773,"台",1,null,"2014-03-31",null,null,{"v":4743.49,"d":"4,743.49"},{"v":3693.97,"d":"3,693.97"},"脱墨浆停产","良好"]
[441,"吉林晨鸣","制浆分厂","一段中浓除渣器入口压力显示","CECYS-153BG22",2000001774,"台",1,null,"2014-03-31",null,null,{"v":4743.49,"d":"4,743.49"},{"v":3693.97,"d":"3,693.97"},"脱墨浆停产","报废"]
[442,"吉林晨鸣","制浆分厂","三粗供料池液位显示","CECYS-153BG22",2000001776,"台",1,null,"2014-03-31",null,null,{"v":4743.49,"d":"4,743.49"},{"v":3693.97,"d":"3,693.97"},"脱墨浆停产","良好"]
[443,"吉林晨鸣","制浆分厂","后浮选供料泵电机Y315L2-4","200KW",2000001777,"台",1,null,"2014-03-31",null,null,{"v":13755.77,"d":"13,755.77"},{"v":10712.3,"d":"10,712.30"},"脱墨浆停产","良好"]
[444,"吉林晨鸣","制浆分厂","减速机","XWD6-17-11",2000001778,"台",1,null,"2014-03-31",null,null,{"v":2924.98,"d":"2,924.98"},{"v":2277.84,"d":"2,277.84"},"脱墨浆停产","良好"]
[445,"吉林晨鸣","制浆分厂","减速机208搅拌","XWD6-17-11",2000001780,"台",1,null,"2014-03-31",null,null,{"v":7826.69,"d":"7,826.69"},{"v":6095.04,"d":"6,095.04"},"脱墨浆停产","良好"]
[446,"吉林晨鸣","制浆分厂","碎浆机冲洗水阀","AP11-25-D3K-DC24V RC1",2000001782,"台",1,null,"2014-03-31",null,null,{"v":5212.27,"d":"5,212.27"},{"v":4059.07,"d":"4,059.07"},"脱墨浆停产","良好"]
[447,"吉林晨鸣","制浆分厂","粗选机渣浆排放阀，汽缸式刀闸阀","336D-C/DN125",2000001784,"台",1,null,"2014-03-31",null,null,{"v":12382.68,"d":"12,382.68"},{"v":9643.01,"d":"9,643.01"},"脱墨浆停产","良好"]
[448,"吉林晨鸣","制浆分厂","中浓除渣器阀门气动刀闸阀","336D-C/DN100",2000001785,"台",1,null,"2014-03-31",null,null,{"v":16932.25,"d":"16,932.25"},{"v":13186,"d":"13,186.00"},"脱墨浆停产","良好"]
[449,"吉林晨鸣","制浆分厂","压力筛阀门","AW13-EO105-31.1T/DN100",2000001788,"台",1,null,"2014-03-31",null,null,{"v":25412.78,"d":"25,412.78"},{"v":19790.2,"d":"19,790.20"},"脱墨浆停产","良好"]
[450,"吉林晨鸣","制浆分厂","一粗电流变送器","LIDJ-12AR",2000001792,"台",1,null,"2014-03-31",null,null,{"v":1107.04,"d":"1,107.04"},862.09,"脱墨浆停产","良好"]
[451,"吉林晨鸣","制浆分厂","二粗电流变送器","LIDJ-12AR",2000001793,"台",1,null,"2014-03-31",null,null,{"v":1107.04,"d":"1,107.04"},862.09,"脱墨浆停产","良好"]
[452,"吉林晨鸣","制浆分厂","三粗电流变送器","LIDJ-12AR",2000001794,"台",1,null,"2014-03-31",null,null,{"v":1107.04,"d":"1,107.04"},862.09,"脱墨浆停产","良好"]
[453,"吉林晨鸣","制浆分厂","一精电流变送器","LIDJ-12AR",2000001795,"台",1,null,"2014-03-31",null,null,{"v":1107.04,"d":"1,107.04"},862.09,"脱墨浆停产","良好"]
[454,"吉林晨鸣","制浆分厂","二精电流变送器","LIDJ-12AR",2000001796,"台",1,null,"2014-03-31",null,null,{"v":1107.04,"d":"1,107.04"},862.09,"脱墨浆停产","良好"]
[455,"吉林晨鸣","制浆分厂","三精电流变送器","LIDJ-12AR",2000001797,"台",1,null,"2014-03-31",null,null,{"v":1107.04,"d":"1,107.04"},862.09,"脱墨浆停产","良好"]
[456,"吉林晨鸣","制浆分厂","预浮选1#泵电流显示","LIDJ-12AR",2000001798,"台",1,null,"2014-03-31",null,null,{"v":1107.04,"d":"1,107.04"},862.09,"脱墨浆停产","良好"]
[457,"吉林晨鸣","制浆分厂","预浮选2#泵电流显示","LIDJ-12AR",2000001799,"台",1,null,"2014-03-31",null,null,{"v":1107.04,"d":"1,107.04"},862.09,"脱墨浆停产","良好"]
[458,"吉林晨鸣","制浆分厂","预浮选3#泵电流显示","LIDJ-12AR",2000001800,"台",1,null,"2014-03-31",null,null,{"v":1107.04,"d":"1,107.04"},862.09,"脱墨浆停产","良好"]
[459,"吉林晨鸣","制浆分厂","预浮选4#泵电流显示","LIDJ-12AR",2000001801,"台",1,null,"2014-03-31",null,null,{"v":1107.04,"d":"1,107.04"},862.09,"脱墨浆停产","良好"]
[460,"吉林晨鸣","制浆分厂","预浮选5#泵电流显示","LIDJ-12AR",2000001802,"台",1,null,"2014-03-31",null,null,{"v":1107.04,"d":"1,107.04"},862.09,"脱墨浆停产","良好"]
[461,"吉林晨鸣","制浆分厂","预浮选6#泵电流显示","LIDJ-12AR",2000001803,"台",1,null,"2014-03-31",null,null,{"v":1107.04,"d":"1,107.04"},862.09,"脱墨浆停产","良好"]
[462,"吉林晨鸣","制浆分厂","预浮选7#泵电流显示","LIDJ-12AR",2000001804,"台",1,null,"2014-03-31",null,null,{"v":1107.04,"d":"1,107.04"},862.09,"脱墨浆停产","良好"]
[463,"吉林晨鸣","制浆分厂","预浮选8#泵电流显示","LIDJ-12AR",2000001805,"台",1,null,"2014-03-31",null,null,{"v":1107.04,"d":"1,107.04"},862.09,"脱墨浆停产","良好"]
[464,"吉林晨鸣","制浆分厂","预浮选9#泵电流显示","LIDJ-12AR",2000001806,"台",1,null,"2014-03-31",null,null,{"v":1107.04,"d":"1,107.04"},862.09,"脱墨浆停产","良好"]
[465,"吉林晨鸣","制浆分厂","预浮选10#泵电流显示","LIDJ-12AR",2000001807,"台",1,null,"2014-03-31",null,null,{"v":1107.04,"d":"1,107.04"},862.09,"脱墨浆停产","良好"]
[466,"吉林晨鸣","制浆分厂","预浮选11#泵电流显示","LIDJ-12AR",2000001808,"台",1,null,"2014-03-31",null,null,{"v":1107.04,"d":"1,107.04"},862.09,"脱墨浆停产","良好"]
[467,"吉林晨鸣","制浆分厂","预浮选12#泵电流显示","LIDJ-12AR",2000001809,"台",1,null,"2014-03-31",null,null,{"v":1107.04,"d":"1,107.04"},862.09,"脱墨浆停产","良好"]
[468,"吉林晨鸣","制浆分厂","预浮选13#泵电流显示","LIDJ-12AR",2000001810,"台",1,null,"2014-03-31",null,null,{"v":1107.04,"d":"1,107.04"},862.09,"脱墨浆停产","良好"]
[469,"吉林晨鸣","制浆分厂","小精筛电流显示","LIDJ-12AR",2000001811,"台",1,null,"2014-03-31",null,null,{"v":1107.04,"d":"1,107.04"},862.09,"脱墨浆停产","良好"]
[470,"吉林晨鸣","制浆分厂","减速机X061","35-5.5",2000001812,"台",1,null,"2014-03-31",null,null,{"v":2529.97,"d":"2,529.97"},{"v":1970.2,"d":"1,970.20"},"脱墨浆停产","良好"]
[471,"吉林晨鸣","制浆分厂","减速机X062","35-5.5",2000001813,"台",1,null,"2014-03-31",null,null,{"v":2529.99,"d":"2,529.99"},{"v":1970.22,"d":"1,970.22"},"脱墨浆停产","良好"]
[472,"吉林晨鸣","制浆分厂","压力变送器","MP50-LT45B3",2000001816,"台",1,null,"2014-03-31",null,null,{"v":6482.88,"d":"6,482.88"},{"v":5048.54,"d":"5,048.54"},"脱墨浆停产","报废"]
[473,"吉林晨鸣","制浆分厂","气动切断阀","MQ-120P",2000001817,"台",1,null,"2014-03-31",null,null,{"v":6798.78,"d":"6,798.78"},{"v":5294.55,"d":"5,294.55"},"脱墨浆停产","良好"]
[474,"吉林晨鸣","制浆分厂","硫酸供料泵","YST7124",2000001818,"台",1,null,"2014-03-31",null,null,{"v":80071.39,"d":"80,071.39"},{"v":62355.6,"d":"62,355.60"},"脱墨浆停产","良好"]
[475,"吉林晨鸣","制浆分厂","PILOT驱动阀碎浆机密封水阀门遥控","B25A-D3K-DC24V",2000001819,"台",1,null,"2014-03-31",null,null,{"v":1976.17,"d":"1,976.17"},{"v":1538.93,"d":"1,538.93"},"脱墨浆停产","良好"]
[476,"吉林晨鸣","制浆分厂","碎浆机冲洗水阀门遥控","B25A-D3K-DC24V",2000001820,"台",1,null,"2014-03-31",null,null,{"v":1977.51,"d":"1,977.51"},{"v":1539.98,"d":"1,539.98"},"脱墨浆停产","良好"]
[477,"吉林晨鸣","制浆分厂","油泵单元冷却水阀门遥控","B25A-D3K-DC24V",2000001821,"台",1,null,"2014-03-31",null,null,{"v":1978.3,"d":"1,978.30"},{"v":1540.61,"d":"1,540.61"},"脱墨浆停产","良好"]
[478,"吉林晨鸣","制浆分厂","单插液位变送器双氧水储存罐液位显示",null,2000001822,"台",1,null,"2014-03-31",null,null,{"v":5492.77,"d":"5,492.77"},{"v":4277.5,"d":"4,277.50"},"脱墨浆停产","良好"]
[479,"吉林晨鸣","制浆分厂","低浓除渣器压力显示7#",null,2000001823,"台",1,null,"2014-03-31",null,null,{"v":5492.77,"d":"5,492.77"},{"v":4277.5,"d":"4,277.50"},"脱墨浆停产","良好"]
[480,"吉林晨鸣","制浆分厂","1段低浓供料池液位",null,2000001824,"台",1,null,"2014-03-31",null,null,{"v":5492.77,"d":"5,492.77"},{"v":4277.5,"d":"4,277.50"},"脱墨浆停产","报废"]
[481,"吉林晨鸣","制浆分厂","单平液位变送器低浓除渣器压力显示8#",null,2000001825,"台",1,null,"2014-03-31",null,null,{"v":6038.44,"d":"6,038.44"},{"v":4702.43,"d":"4,702.43"},"脱墨浆停产","报废"]
[482,"吉林晨鸣","制浆分厂","单平液位变送器低浓除渣器压力显示9#",null,2000001826,"台",1,null,"2014-03-31",null,null,{"v":6038.44,"d":"6,038.44"},{"v":4702.43,"d":"4,702.43"},"脱墨浆停产","报废"]
[483,"吉林晨鸣","制浆分厂","单平液位变送器低浓除渣器压力显示10#",null,2000001827,"台",1,null,"2014-03-31",null,null,{"v":6038.44,"d":"6,038.44"},{"v":4702.43,"d":"4,702.43"},"脱墨浆停产","报废"]
[484,"吉林晨鸣","制浆分厂","成浆出口电磁流量计","DN200",2000001828,"台",1,null,"2014-03-31",null,null,{"v":19606.29,"d":"19,606.29"},{"v":15268.41,"d":"15,268.41"},"脱墨浆停产","良好"]
[485,"吉林晨鸣","制浆分厂","三精尾浆出口电磁流量计","LDY-100S",2000001829,"台",1,null,"2014-03-31",null,null,{"v":7510.24,"d":"7,510.24"},{"v":5848.6,"d":"5,848.60"},"脱墨浆停产","良好"]
[486,"吉林晨鸣","制浆分厂","商品浆电磁流量计","LDY-200S",2000001830,"台",1,null,"2014-03-31",null,null,{"v":9486.96,"d":"9,486.96"},{"v":7387.99,"d":"7,387.99"},"脱墨浆停产","良好"]
[487,"吉林晨鸣","制浆分厂","浆泵2#气浮","S3-100-350DD18.5KW",2000001831,"台",1,null,"2014-03-31",null,null,{"v":22506.84,"d":"22,506.84"},{"v":17527.19,"d":"17,527.19"},"脱墨浆停产","良好"]
[488,"吉林晨鸣","制浆分厂","浆泵跳筛供料","S3-100-350GDD/S18.5KW",2000001832,"台",1,null,"2014-03-31",null,null,{"v":22759.89,"d":"22,759.89"},{"v":17724.26,"d":"17,724.26"},"脱墨浆停产","良好"]
[489,"吉林晨鸣","制浆分厂","浆泵1#气浮循环","S3-100-350W55KW",2000001833,"台",1,null,"2014-03-31",null,null,{"v":25590.64,"d":"25,590.64"},{"v":19928.7,"d":"19,928.70"},"脱墨浆停产","良好"]
[490,"吉林晨鸣","制浆分厂","液碱储存罐出口电磁流量计","LDY-25S-61",2000001834,"台",1,null,"2014-03-31",null,null,{"v":6982.02,"d":"6,982.02"},{"v":5437.25,"d":"5,437.25"},"脱墨浆停产","良好"]
[491,"吉林晨鸣","制浆分厂","污泥絮凝剂电磁流量计","LDY-50S-61",2000001835,"台",1,null,"2014-03-31",null,null,{"v":6982.02,"d":"6,982.02"},{"v":5437.25,"d":"5,437.25"},"脱墨浆停产","良好"]
[492,"吉林晨鸣","制浆分厂","1#中浓控制泵变频控制柜","GGD132KW",2000001836,"台",1,null,"2014-03-31",null,null,{"v":50596.05,"d":"50,596.05"},{"v":39401.68,"d":"39,401.68"},"脱墨浆停产","良好"]
[493,"吉林晨鸣","制浆分厂","气动调节阀温水罐清水加入阀门","DN200",2000001842,"台",1,null,"2014-03-31",null,null,{"v":7945.35,"d":"7,945.35"},{"v":6187.44,"d":"6,187.44"},"脱墨浆停产","良好"]
[494,"吉林晨鸣","制浆分厂","管道泵电机变频器备用","EV2000-4T0370C",2000001843,"台",1,null,"2014-03-31",null,null,{"v":10277.54,"d":"10,277.54"},{"v":8003.63,"d":"8,003.63"},"脱墨浆停产","良好"]
[495,"吉林晨鸣","制浆分厂","1#热分散蒸汽加入气动V型调节球阀","DN150",2000001844,"台",1,null,"2014-03-31",null,null,{"v":3417.14,"d":"3,417.14"},{"v":2661.1,"d":"2,661.10"},"脱墨浆停产","良好"]
[496,"吉林晨鸣","制浆分厂","2#热分散蒸汽加入气动V型调节球阀","DN150",2000001845,"台",1,null,"2014-03-31",null,null,{"v":3417.14,"d":"3,417.14"},{"v":2661.1,"d":"2,661.10"},"脱墨浆停产","良好"]
[497,"吉林晨鸣","制浆分厂","温水罐纸机白水加入气动通断球阀","DN200",2000001846,"台",1,null,"2014-03-31",null,null,{"v":8593.43,"d":"8,593.43"},{"v":6692.14,"d":"6,692.14"},"脱墨浆停产","良好"]
[498,"吉林晨鸣","制浆分厂","搅拌器","2000*2500",2000001847,"台",1,null,"2014-03-31",null,null,{"v":11858.71,"d":"11,858.71"},{"v":9234.98,"d":"9,234.98"},"脱墨浆停产","良好"]
[499,"吉林晨鸣","制浆分厂","搅拌器","2000*4000",2000001848,"台",1,null,"2014-03-31",null,null,{"v":21187.45,"d":"21,187.45"},{"v":16499.72,"d":"16,499.72"},"脱墨浆停产","良好"]
[500,"吉林晨鸣","制浆分厂","干粉加湿器",null,2000001849,"台",1,null,"2014-03-31",null,null,{"v":75894.64,"d":"75,894.64"},{"v":59102.94,"d":"59,102.94"},"脱墨浆停产","良好"]
[501,"吉林晨鸣","制浆分厂","二浊泵电机","90KW",2000001850,"台",1,null,"2014-03-31",null,null,{"v":10593.44,"d":"10,593.44"},{"v":8249.64,"d":"8,249.64"},"脱墨浆停产","良好"]
[502,"吉林晨鸣","制浆分厂","三精筛电机","MDIC200L1-6-22KW",2000001851,"台",1,null,"2014-03-31",null,null,{"v":3756.86,"d":"3,756.86"},{"v":2925.64,"d":"2,925.64"},"脱墨浆停产","良好"]
[503,"吉林晨鸣","制浆分厂","转鼓碎浆机NaoH电磁流量计","AE202DG-AS2-TSJ/Q2C",2000001852,"台",1,null,"2014-03-31",null,null,{"v":10577.72,"d":"10,577.72"},{"v":8237.39,"d":"8,237.39"},"脱墨浆停产","良好"]
[504,"吉林晨鸣","制浆分厂","转鼓碎浆机固体脱墨剂电磁流量计","AE202DG-AS2-TSJ/Q2C",2000001853,"台",1,null,"2014-03-31",null,null,{"v":10577.73,"d":"10,577.73"},{"v":8237.4,"d":"8,237.40"},"脱墨浆停产","良好"]
[505,"吉林晨鸣","制浆分厂","大磨NaSiO3电磁流量计","AE202DG-AS2-TSJ/Q2C",2000001854,"台",1,null,"2014-03-31",null,null,{"v":10577.73,"d":"10,577.73"},{"v":8237.4,"d":"8,237.40"},"脱墨浆停产","良好"]
[506,"吉林晨鸣","制浆分厂","污泥絮凝剂储存罐出口电磁流量计","AE204DG-AS2-TSJ/Q2C",2000001855,"台",1,null,"2014-03-31",null,null,{"v":10735.96,"d":"10,735.96"},{"v":8360.62,"d":"8,360.62"},"脱墨浆停产","良好"]
[507,"吉林晨鸣","制浆分厂","三楼碳酸钙加入泵检修电源柜","GGD",2000001856,"台",1,null,"2014-03-31",null,null,{"v":11621.37,"d":"11,621.37"},{"v":9050.15,"d":"9,050.15"},"脱墨浆停产","良好"]
[508,"吉林晨鸣","制浆分厂","成浆机量检修电源柜","GGD",2000001857,"台",1,null,"2014-03-31",null,null,{"v":11621.37,"d":"11,621.37"},{"v":9050.15,"d":"9,050.15"},"脱墨浆停产","良好"]
[509,"吉林晨鸣","制浆分厂","后浮选供料泵电机","Y315-4-200KW",2000001858,"台",1,null,"2014-03-31",null,null,{"v":15021.05,"d":"15,021.05"},{"v":11697.63,"d":"11,697.63"},"脱墨浆停产","良好"]
[510,"吉林晨鸣","制浆分厂","中浓浆泵出口泵温度指示调节","DN80",2000001860,"台",1,null,"2014-03-31",null,null,{"v":3912.75,"d":"3,912.75"},{"v":3047.07,"d":"3,047.07"},"脱墨浆停产","良好"]
[511,"吉林晨鸣","制浆分厂","成浆池出口稀释水气动V型调节阀","DN80",2000001861,"台",1,null,"2014-03-31",null,null,{"v":3912.77,"d":"3,912.77"},{"v":3047.07,"d":"3,047.07"},"脱墨浆停产","良好"]
[512,"吉林晨鸣","制浆分厂","匀浆池入口浆加入气动O型开关阀","DN200",2000001862,"台",1,null,"2014-03-31",null,null,{"v":7370.62,"d":"7,370.62"},{"v":5739.86,"d":"5,739.86"},"脱墨浆停产","良好"]
[513,"吉林晨鸣","制浆分厂","温水罐顶部白水加入气动开关蝶阀","DN250",2000001863,"台",1,null,"2014-03-31",null,null,{"v":10299.67,"d":"10,299.67"},{"v":8020.87,"d":"8,020.87"},"脱墨浆停产","良好"]
[514,"吉林晨鸣","制浆分厂","格力空调低压变电所","KFR-120LW/E(1253L)-SNS",2000001864,"台",1,null,"2014-03-31",null,null,{"v":7549.8,"d":"7,549.80"},{"v":5879.41,"d":"5,879.41"},"脱墨浆停产","良好"]
[515,"吉林晨鸣","制浆分厂","格力空调纸库变电所","KFR-120LW/E(1253L)-SNS",2000001865,"台",1,null,"2014-03-31",null,null,{"v":9502.67,"d":"9,502.67"},{"v":7400.2,"d":"7,400.20"},"脱墨浆停产","良好"]
[516,"吉林晨鸣","制浆分厂","大磨双氧水加入电磁流量计","AE202DG-CS2-ESJ/QIC",2000001868,"台",1,null,"2014-03-31",null,null,{"v":11621.37,"d":"11,621.37"},{"v":9050.15,"d":"9,050.15"},"脱墨浆停产","良好"]
[517,"吉林晨鸣","制浆分厂","1#热分散NaoH加入电磁流量计","AE202DG-CS2-ESJ/QIC",2000001869,"台",1,null,"2014-03-31",null,null,{"v":11621.37,"d":"11,621.37"},{"v":9050.15,"d":"9,050.15"},"脱墨浆停产","良好"]
[518,"吉林晨鸣","制浆分厂","2#热分散NaoH加入电磁流量计","AE202DG-CS2-ESJ/QIC",2000001870,"台",1,null,"2014-03-31",null,null,{"v":11621.37,"d":"11,621.37"},{"v":9050.15,"d":"9,050.15"},"脱墨浆停产","良好"]
[519,"吉林晨鸣","制浆分厂","2#热分散NaSiO3加入电磁流量计","AE202DG-CS2-ESJ/QIC",2000001871,"台",1,null,"2014-03-31",null,null,{"v":11621.37,"d":"11,621.37"},{"v":9050.15,"d":"9,050.15"},"脱墨浆停产","良好"]
[520,"吉林晨鸣","制浆分厂","电磁流量计","AE215DG-AS2-TTJ/QIC",2000001874,"台",1,null,"2014-03-31",null,null,{"v":15346.24,"d":"15,346.24"},{"v":11950.88,"d":"11,950.88"},"脱墨浆停产","良好"]
[521,"吉林晨鸣","制浆分厂","电动机","Y4-37KW",2000001875,"台",1,null,"2014-03-31",null,null,{"v":3557.33,"d":"3,557.33"},{"v":2770.27,"d":"2,770.27"},"脱墨浆停产","良好"]
[522,"吉林晨鸣","制浆分厂","辅房计量泵检修电源柜","GGD",2000001876,"台",1,null,"2014-03-31",null,null,{"v":11542.25,"d":"11,542.25"},{"v":8988.53,"d":"8,988.53"},"脱墨浆停产","良好"]
[523,"吉林晨鸣","制浆分厂","2#还原漂白搅龙电机","30KW—4级",2000001878,"台",1,null,"2014-03-31",null,null,{"v":68385.91,"d":"68,385.91"},{"v":53255.51,"d":"53,255.51"},"脱墨浆停产","良好"]
[524,"吉林晨鸣","制浆分厂","2#还原漂白电机","55KW—4级",2000001879,"台",1,null,"2014-03-31",null,null,{"v":71160.8,"d":"71,160.80"},{"v":55416.45,"d":"55,416.45"},"脱墨浆停产","良好"]
[525,"吉林晨鸣","制浆分厂","输送搅笼","直径660×7110",2000001881,"台",1,null,"2014-03-31",null,null,{"v":144818.78,"d":"144,818.78"},{"v":112777.63,"d":"112,777.63"},"脱墨浆停产","良好"]
[526,"吉林晨鸣","制浆分厂","输送搅笼","直径660×5000",2000001882,"台",1,null,"2014-03-31",null,null,{"v":144818.78,"d":"144,818.78"},{"v":112777.63,"d":"112,777.63"},"脱墨浆停产","良好"]
[527,"吉林晨鸣","制浆分厂","1#挤浆机减速机","SEW-EURODRIVE TYP M3PSE8",2000001883,"台",1,null,"2014-03-31",null,null,{"v":163318.04,"d":"163,318.04"},{"v":127183.93,"d":"127,183.93"},"脱墨浆停产","良好"]
[528,"吉林晨鸣","制浆分厂","挤浆机","ZNJ160",2000001884,"台",1,null,"2014-03-31",null,null,{"v":281975.96,"d":"281,975.96"},{"v":219588.77,"d":"219,588.77"},"脱墨浆停产","良好"]
[529,"吉林晨鸣","制浆分厂","2#挤浆机",null,2000001886,"台",1,null,"2014-03-31",null,null,{"v":402342.73,"d":"402,342.73"},{"v":313324.41,"d":"313,324.41"},"脱墨浆停产","良好"]
[530,"吉林晨鸣","制浆分厂","MD1型电动葫芦","5T*18M",2000001887,"台",1,null,"2014-03-31",null,null,{"v":6012.03,"d":"6,012.03"},{"v":4681.87,"d":"4,681.87"},"脱墨浆停产","良好"]
[531,"吉林晨鸣","制浆分厂","转鼓碎浆机蒸汽加入气动V型调节球阀","ZSSV-16TK150YPD2D",2000001889,"台",1,null,"2014-03-31",null,null,{"v":9987.85,"d":"9,987.85"},{"v":7778.05,"d":"7,778.05"},"脱墨浆停产","良好"]
[532,"吉林晨鸣","制浆分厂","1#中浓泵附属检修电源柜","GGD",2000001890,"台",1,null,"2014-03-31",null,null,{"v":11542.25,"d":"11,542.25"},{"v":8988.53,"d":"8,988.53"},"脱墨浆停产","良好"]
[533,"吉林晨鸣","制浆分厂","变送器","EJA438N-EASG24EB-AB05-92",2000001891,"台",1,null,"2014-03-31",null,null,{"v":51114.95,"d":"51,114.95"},{"v":39805.78,"d":"39,805.78"},"脱墨浆停产","良好"]
[534,"吉林晨鸣","制浆分厂","新一精筛子电机","90KW—8  两台",2000001892,"台",1,null,"2014-03-31",null,null,{"v":181817.29,"d":"181,817.29"},{"v":141590.2,"d":"141,590.20"},"脱墨浆停产","良好"]
[535,"吉林晨鸣","制浆分厂","新四精","S3—80—265DD",2000001893,"台",1,null,"2014-03-31",null,null,{"v":209566.18,"d":"209,566.18"},{"v":163199.65,"d":"163,199.65"},"脱墨浆停产","良好"]
[536,"吉林晨鸣","制浆分厂","新一精2","S3—200—470DD",2000001894,"台",1,null,"2014-03-31",null,null,{"v":263598.32,"d":"263,598.32"},{"v":205277.2,"d":"205,277.20"},"脱墨浆停产","良好"]
[537,"吉林晨鸣","制浆分厂","新三精","S3—150—400DD",2000001895,"台",1,null,"2014-03-31",null,null,{"v":483879.17,"d":"483,879.17"},{"v":376820.92,"d":"376,820.92"},"脱墨浆停产","良好"]
[538,"吉林晨鸣","制浆分厂","新一精筛子1","1.2米两台",2000001896,"台",1,null,"2014-03-31",null,null,{"v":676628.27,"d":"676,628.27"},{"v":526924.28,"d":"526,924.28"},"脱墨浆停产","良好"]
[539,"吉林晨鸣","制浆分厂","电磁流量计","AE215DG-AS2-LSJ/QIC",2000001898,"台",1,null,"2014-03-31",null,null,{"v":13652.03,"d":"13,652.03"},{"v":10631.52,"d":"10,631.52"},"脱墨浆停产","良好"]
[540,"吉林晨鸣","制浆分厂","电磁流量计","AE205DG-AS2-LSJ/QIC",2000001900,"台",1,null,"2014-03-31",null,null,{"v":10279.25,"d":"10,279.25"},{"v":8004.95,"d":"8,004.95"},"脱墨浆停产","良好"]
[541,"吉林晨鸣","制浆分厂","电机","Y2-280S-4    75KW",2000001901,"台",1,null,"2014-03-31",null,null,{"v":9214.76,"d":"9,214.76"},{"v":7176.01,"d":"7,176.01"},"脱墨浆停产","良好"]
[542,"吉林晨鸣","制浆分厂","电机","Y2-160L-4     30KW    F",2000001902,"台",1,null,"2014-03-31",null,null,{"v":4168.84,"d":"4,168.84"},{"v":3246.47,"d":"3,246.47"},"脱墨浆停产","良好"]
[543,"吉林晨鸣","制浆分厂","电磁流量计","AE215DG-AS2-LSJ/QIC",2000001903,"台",1,null,"2014-03-31",null,null,{"v":13796.76,"d":"13,796.76"},{"v":10744.24,"d":"10,744.24"},"脱墨浆停产","良好"]
[544,"吉林晨鸣","制浆分厂","柜式暧风机","二匹",2000001905,"台",1,null,"2014-03-31",null,null,{"v":4138.25,"d":"4,138.25"},{"v":3222.66,"d":"3,222.66"},"脱墨浆停产","良好"]
[545,"吉林晨鸣","制浆分厂","电磁流量计","LDY100",2000001906,"台",1,null,"2014-03-31",null,null,{"v":7784.72,"d":"7,784.72"},{"v":6062.36,"d":"6,062.36"},"脱墨浆停产","良好"]
[546,"吉林晨鸣","制浆分厂","电焊机","PE10-500",2000001907,"台",1,null,"2014-03-31",null,null,{"v":5456.41,"d":"5,456.41"},{"v":4249.17,"d":"4,249.17"},"脱墨浆停产","良好"]
[547,"吉林晨鸣","制浆分厂","压力变送器","PMP48",2000001908,"台",1,"0-100KPA","2014-03-31","E+H",null,{"v":23454.78,"d":"23,454.78"},{"v":18265.41,"d":"18,265.41"},"脱墨浆停产","良好"]
[548,"吉林晨鸣","制浆分厂","压力变送器","PMP48",2000001909,"台",1,"0-100KPA","2014-03-31","E+H",null,{"v":23454.78,"d":"23,454.78"},{"v":18265.41,"d":"18,265.41"},"脱墨浆停产","良好"]
[549,"吉林晨鸣","制浆分厂","压力变送器","PMP48",2000001910,"台",1,"0-100KPA","2014-03-31","E+H",null,{"v":23454.78,"d":"23,454.78"},{"v":18265.41,"d":"18,265.41"},"脱墨浆停产","良好"]
[550,"吉林晨鸣","制浆分厂","电磁流量计","50P1H-ECGA1A2AAAW DN100",2000001912,"台",1,"DN100 PN16","2014-03-31","E+H",null,{"v":19688.99,"d":"19,688.99"},{"v":15332.81,"d":"15,332.81"},"脱墨浆停产","良好"]
[551,"吉林晨鸣","制浆分厂","电磁流量计","50P1H-ECGA1A2AAAW DN100",2000001913,"台",1,"DN100 PN16","2014-03-31","E+H",null,{"v":19867.45,"d":"19,867.45"},{"v":15471.77,"d":"15,471.77"},"脱墨浆停产","良好"]
[552,"吉林晨鸣","制浆分厂","电磁流量计","50P1F-ECGA1AC2AAAW DN150",2000001917,"台",1,"DN150 PN16","2014-03-31","E+H",null,{"v":23791.69,"d":"23,791.69"},{"v":18527.76,"d":"18,527.76"},"脱墨浆停产","良好"]
[553,"吉林晨鸣","制浆分厂","长颈泵","DYWS60-9",2000001918,"台",1,null,"2014-03-31",null,null,{"v":3643.96,"d":"3,643.96"},{"v":2837.72,"d":"2,837.72"},"脱墨浆停产","良好"]
[554,"吉林晨鸣","制浆分厂","电磁流量计","50PIF-ECGAIAC2AAAW DN150",2000001919,"台",1,"DN150 PN16","2014-03-31","E+H",null,{"v":27452.04,"d":"27,452.04"},{"v":21378.28,"d":"21,378.28"},"脱墨浆停产","良好"]
[555,"吉林晨鸣","制浆分厂","电机","Y2 315M-2 132KW 380卧式",2000001920,"台",1,null,"2014-03-31",null,null,{"v":24353.08,"d":"24,353.08"},{"v":18964.95,"d":"18,964.95"},"脱墨浆停产","良好"]
[556,"吉林晨鸣","制浆分厂","电磁流量计","50P2H-EDIAIAC2AAW DN200",2000001921,"台",1,"DN200 PN16","2014-03-31","E+H",null,{"v":32177.46,"d":"32,177.46"},{"v":25058.19,"d":"25,058.19"},"脱墨浆停产","良好"]
[557,"吉林晨鸣","制浆分厂","电磁流量计","53P25-EA1B1AC2AAAA DN25",2000001922,"台",1,"DN25 PN16","2014-03-31","E+H",null,{"v":22674.71,"d":"22,674.71"},{"v":17657.94,"d":"17,657.94"},"脱墨浆停产","良好"]
[558,"吉林晨鸣","制浆分厂","减速机","GFSZT97-22.11-M1",2000001924,"台",1,null,"2014-03-31",null,null,{"v":6476.5,"d":"6,476.50"},{"v":5043.59,"d":"5,043.59"},"脱墨浆停产","良好"]
[559,"吉林晨鸣","制浆分厂","潜水泵","DYWS100-23-15",2000001925,"台",1,null,"2014-03-31",null,null,{"v":8293.66,"d":"8,293.66"},{"v":6458.7,"d":"6,458.70"},"脱墨浆停产","良好"]
[560,"吉林晨鸣","制浆分厂","潜水泵","DYWS100-23-15",2000001926,"台",1,null,"2014-03-31",null,null,{"v":8293.66,"d":"8,293.66"},{"v":6458.7,"d":"6,458.70"},"脱墨浆停产","良好"]
[561,"吉林晨鸣","制浆分厂","浓度转换器",null,2000001927,"台",1,null,"2014-03-31",null,null,{"v":61848.19,"d":"61,848.19"},{"v":48164.27,"d":"48,164.27"},"脱墨浆停产","良好"]
[562,"吉林晨鸣","制浆分厂","电磁流量计","DN350E+H",2000006703,"台",1,"DN350 PN16","2014-04-30","E+H",null,{"v":4102.57,"d":"4,102.57"},{"v":3210.25,"d":"3,210.25"},"脱墨浆停产","良好"]
[563,"吉林晨鸣","制浆分厂","白度仪",null,2000006718,"台",2,"插入式 50-80ISO","2014-05-16","BTG",null,{"v":137488.1,"d":"137,488.10"},{"v":108100.03,"d":"108,100.03"},"脱墨浆停产","良好"]
[564,"吉林晨鸣","制浆分厂","亚硫酸氢钠泵",null,2000006740,"台",3,null,"2014-09-27",null,null,{"v":18372.65,"d":"18,372.65"},{"v":14721.07,"d":"14,721.07"},"脱墨浆停产","良好"]
[565,"吉林晨鸣","制浆分厂","亚硫轻纳玻璃钢储罐",null,2000006741,"个",4,null,"2014-10-22",107017,null,{"v":119658.12,"d":"119,658.12"},{"v":96324.77,"d":"96,324.77"},"脱墨浆停产","良好"]
[566,"吉林晨鸣","制浆分厂","电动阀DN400",null,2000006759,"台",3,"DN400 PN16","2014-12-22","天津塘沽",null,{"v":43542.73,"d":"43,542.73"},{"v":35378.48,"d":"35,378.48"},"脱墨浆停产","一台已报废，2台碎解白纸边用"]
[567,"吉林晨鸣","制浆分厂","电磁流量计DN350",null,2000006760,"台",2,"DN350 PN16","2014-12-22","科隆",null,{"v":46297.16,"d":"46,297.16"},{"v":37616.45,"d":"37,616.45"},"脱墨浆停产","良好"]
[568,"吉林晨鸣","制浆分厂","重质除渣器",null,2000006762,"套",2,null,"2015-02-26",null,null,{"v":260318.51,"d":"260,318.51"},{"v":213461.13,"d":"213,461.13"},"脱墨浆停产","良好"]
[569,"吉林晨鸣","制浆分厂","弧形筛及其附属设施-新安装",null,2000006763,"套",1,null,"2015-03-30",null,null,{"v":161655.95,"d":"161,655.95"},{"v":133164.04,"d":"133,164.04"},"脱墨浆停产","良好"]
[570,"吉林晨鸣","制浆分厂","螺旋输送机",null,2000006767,"台",8,null,"2015-05-27",null,null,{"v":247989.83,"d":"247,989.83"},{"v":206141.53,"d":"206,141.53"},"脱墨浆停产","良好"]
[571,"吉林晨鸣","制浆分厂","成浆塔防返黄加碱系统",null,2000006803,"套",1,null,"2016-06-28",null,null,{"v":160336.66,"d":"160,336.66"},{"v":141096.17,"d":"141,096.17"},"脱墨浆停产","良好"]
[572,"吉林晨鸣","制浆分厂","屋顶通风器",null,2000006805,"台",5,null,"2016-09-26",null,null,{"v":222222.22,"d":"222,222.22"},{"v":198055.55,"d":"198,055.55"},"脱墨浆停产","良好"]
[573,"吉林晨鸣","制浆分厂","搅拌器（絮凝剂储存槽）",null,2000006819,"台",2,null,"2017-01-22",null,null,{"v":15384.62,"d":"15,384.62"},{"v":13942.3,"d":"13,942.30"},"脱墨浆停产","良好"]
[574,"吉林晨鸣","制浆分厂","稀释水罐",null,2000006824,"套",2,null,"2017-03-21",115119,null,{"v":43734.95,"d":"43,734.95"},{"v":39962.82,"d":"39,962.82"},"脱墨浆停产","良好"]
[575,"吉林晨鸣","制浆分厂","除渣器",null,2000006828,"套",1,null,"2017-05-03",null,null,{"v":507235.97,"d":"507,235.97"},{"v":467291.07,"d":"467,291.07"},"脱墨浆停产","良好"]
[576,"吉林晨鸣","制浆分厂","减速机-1#污泥压榨机",null,2000006972,"台",1,null,"2017-09-28",null,null,{"v":766580,"d":"766,580.00"},{"v":717710.52,"d":"717,710.52"},"脱墨浆停产","良好"]
[null,"经核查吉林晨鸣脱墨浆闲置设备共576项673台，固定资产原值6968.86万元、净值5445.07万元。",{"$nulls":7},"合计",null,null,69688560.66000009,54550747.66000018]

{"sheet":"重点设备","index":1,"n_rows":45,"n_cols":12,"rows_kept":45,"merged":[[0,0,0,11],[44,1,44,6]],"flags":["formulas_cached_only"]}
["重点设备清单（单台设备净值20万元以上）"]
["序号","物料名称","规格型号","资产编号","单位","数量","主要性能指标、参数","购入时间","购进厂家","资产原值","现账面净值","设备状况"]
[1,"散包机","BO1500",2000000819,"台",1,"长×宽×高：5700×3500×8000mm，变频调速，1500rpm，380V，B5，IP55  正反转（5台)                                \n\n\n",2013.9," VOITH",{"v":686637.84,"d":"686,637.84"},{"v":534719.23,"d":"534,719.23"},"良好"]
[2,"复合筛","CSM22B",2000000840,"台",1,"进浆浓度：1.88％  筛板孔径：2.0mm ，筛鼓孔径：2.2mm",2013.9," VOITH",{"v":278252.38,"d":"278,252.38"},{"v":216689.03,"d":"216,689.03"},"良好"]
[3,"高浓除渣器","HCC170-83S",2000000841,"台",1,"最大进浆压力：3.0bar   正常压降：1.3bar",2013.9," VOITH",{"v":268013.43,"d":"268,013.43"},{"v":208715.47,"d":"208,715.47"},"良好"]
[4,"一段前浮选槽","ECC4/44P",2000000855,"台",1,"  进浆量：26312l/min   进浆浓度：1.31％",2013.9," VOITH",{"v":1778465.91,"d":"1,778,465.91"},{"v":1384980.31,"d":"1,384,980.31"},"良好"]
[5,"前浮选一段2#喂料泵","APP54-500/O",2000000856,"台",1,"Q=1800m3/h  H=10m C=1.31%",2013.9,"苏尔寿",{"v":324547.51,"d":"324,547.51"},{"v":252741.36,"d":"252,741.36"},"良好"]
[6,"前浮选一段3#喂料泵","APP54-500/O",2000000857,"台",1,"Q=1800m3/h  H=10m C=1.31%",2013.9,"苏尔寿",{"v":324547.51,"d":"324,547.51"},{"v":252741.36,"d":"252,741.36"},"良好"]
[7,"前浮选一段4#喂料泵","APP54-500/O",2000000858,"台",1,"Q=1800m3/h  H=10m C=1.31%",2013.9,"苏尔寿",{"v":324547.51,"d":"324,547.51"},{"v":252741.36,"d":"252,741.36"},"良好"]
[8,"前浮选一段5#喂料泵","APP54-500/O",2000000859,"台",1,"Q=1800m3/h  H=10m C=1.31%",2013.9,"苏尔寿",{"v":324547.51,"d":"324,547.51"},{"v":252741.36,"d":"252,741.36"},"良好"]
[9,"前浮选二段槽","SFL5DD",2000000863,"台",1,"进浆量：7560l/min   进浆浓度：0.91％",2013.9,"安德里兹",{"v":1778465.91,"d":"1,778,465.91"},{"v":1384980.31,"d":"1,384,980.31"},"良好"]
[10,"一段精筛","GFF-1200",2000000867,"台",1,"进浆浓度：0.98％  缝宽：0.15mm ",2013.9,"日本相川",{"v":385269.3,"d":"385,269.30"},{"v":300028.46,"d":"300,028.46"},"良好"]
[11,"二段精筛","GFF-1000",2000000869,"台",1,"进浆浓度：0.80％ 缝宽：0.15mm ",2013.9,"日本相川",{"v":311984.38,"d":"311,984.38"},{"v":242957.82,"d":"242,957.82"},"良好"]
[12,"1#快速加热器","PMAS36",2000000878,"台",1,"进浆28-30%，出浆30%,  良浆能力：386 BDT/D",2013.9," VOITH",{"v":939093.92,"d":"939,093.92"},{"v":731319.37,"d":"731,319.37"},"良好"]
[13,"1#热分散机","KRD-110HC",2000000879,"台",1,"进浆浓度30%，出浆28%，能力：386 BDT/D",2013.9," VOITH",{"v":4876588.06,"d":"4,876,588.06"},{"v":3797642.96,"d":"3,797,642.96"},"良好"]
[14,"氧化漂白塔","HTC500-114",2000000880,"台",1,"计量140m3，直径φ5000X8800mm",2013.9," VOITH",{"v":314078.24,"d":"314,078.24"},{"v":244588.43,"d":"244,588.43"},"良好"]
[15,"后浮选槽一段","ECC4/44P",2000000885,"台",1,"  进浆量：25376 l/min   进浆浓度：1.20％",2013.9," VOITH",{"v":2093854.9,"d":"2,093,854.90"},{"v":1630589.51,"d":"1,630,589.51"},"良好"]
[16,"后浮选一段2#喂料泵","APP54-500/O",2000000886,"台",1,"Q=1700m3/h H=10m C=1.20%",2013.9,"苏尔寿",{"v":324547.51,"d":"324,547.51"},{"v":252741.36,"d":"252,741.36"},"良好"]
[17,"后浮选一段3#喂料泵","APP54-500/O",2000000887,"台",1,"Q=1700m3/h H=10m C=1.20%",2013.9,"苏尔寿",{"v":324547.51,"d":"324,547.51"},{"v":252741.36,"d":"252,741.36"},"良好"]
[18,"后浮选一段4#喂料泵","APP54-500/O",2000000888,"台",1,"Q=1700m3/h H=10m C=1.20%",2013.9,"苏尔寿",{"v":324547.51,"d":"324,547.51"},{"v":252741.36,"d":"252,741.36"},"良好"]
[19,"二段后浮选槽","SFL4DD",2000000892,"台",1,"  进浆量：6040l/min   进浆浓度：0.87％",2013.9,"安德里兹",{"v":2093854.9,"d":"2,093,854.90"},{"v":1630589.51,"d":"1,630,589.51"},"良好"]
[20,"后多盘浓缩机","VDF5.2-16/15-325",2000000897,"台",1,"滤盘直径：5200mm    16盘  过滤面积：489m2",2013.9,"G&LV",{"v":6051240.66,"d":"6,051,240.66"},{"v":4712403.66,"d":"4,712,403.66"},"良好"]
[21,"2#3#螺旋挤浆机","SHX-900X5500",2000000899,"台",2,"螺旋直径：φ900mm， 螺旋长度：5500mm",2013.9,"日本相川",{"v":1758838.12,"d":"1,758,838.12"},{"v":1369695.17,"d":"1,369,695.17"},"良好"]
[22,"后热分散机","KRD85XLC",2000000902,"台",1,"进浆浓度30%，出浆28%, 能力410 BDt/d，浆温≤90℃",2013.9,"VOITH  ",{"v":4899620.47,"d":"4,899,620.47"},{"v":3815579.45,"d":"3,815,579.45"},"良好"]
[23,"2#中浓泵","LCE21-100V",2000000904,"台",1,"Q=180m3/h    H=70m    C=10%",2013.9,"苏尔寿",{"v":374800.03,"d":"374,800.03"},{"v":291875.53,"d":"291,875.53"},"良好"]
[24,"1#气浮","CQJ-10",2000000932,"台",1,"处理水量：7650L/min，Φ10000mm  ",2013.9,"无锡沪东",{"v":565340.82,"d":"565,340.82"},{"v":440259.14,"d":"440,259.14"},"良好"]
[25,"重力床"," BD3XL",2000000938,"台",1,"工作面宽：3150mm,网案长度：10200mm，面积25.4m2",2013.9,"VOITH   ",{"v":361189.97,"d":"361,189.97"},{"v":281276.68,"d":"281,276.68"},"良好"]
[26,"污泥压榨螺旋","RSP-80",2000000939,"台",2,"能力:120 绝干t/d，进口浓度10-15%，出口浓度50%-60%",2013.9,"VOITH   ",{"v":4187709.8,"d":"4,187,709.80"},{"v":3261179.01,"d":"3,261,179.01"},"良好"]
[27,"2#气浮","CQJ-10",2000000942,"台",1,"处理水量：5200L/min，Φ8000mm  ",2013.9,"无锡沪东",{"v":565340.82,"d":"565,340.82"},{"v":440259.14,"d":"440,259.14"},"良好"]
[28,"压滤机","CPN-NS2500S6",2000000998,"台",1,"外型：5.5*3.62*2.3",2013.9,"绿昇环保工程",{"v":366424.61,"d":"366,424.61"},{"v":285353.15,"d":"285,353.15"},"良好"]
[29,"中浓立管",null,2000000903,"台",1,null,"2014-03-31",null,{"v":1046927.45,"d":"1,046,927.45"},{"v":815294.75,"d":"815,294.75"},"良好"]
[30,"Na2SiO3贮存槽","V=50M3",2000001733,"台",1,null,"2014-03-31",null,{"v":287513.17,"d":"287,513.17"},{"v":223900.89,"d":"223,900.89"},"良好"]
[31,"NaOH贮存槽","V=10M3",2000001734,"台",1,null,"2014-03-31",null,{"v":287513.17,"d":"287,513.17"},{"v":223900.89,"d":"223,900.89"},"良好"]
[32,"后浮选槽","MACC114A-800",2000001735,"台",1,null,"2014-03-31",null,{"v":422495.79,"d":"422,495.79"},{"v":329018.6,"d":"329,018.60"},"良好"]
[33,"清水罐","V=10M3",2000001736,"台",1,null,"2014-03-31",null,{"v":810791.95,"d":"810,791.95"},{"v":631404.22,"d":"631,404.22"},"良好"]
[34,"二段中浓除渣器供料泵","S125—400CD",2000001737,"台",1,null,"2014-03-31",null,{"v":1090648.4,"d":"1,090,648.40"},{"v":849342.43,"d":"849,342.43"},"良好"]
[35,"前多盘浓缩机","VDF5.2-10/12",2000001739,"台",1,null,"2014-03-31",null,{"v":1461376.27,"d":"1,461,376.27"},{"v":1138046.78,"d":"1,138,046.78"},"良好"]
[36,"链板机","V=10M3",2000001740,"台",1,null,"2014-03-31",null,{"v":1550762.14,"d":"1,550,762.14"},{"v":1207655.99,"d":"1,207,655.99"},"良好"]
[37,"挤浆机","ZNJ160",2000001884,"台",1,null,"2014-03-31",null,{"v":281975.96,"d":"281,975.96"},{"v":219588.77,"d":"219,588.77"},"良好"]
[38,"2#挤浆机",null,2000001886,"台",1,null,"2014-03-31",null,{"v":402342.73,"d":"402,342.73"},{"v":313324.41,"d":"313,324.41"},"良好"]
[39,"新一精2","S3—200—470DD",2000001894,"台",1,null,"2014-03-31",null,{"v":263598.32,"d":"263,598.32"},{"v":205277.2,"d":"205,277.20"},"良好"]
[40,"新三精","S3—150—400DD",2000001895,"台",1,null,"2014-03-31",null,{"v":483879.17,"d":"483,879.17"},{"v":376820.92,"d":"376,820.92"},"良好"]
[41,"除渣器",null,2000006828,"套",1,null,"2017-05-03",null,{"v":507235.97,"d":"507,235.97"},{"v":467291.07,"d":"467,291.07"},"良好"]
[42,"减速机-1#污泥压榨机",null,2000006972,"台",1,null,"2017-09-28",null,{"v":766580,"d":"766,580.00"},{"v":717710.52,"d":"717,710.52"},"良好"]
[null,"其中单台设备净值20万元以上共46台，原值4687.05万元、净值3669.34万元。",{"$nulls":6},"合计",46870537.53000001,36693448.30000001]

{"sheet":"Sheet2","index":2,"n_rows":44,"n_cols":12,"rows_kept":44,"merged":[[43,1,43,6]],"flags":["formulas_cached_only"]}
["序号","物料名称","规格型号","资产编号","单位","数量","主要性能指标、参数","购入时间","购进厂家","资产原值","现账面净值","设备状况"]
[1,"散包机","BO1500",2000000819,"台",1,"长×宽×高：5700×3500×8000mm，变频调速，1500rpm，380V，B5，IP55  正反转（5台)                                \n\n\n",2013.9," VOITH",{"v":686637.84,"d":"686,637.84"},{"v":534719.23,"d":"534,719.23"},"良好"]
[2,"复合筛","CSM22B",2000000840,"台",1,"进浆浓度：1.88％  筛板孔径：2.0mm ，筛鼓孔径：2.2mm",2013.9," VOITH",{"v":278252.38,"d":"278,252.38"},{"v":216689.03,"d":"216,689.03"},"良好"]
[3,"高浓除渣器","HCC170-83S",2000000841,"台",1,"最大进浆压力：3.0bar   正常压降：1.3bar",2013.9," VOITH",{"v":268013.43,"d":"268,013.43"},{"v":208715.47,"d":"208,715.47"},"良好"]
[4,"一段前浮选槽","ECC4/44P",2000000855,"台",1,"  进浆量：26312l/min   进浆浓度：1.31％",2013.9," VOITH",{"v":1778465.91,"d":"1,778,465.91"},{"v":1384980.31,"d":"1,384,980.31"},"良好"]
[5,"前浮选一段2#喂料泵","APP54-500/O",2000000856,"台",1,"Q=1800m3/h  H=10m C=1.31%",2013.9,"苏尔寿",{"v":324547.51,"d":"324,547.51"},{"v":252741.36,"d":"252,741.36"},"良好"]
[6,"前浮选一段3#喂料泵","APP54-500/O",2000000857,"台",1,"Q=1800m3/h  H=10m C=1.31%",2013.9,"苏尔寿",{"v":324547.51,"d":"324,547.51"},{"v":252741.36,"d":"252,741.36"},"良好"]
[7,"前浮选一段4#喂料泵","APP54-500/O",2000000858,"台",1,"Q=1800m3/h  H=10m C=1.31%",2013.9,"苏尔寿",{"v":324547.51,"d":"324,547.51"},{"v":252741.36,"d":"252,741.36"},"良好"]
[8,"前浮选一段5#喂料泵","APP54-500/O",2000000859,"台",1,"Q=1800m3/h  H=10m C=1.31%",2013.9,"苏尔寿",{"v":324547.51,"d":"324,547.51"},{"v":252741.36,"d":"252,741.36"},"良好"]
[9,"前浮选二段槽","SFL5DD",2000000863,"台",1,"进浆量：7560l/min   进浆浓度：0.91％",2013.9,"安德里兹",{"v":1778465.91,"d":"1,778,465.91"},{"v":1384980.31,"d":"1,384,980.31"},"良好"]
[10,"一段精筛","GFF-1200",2000000867,"台",1,"进浆浓度：0.98％  缝宽：0.15mm ",2013.9,"日本相川",{"v":385269.3,"d":"385,269.30"},{"v":300028.46,"d":"300,028.46"},"良好"]
[11,"二段精筛","GFF-1000",2000000869,"台",1,"进浆浓度：0.80％ 缝宽：0.15mm ",2013.9,"日本相川",{"v":311984.38,"d":"311,984.38"},{"v":242957.82,"d":"242,957.82"},"良好"]
[12,"1#快速加热器","PMAS36",2000000878,"台",1,"进浆28-30%，出浆30%,  良浆能力：386 BDT/D",2013.9," VOITH",{"v":939093.92,"d":"939,093.92"},{"v":731319.37,"d":"731,319.37"},"良好"]
[13,"1#热分散机","KRD-110HC",2000000879,"台",1,"进浆浓度30%，出浆28%，能力：386 BDT/D",2013.9," VOITH",{"v":4876588.06,"d":"4,876,588.06"},{"v":3797642.96,"d":"3,797,642.96"},"良好"]
[14,"氧化漂白塔","HTC500-114",2000000880,"台",1,"计量140m3，直径φ5000X8800mm",2013.9," VOITH",{"v":314078.24,"d":"314,078.24"},{"v":244588.43,"d":"244,588.43"},"良好"]
[15,"后浮选槽一段","ECC4/44P",2000000885,"台",1,"进浆量：25376 l/min   进浆浓度：1.20％",2013.9," VOITH",{"v":2093854.9,"d":"2,093,854.90"},{"v":1630589.51,"d":"1,630,589.51"},"良好"]
[16,"后浮选一段2#喂料泵","APP54-500/O",2000000886,"台",1,"Q=1700m3/h H=10m C=1.20%",2013.9,"苏尔寿",{"v":324547.51,"d":"324,547.51"},{"v":252741.36,"d":"252,741.36"},"良好"]
[17,"后浮选一段3#喂料泵","APP54-500/O",2000000887,"台",1,"Q=1700m3/h H=10m C=1.20%",2013.9,"苏尔寿",{"v":324547.51,"d":"324,547.51"},{"v":252741.36,"d":"252,741.36"},"良好"]
[18,"后浮选一段4#喂料泵","APP54-500/O",2000000888,"台",1,"Q=1700m3/h H=10m C=1.20%",2013.9,"苏尔寿",{"v":324547.51,"d":"324,547.51"},{"v":252741.36,"d":"252,741.36"},"良好"]
[19,"二段后浮选槽","SFL4DD",2000000892,"台",1,"  进浆量：6040l/min   进浆浓度：0.87％",2013.9,"安德里兹",{"v":2093854.9,"d":"2,093,854.90"},{"v":1630589.51,"d":"1,630,589.51"},"良好"]
[20,"后多盘浓缩机","VDF5.2-16/15-325",2000000897,"台",1,"滤盘直径：5200mm    16盘  过滤面积：489m2",2013.9,"G&LV",{"v":6051240.66,"d":"6,051,240.66"},{"v":4712403.66,"d":"4,712,403.66"},"良好"]
[21,"2#3#螺旋挤浆机","SHX-900X5500",2000000899,"台",2,"螺旋直径：φ900mm， 螺旋长度：5500mm",2013.9,"日本相川",{"v":1758838.12,"d":"1,758,838.12"},{"v":1369695.17,"d":"1,369,695.17"},"良好"]
[22,"后热分散机","KRD85XLC",2000000902,"台",1,"进浆浓度30%，出浆28%, 能力410 BDt/d，浆温≤90℃",2013.9,"VOITH  ",{"v":4899620.47,"d":"4,899,620.47"},{"v":3815579.45,"d":"3,815,579.45"},"良好"]
[23,"2#中浓泵","LCE21-100V",2000000904,"台",1,"Q=180m3/h    H=70m    C=10%",2013.9,"苏尔寿",{"v":374800.03,"d":"374,800.03"},{"v":291875.53,"d":"291,875.53"},"良好"]
[24,"1#气浮","CQJ-10",2000000932,"台",1,"处理水量：7650L/min，Φ10000mm  ",2013.9,"无锡沪东",{"v":565340.82,"d":"565,340.82"},{"v":440259.14,"d":"440,259.14"},"良好"]
[25,"重力床"," BD3XL",2000000938,"台",1,"工作面宽：3150mm,网案长度：10200mm，面积25.4m2",2013.9,"VOITH   ",{"v":361189.97,"d":"361,189.97"},{"v":281276.68,"d":"281,276.68"},"良好"]
[26,"污泥压榨螺旋","RSP-80",2000000939,"台",2,"能力:120 绝干t/d，进口浓度10-15%，出口浓度50%-60%",2013.9,"VOITH   ",{"v":4187709.8,"d":"4,187,709.80"},{"v":3261179.01,"d":"3,261,179.01"},"良好"]
[27,"2#气浮","CQJ-10",2000000942,"台",1,"处理水量：5200L/min，Φ8000mm  ",2013.9,"无锡沪东",{"v":565340.82,"d":"565,340.82"},{"v":440259.14,"d":"440,259.14"},"良好"]
[28,"压滤机","CPN-NS2500S6",2000000998,"台",1,"外型：5.5*3.62*2.3",2013.9,"绿昇环保工程",{"v":366424.61,"d":"366,424.61"},{"v":285353.15,"d":"285,353.15"},"良好"]
[29,"中浓立管",null,2000000903,"台",1,null,"2014-03-31",null,{"v":1046927.45,"d":"1,046,927.45"},{"v":815294.75,"d":"815,294.75"},"良好"]
[30,"Na2SiO3贮存槽","V=50M3",2000001733,"台",1,null,"2014-03-31",null,{"v":287513.17,"d":"287,513.17"},{"v":223900.89,"d":"223,900.89"},"良好"]
[31,"NaOH贮存槽","V=10M3",2000001734,"台",1,null,"2014-03-31",null,{"v":287513.17,"d":"287,513.17"},{"v":223900.89,"d":"223,900.89"},"良好"]
[32,"后浮选槽","MACC114A-800",2000001735,"台",1,null,"2014-03-31",null,{"v":422495.79,"d":"422,495.79"},{"v":329018.6,"d":"329,018.60"},"良好"]
[33,"清水罐","V=10M3",2000001736,"台",1,null,"2014-03-31",null,{"v":810791.95,"d":"810,791.95"},{"v":631404.22,"d":"631,404.22"},"良好"]
[34,"二段中浓除渣器供料泵","S125—400CD",2000001737,"台",1,null,"2014-03-31",null,{"v":1090648.4,"d":"1,090,648.40"},{"v":849342.43,"d":"849,342.43"},"良好"]
[36,"前多盘浓缩机","VDF5.2-10/12",2000001739,"台",1,null,"2014-03-31",null,{"v":1461376.27,"d":"1,461,376.27"},{"v":1138046.78,"d":"1,138,046.78"},"良好"]
[37,"链板机","V=10M3",2000001740,"台",1,null,"2014-03-31",null,{"v":1550762.14,"d":"1,550,762.14"},{"v":1207655.99,"d":"1,207,655.99"},"良好"]
[39,"挤浆机","ZNJ160",2000001884,"台",1,null,"2014-03-31",null,{"v":281975.96,"d":"281,975.96"},{"v":219588.77,"d":"219,588.77"},"良好"]
[40,"2#挤浆机",null,2000001886,"台",1,null,"2014-03-31",null,{"v":402342.73,"d":"402,342.73"},{"v":313324.41,"d":"313,324.41"},"良好"]
[41,"新一精筛泵2","S3—200—470DD",2000001894,"台",1,null,"2014-03-31",null,{"v":263598.32,"d":"263,598.32"},{"v":205277.2,"d":"205,277.20"},"良好"]
[42,"新三精筛泵","S3—150—400DD",2000001895,"台",1,null,"2014-03-31",null,{"v":483879.17,"d":"483,879.17"},{"v":376820.92,"d":"376,820.92"},"良好"]
[43,"除渣器",null,2000006828,"套",1,null,"2017-05-03",null,{"v":507235.97,"d":"507,235.97"},{"v":467291.07,"d":"467,291.07"},"良好"]
[44,"减速机-1#污泥压榨机",null,2000006972,"台",1,null,"2017-09-28",null,{"v":766580,"d":"766,580.00"},{"v":717710.52,"d":"717,710.52"},"良好"]
[null,"其中单台设备净值20万元以上共46台，原值5271.98万元、净值4124.85万元。",{"$nulls":6},"合计",46870537.53000001,36693448.30000001]